(footprint "1P_2x0.75"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "ANT1"
		(at 0 -1.1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4dbddf4d-659f-4a85-84cd-d39d945b560f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SENSE_PIN"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "9bf126fb-d896-4c91-98ee-810dabae29d3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "SH_Solder_Pads:1P_2x0.75"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c4af321b-2e47-413f-a6cb-dee7a431b0f5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "db494798-fa40-40e9-998b-1185c32eac1d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "98725f0d-6afe-473d-8dba-cfc06c494e16")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole exclude_from_pos_files)
	(fp_circle
		(center 0 0)
		(end 0 -0.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "B.CrtYd")
		(uuid "4bf10458-5b1d-421b-bece-3957f20da4e4")
	)
	(fp_line
		(start -1.15 0.025)
		(end -1.15 -0.025)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bbb867a5-20c0-4a34-8e42-8bf98a9a4fb8")
	)
	(fp_line
		(start -0.65 -0.525)
		(end 0.65 -0.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f751dd8c-9c97-4bde-a78f-77e56bd2e18b")
	)
	(fp_line
		(start 0.65 0.525)
		(end -0.65 0.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5d6d81a8-812c-4221-88cd-f8cc1931623c")
	)
	(fp_line
		(start 1.15 -0.025)
		(end 1.15 0.025)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1b22b7ed-3ce6-4a8b-a4e5-b49958e255c3")
	)
	(fp_arc
		(start -1.15 -0.025)
		(mid -1.003553 -0.378553)
		(end -0.65 -0.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "99a41992-84b3-422a-ad82-c563c9cc5ddb")
	)
	(fp_arc
		(start -0.65 0.525)
		(mid -1.003553 0.378553)
		(end -1.15 0.025)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9c4eb2ec-d99f-49ca-9a85-d2f19cf14877")
	)
	(fp_arc
		(start 0.65 -0.525)
		(mid 1.003553 -0.378553)
		(end 1.15 -0.025)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6cd4be82-1471-4469-ae1b-fffaded3fe3d")
	)
	(fp_arc
		(start 1.15 0.025)
		(mid 1.003553 0.378553)
		(end 0.65 0.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2b88cb9d-3833-4616-8ea9-699c54e07210")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "261eade3-c62e-475b-a616-89d5d71dab03")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 0.75 0.75)
		(drill 0.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "825b21f9-f978-4627-b43b-6d98288dc694")
	)
	(pad "1" connect oval
		(at 0 0)
		(size 2 0.75)
		(layers "F.Cu" "F.Mask")
		(uuid "21041ba0-fbf3-4818-94bd-279ae2c914d8")
	)
)