(footprint "Yageo_YC104" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Field2" "")
  (property "Sheetfile" "Ethernet.kicad_sch")
  (property "Sheetname" "Ethernet")
  (attr smd)
  (fp_text reference "R5" (at -1.55 0 90 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 0f332955-16db-4943-8792-1365439d776e)
  )
  (fp_text value "22" (at 0 0.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 6fb5e6c8-382f-4b99-8d7f-b1f37d15693b)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 4f184b60-6b48-4b68-b841-8e9558ea55a2)
  )
  (fp_rect (start -1 -0.3) (end -0.85 0.3)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 057748e5-8d94-493a-9ae1-8f99aa4f2e46))
  (fp_rect (start 0.85 -0.3) (end 1 0.3)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp f27193a5-2016-4c68-8c0a-9d872b83b350))
  (fp_line (start -0.95 -0.3) (end -0.95 0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3acb9147-0842-4c5b-a002-8de10daf98f4))
  (fp_line (start -0.7 0.55) (end 0.7 0.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 695885c1-143c-4066-ba61-9a97de17d902))
  (fp_line (start 0.7 -0.55) (end -0.7 -0.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6536dff9-9ff1-47d8-8c5d-715cd7b36b11))
  (fp_line (start 0.95 -0.3) (end 0.95 0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fcfad448-a8df-4329-9b49-54e1963760e4))
  (fp_arc (start -0.95 -0.3) (mid -0.876777 -0.476777) (end -0.7 -0.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b80b7385-8916-4e23-bfc3-9bda5feafda5))
  (fp_arc (start -0.7 0.55) (mid -0.876777 0.476777) (end -0.95 0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b68be4eb-a4a2-45a5-a619-76f141a0372d))
  (fp_arc (start 0.7 -0.55) (mid 0.876777 -0.476777) (end 0.95 -0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 83e55014-123b-4450-9270-fcbc22042cf4))
  (fp_arc (start 0.95 0.3) (mid 0.876777 0.476777) (end 0.7 0.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a1dff8ed-54b2-44e8-a68f-03e85b86208f))
  (fp_rect (start -0.7 -0.3) (end 0.7 0.3)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.Fab") (tstamp b7bac132-8595-43f7-a223-5b8a92205a88))
  (pad "" smd oval (at -0.6 -0.25) (size 0.2 0.25) (layers "F.Paste") (tstamp fcc8ffe9-38e8-4162-8092-e9adb9bcd92a))
  (pad "" smd oval (at -0.6 0.25) (size 0.2 0.25) (layers "F.Paste") (tstamp 845216d2-c165-44b0-a572-bb6f188ea2c7))
  (pad "" smd oval (at -0.2 -0.25) (size 0.2 0.25) (layers "F.Paste") (tstamp a961dd21-bc12-490a-86d3-91e9dee05c21))
  (pad "" smd oval (at -0.2 0.25) (size 0.2 0.25) (layers "F.Paste") (tstamp f04e6efe-2c4c-401c-845c-8f9f45bf8dad))
  (pad "" smd oval (at 0.2 -0.25) (size 0.2 0.25) (layers "F.Paste") (tstamp 11577f4a-ad3b-4c35-90d2-10f3402634b6))
  (pad "" smd oval (at 0.2 0.25) (size 0.2 0.25) (layers "F.Paste") (tstamp a6e76051-590d-4c9c-bb06-6b1960b7b699))
  (pad "" smd oval (at 0.6 -0.25) (size 0.2 0.25) (layers "F.Paste") (tstamp 7e7461c4-5c13-4cbd-9b45-519af2aaa5e3))
  (pad "" smd oval (at 0.6 0.25) (size 0.2 0.25) (layers "F.Paste") (tstamp 367597e2-cd57-4cb5-a9cd-4520f357764d))
  (pad "1" smd roundrect (at -0.6 0.25) (size 0.25 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.35)
    (chamfer_ratio 0.05) (chamfer top_left top_right)
    (thermal_bridge_angle 45) (tstamp 3e80104b-88a3-4b9b-a6a0-32ea303d8c93))
  (pad "2" smd roundrect (at -0.2 0.25) (size 0.25 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.35)
    (chamfer_ratio 0.05) (chamfer top_left top_right)
    (thermal_bridge_angle 45) (tstamp 71f8456e-d906-4f44-88f1-d183bde9e450))
  (pad "3" smd roundrect (at 0.2 0.25) (size 0.25 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.35)
    (chamfer_ratio 0.05) (chamfer top_left top_right)
    (thermal_bridge_angle 45) (tstamp 4cf7b87a-45e5-4dd6-b918-b347318a14a6))
  (pad "4" smd roundrect (at 0.6 0.25) (size 0.25 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.35)
    (chamfer_ratio 0.05) (chamfer top_left top_right)
    (thermal_bridge_angle 45) (tstamp 9fee9b33-5cd0-431b-b79c-4a6547e8076c))
  (pad "5" smd roundrect (at 0.6 -0.25 180) (size 0.25 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.35)
    (chamfer_ratio 0.05) (chamfer top_left top_right)
    (thermal_bridge_angle 45) (tstamp 291c8cf9-74b0-4a4f-88f0-6ec672a5d1bc))
  (pad "6" smd roundrect (at 0.2 -0.25 180) (size 0.25 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.35)
    (chamfer_ratio 0.05) (chamfer top_left top_right)
    (thermal_bridge_angle 45) (tstamp 0e85a195-b433-4f1e-8e34-f33aeeac08ad))
  (pad "7" smd roundrect (at -0.2 -0.25 180) (size 0.25 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.35)
    (chamfer_ratio 0.05) (chamfer top_left top_right)
    (thermal_bridge_angle 45) (tstamp fda347c8-d053-46f1-a05a-4c93b9199129))
  (pad "8" smd roundrect (at -0.6 -0.25 180) (size 0.25 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.35)
    (chamfer_ratio 0.05) (chamfer top_left top_right)
    (thermal_bridge_angle 45) (tstamp 42a9edc4-7f2f-4e80-8ed4-aa54d9cb1488))
)
