(footprint "3P_1.3x2_P1.5" (version 20220427) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 2 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp bbb6f26a-4f6b-47d0-abf2-da76280cdb20)
  )
  (fp_text value "3P_1.3x2_P1.5" (at 0 -1.75 unlocked) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp d8591878-c41a-47be-b0e5-d69eefb6358e)
  )
  (fp_text user "${REFERENCE}" (at 0 1.5 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp eaae000d-7856-487f-ad4f-f7a29b7a7c73)
  )
  (fp_line (start -2.65 -0.75) (end -2.65 0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp dd1e5755-5509-4637-868f-44070daca1ac))
  (fp_line (start -1.9 1.5) (end 1.9 1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8b2c516d-fc40-403a-8af0-22671ec847cf))
  (fp_line (start 1.9 -1.5) (end -1.9 -1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp effe43b9-7c2b-47cc-bd4f-ac360256621b))
  (fp_line (start 2.65 -0.75) (end 2.65 0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 39c76dbc-c1c7-4bb4-a8d0-82ae3543b491))
  (fp_arc (start -2.65 -0.75) (mid -2.43033 -1.28033) (end -1.9 -1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 48efbbee-b3e8-4812-b0eb-dfc0c17df020))
  (fp_arc (start -1.9 1.5) (mid -2.43033 1.28033) (end -2.65 0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 257f7694-dcee-4db7-b51c-15a8917296ad))
  (fp_arc (start 1.9 -1.5) (mid 2.43033 -1.28033) (end 2.65 -0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6b02d3c4-90ad-481d-af56-2af3e6e790b7))
  (fp_arc (start 2.65 0.75) (mid 2.43033 1.28033) (end 1.9 1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a1582d0a-af82-4eac-a793-bbb7394843d0))
  (pad "1" smd roundrect (at -1.5 0) (size 1.3 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
    (thermal_bridge_angle 45) (tstamp dfda4c93-2972-41b9-93e8-e17f3c94a62a))
  (pad "2" smd roundrect (at 0 0) (size 1.3 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
    (thermal_bridge_angle 45) (tstamp 858e645d-b585-4b14-94da-800b49a16074))
  (pad "3" smd roundrect (at 1.5 0) (size 1.3 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
    (thermal_bridge_angle 45) (tstamp 9543b627-b144-4b00-a82e-737108de40e4))
)
