(footprint "Jushuo_AFC07-S10ECA-00_1x10-1MP_P0.50_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Jushuo AFC07, FFC/FPC connector, AFC07-S06FCA-00, 6 Pins per row (https://datasheet.lcsc.com/lcsc/1811040204_JUSHUO-AFC07-S32FCC-00_C11061.pdf)")
  (tags "connector jushuo horizontal")
  (property "LCSC" "C262583")
  (property "MFG" "JUSHUO")
  (property "MPN" "AFC07-S10ECA-00")
  (property "Sheetfile" "DisplayModule.kicad_sch")
  (property "Sheetname" "")
  (property "ki_keywords" "TFT")
  (attr smd)
  (fp_text reference "J6" (at 0 -3.6 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 56c56f63-3047-48b9-90e9-b1f498dc6e29)
  )
  (fp_text value "Display" (at 0 5.4 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f60601d9-3187-4367-94ca-0c56a272cf8e)
  )
  (fp_text user "${REFERENCE}" (at 0 1.4 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7d9e2218-29d9-4634-8ef3-555430c247b2)
  )
  (fp_line (start -4.87 2.45) (end -4.87 3.13)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 26f74070-b8cb-4399-ab15-e7f6378ae178))
  (fp_line (start -2.6 -0.95) (end -4.9 -0.95)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4a6c3965-6dc6-43a2-a5b7-2ad8346f798a))
  (fp_line (start -2.6 -0.95) (end -2.6 -2.25)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a6d66679-f240-496d-9524-6568fdf1ecbd))
  (fp_line (start 2.6 -0.95) (end 4.9 -0.95)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f9f7ed3f-7cd8-4723-a055-275bd0ce612e))
  (fp_line (start 4.87 2.45) (end 4.87 3.13)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2b1e20f7-8a0d-4370-9453-523a5b69783e))
  (fp_line (start -5.8 -1.25) (end -5.8 4.15)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 66fbadb9-3801-4db6-839a-8c536ac33b08))
  (fp_line (start -5.8 4.15) (end 5.8 4.15)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b479de2f-f7cd-49ce-9324-5ee94839692d))
  (fp_line (start -2.9 -2.75) (end -2.9 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3d60b02e-9110-4264-abdc-6f1e5c6b7ec0))
  (fp_line (start -2.9 -1.25) (end -5.8 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fb6b3451-1447-403b-8479-2d97b22f5c6f))
  (fp_line (start 2.9 -2.75) (end -2.9 -2.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 663c8664-8212-4268-b35e-d1786268d364))
  (fp_line (start 2.9 -1.25) (end 2.9 -2.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 687b54f3-4995-412d-b7c0-587d871ca866))
  (fp_line (start 5.8 -1.25) (end 2.9 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fa76be2a-0112-461b-9c48-8b14c26c1bf5))
  (fp_line (start 5.8 4.15) (end 5.8 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ea00eff7-b3f1-4068-b11f-1003fe3df9d6))
  (fp_line (start -5.3 3.25) (end -5.3 3.65)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4f4ee04e-5569-4527-8b69-01032292a436))
  (fp_line (start -5.3 3.65) (end 5.3 3.65)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f8f81242-1554-4139-8e5e-8002810bec11))
  (fp_line (start -4.75 -0.75) (end 4.75 -0.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8c76e321-0de9-4177-89ff-de32f328b30b))
  (fp_line (start -4.75 3.25) (end -5.3 3.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 64ae3f7b-2845-403b-a070-e8fbb5ccb068))
  (fp_line (start -4.75 3.25) (end -4.75 -0.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 14d83c12-ddd1-46b2-867f-fa2e87d08b33))
  (fp_line (start -2.5 -0.75) (end -2.25 -0.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ee15c4dd-001a-465f-9c6b-a10d2a34eef2))
  (fp_line (start -2.25 -0.25) (end -2 -0.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d85fd14-0b0a-4127-8a5d-9414c74421ec))
  (fp_line (start 4.75 3.25) (end -4.75 3.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc2af239-98de-4b9b-ad41-97743971510d))
  (fp_line (start 4.75 3.25) (end 4.75 -0.75)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp daafd6bd-8558-482d-8997-7fa2a678343b))
  (fp_line (start 5.3 3.25) (end 4.75 3.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5ee4ebcf-a76c-470f-a0d1-6657b0ff96fd))
  (fp_line (start 5.3 3.65) (end 5.3 3.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 503144fa-559f-49a6-8119-4ab833a4e0f2))
  (pad "1" smd roundrect (at -2.25 -1.6) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1697659a-eea3-40b4-ae24-b9e7b12d73ee))
  (pad "2" smd roundrect (at -1.75 -1.6) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b1d87228-dbc5-4e9b-9c57-165af32ef8e5))
  (pad "3" smd roundrect (at -1.25 -1.6) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 91b90311-e8e7-4afa-ab0a-89b229f9d873))
  (pad "4" smd roundrect (at -0.75 -1.6) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp eff1adf8-85ab-4e6e-8474-39dd07d4d852))
  (pad "5" smd roundrect (at -0.25 -1.6) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ee896ac2-db33-400d-9eb5-2a43c23d48ee))
  (pad "6" smd roundrect (at 0.25 -1.6) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d317f5c4-adb7-4c6c-8fa7-917d41902def))
  (pad "7" smd roundrect (at 0.75 -1.6) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8c1ff588-da66-41e6-b2ef-99cee8355ace))
  (pad "8" smd roundrect (at 1.25 -1.6) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b940b2f7-8f6f-47b7-b4c5-030d155b540a))
  (pad "9" smd roundrect (at 1.75 -1.6) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2c5c9e0d-cc97-4aa0-846f-e24ce04f9687))
  (pad "10" smd roundrect (at 2.25 -1.6) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 64975b13-eddf-450f-b5ac-c0ec5e8d386b))
  (pad "MP" smd roundrect (at -3.9 0.75) (size 2 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.075) (tstamp 1c08e834-86bc-4da2-9c61-9fabeb36bb98))
  (pad "MP" smd roundrect (at 3.9 0.75) (size 2 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.075) (tstamp 02e835bb-63e1-4bdd-a5ff-c7134c083042))
  (model "${KICAD6_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Jushuo_AFC07-S06FCA-00_1x6-1MP_P0.50_Horizontal.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "/home/stefan/kicad/library/3dmodels/Connector_FFC-FPC.3dshapes/FPC-SMD_P0.50-10P_LCS-SJ-H2.0.wrl"
    (offset (xyz 0 -0.75 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -180))
  )
)
