(footprint "DFN-6_2x2mm_P0.65mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "DFN, 6 Pin (https://www.diodes.com/assets/Package-Files/U-DFN2020-6%20(Type%20C).pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "DFN NoLead")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp cb09353c-188a-467d-bf0c-ed7ef0929c97)
  )
  (fp_text value "DFN-6_2x2mm_P0.65mm" (at 0 1.35) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp bddfa900-f1c3-4b17-a9de-167750cbe76d)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.35) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp bdcd6742-bf5f-49fb-b7b4-f35476e431ba)
  )
  (fp_line (start -1 1.11) (end 1 1.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dbcfec85-b30b-424b-8ab0-7bbe7577c517))
  (fp_line (start 0 -1.11) (end 1 -1.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 413108cd-b6b9-4a1c-837d-8772fffb6c45))
  (fp_line (start -1.4 0.7) (end -1.4 -0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 37b55467-e7ce-434c-a321-9b282bd3a977))
  (fp_line (start -1.247984 -0.945967) (end -1.25 -1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d73fdfe6-1a46-48b7-bdd4-e91890c8217c))
  (fp_line (start -1.247984 0.945967) (end -1.25 1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e400b2d2-21a0-4f0f-b97b-4ff324183457))
  (fp_line (start -1 -1.25) (end 1 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e9bd6e0f-bc35-4e6e-bcbc-2e30caf630fd))
  (fp_line (start 1 1.25) (end -1 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 51bd34e5-159c-4475-84bc-d13d7cfcf52f))
  (fp_line (start 1.247984 -0.945967) (end 1.25 -1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0df157c3-2e0e-4d80-9d08-90e6c2694158))
  (fp_line (start 1.247984 0.945967) (end 1.25 1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2338d260-ef5a-433d-8921-b23e3854e09e))
  (fp_line (start 1.4 -0.7) (end 1.4 0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f861b021-372d-4ac6-951c-438321a73717))
  (fp_arc (start -1.4 -0.7) (mid -1.358929 -0.844576) (end -1.247984 -0.945967)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 70ffaeb9-6352-4f60-8f5f-de07ae3a774e))
  (fp_arc (start -1.25 -1) (mid -1.176777 -1.176777) (end -1 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5ab03828-7616-438d-9b17-2d39614f4cb1))
  (fp_arc (start -1.247984 0.945967) (mid -1.358929 0.844576) (end -1.4 0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 43862b9f-cdb0-4935-bdd5-3b4bd0211a7d))
  (fp_arc (start -1 1.25) (mid -1.176777 1.176777) (end -1.25 1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fc4b54d1-5d34-4be1-adfd-90b71a7fa947))
  (fp_arc (start 1 -1.25) (mid 1.176777 -1.176777) (end 1.25 -1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9dead1e2-23d9-4bc4-ae3b-87cb10a4b643))
  (fp_arc (start 1.247984 -0.945967) (mid 1.358929 -0.844576) (end 1.4 -0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 998b9596-f43c-48ad-8ba3-92066a72ac11))
  (fp_arc (start 1.25 1) (mid 1.176777 1.176777) (end 1 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1bbfc65f-164f-4ba6-b725-4a8579f29777))
  (fp_arc (start 1.4 0.7) (mid 1.358929 0.844576) (end 1.247984 0.945967)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e3c05614-7572-450b-a487-798a4875ca72))
  (fp_line (start -1 -1) (end 1 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 02438bfa-0792-4500-8b4b-116d90eaba75))
  (fp_line (start -1 -0.5) (end -0.5 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b2cb8383-ff7d-417a-875c-bb2ccc470f1b))
  (fp_line (start -1 1) (end -1 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e1327bb1-ac26-48a6-a3c8-10a41df4164a))
  (fp_line (start 1 -1) (end 1 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 19b2cdcd-2203-4dc9-ba4a-32d814fbce12))
  (fp_line (start 1 1) (end -1 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6cc77169-c181-4e38-b4a7-004960216ee9))
  (pad "" smd oval (at -0.9 -0.65) (size 0.55 0.25) (layers "F.Paste") (tstamp e68688c3-b272-431e-aed8-b43dfb70ff49))
  (pad "" smd oval (at -0.9 0) (size 0.55 0.25) (layers "F.Paste") (tstamp 6f95e93e-a958-4235-a4b3-fe522be9dd80))
  (pad "" smd oval (at -0.9 0.65) (size 0.55 0.25) (layers "F.Paste") (tstamp efc7ab29-4ffc-4812-889d-38fdeb9fa2cd))
  (pad "" smd oval (at 0.9 -0.65) (size 0.55 0.25) (layers "F.Paste") (tstamp 01aaa08c-4d17-4a3f-a0ef-ab4ea71af0a1))
  (pad "" smd oval (at 0.9 0) (size 0.55 0.25) (layers "F.Paste") (tstamp 95c9b3ba-9cd6-47a9-aebd-d39de64fa32c))
  (pad "" smd oval (at 0.9 0.65) (size 0.55 0.25) (layers "F.Paste") (tstamp 1523a0e5-7c2b-477a-b99d-078d5b30ddee))
  (pad "1" smd roundrect (at -0.85 -0.65) (size 0.8 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right) (tstamp f4c37fe8-f38d-4457-8212-2917fbb2e4c8))
  (pad "2" smd roundrect (at -0.9 0) (size 0.7 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right) (tstamp fa348157-2c2f-43d7-99f5-cc766ba620a0))
  (pad "3" smd roundrect (at -0.9 0.65) (size 0.7 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right) (tstamp 2bd51187-dd81-4442-a9e6-01412c325629))
  (pad "4" smd roundrect (at 0.9 0.65 180) (size 0.7 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right) (tstamp c89b8ad9-8f30-44d2-a449-68c909985618))
  (pad "5" smd roundrect (at 0.9 0 180) (size 0.7 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right) (tstamp be119b50-b1ff-4639-95f1-af3078b500ba))
  (pad "6" smd roundrect (at 0.9 -0.65 180) (size 0.7 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.15) (chamfer top_right bottom_right) (tstamp 4a3892b6-e545-410c-93a2-5e7cecb58006))
  (model ":KICAD7_3DMODEL_DIR:Package_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
