(footprint "SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm_NumberLabels" (version 20210722) (generator pcbnew) (layer "F.Cu")
  (tedit 610BDBBC)
  (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers")
  (tags "net tie solder jumper bridged")
  (property "Sheetfile" "StepperDriverModuleCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "USD_per_1" "0,25")
  (property "USD_per_1000" "0,085")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "JP9" (at 0 -1.8) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 68a9884b-af37-4286-9d80-25e1f1ac85cb)
  )
  (fp_text value "MS2" (at 0 1.9) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f4430a7f-46dc-46cc-a7c7-65b07a593916)
  )
  (fp_poly (pts (xy -0.85 -0.15)
    (xy -0.4 -0.15)
    (xy -0.4 0.15)
    (xy -0.85 0.15)) (layer "F.Cu") (width 0) (fill solid) (tstamp 867b58f9-2c37-426a-9612-a47e4613dd94))
  (fp_line (start 2.05 -0.3) (end 2.05 0.3) (layer "F.SilkS") (width 0.12) (tstamp 57e31c57-d2fd-407a-bec2-c84ec85757b9))
  (fp_line (start -1.4 -1) (end 1.4 -1) (layer "F.SilkS") (width 0.12) (tstamp b9d38c0c-08fa-48aa-aed8-d3b61c5b842d))
  (fp_line (start 1.4 1) (end -1.4 1) (layer "F.SilkS") (width 0.12) (tstamp c3e75604-f518-4f99-84f3-97b8081aa177))
  (fp_line (start -2.05 0.3) (end -2.05 -0.3) (layer "F.SilkS") (width 0.12) (tstamp c65bd334-e7f1-43ed-ad9d-9a495e667603))
  (fp_arc (start 1.35 -0.3) (end 2.05 -0.3) (angle -90) (layer "F.SilkS") (width 0.12) (tstamp 732455ff-480a-455c-bb90-2939bd8e900a))
  (fp_arc (start -1.35 -0.3) (end -1.35 -1) (angle -90) (layer "F.SilkS") (width 0.12) (tstamp a8e74f19-a3d3-406e-b454-613a66b7700d))
  (fp_arc (start 1.35 0.3) (end 1.35 1) (angle -90) (layer "F.SilkS") (width 0.12) (tstamp d81f732e-2f0e-4420-ad85-d4a6e7c048f9))
  (fp_arc (start -1.35 0.3) (end -2.05 0.3) (angle -90) (layer "F.SilkS") (width 0.12) (tstamp fb2c7c85-53b5-45cd-a239-d2ddda5acb0c))
  (fp_line (start -2.3 -1.25) (end -2.3 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 39da749c-a8de-4c4e-9d86-0e548b8e054f))
  (fp_line (start 2.3 1.25) (end 2.3 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 82773c4c-47fe-477d-8e27-05e13f9e3503))
  (fp_line (start 2.3 1.25) (end -2.3 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 866154eb-f2f1-4a8c-9bfe-565598780d9e))
  (fp_line (start -2.3 -1.25) (end 2.3 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp f45e6b24-6107-4774-bdd1-bd0977fa0f25))
  (pad "1" smd custom (at -1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
        (xy 0.55 -0.75)
        (xy 0 -0.75)
        (xy 0 0.75)
        (xy 0.55 0.75)
      ) (width 0) (fill yes))
      (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
      (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
    ) (tstamp be297f2d-0428-4b5d-87c8-4159a99630c4))
  (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask") (tstamp 358370a3-63bf-4232-849c-db2c458a3d05))
  (pad "3" smd custom (at 1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
      (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
      (gr_poly (pts
        (xy -0.55 -0.75)
        (xy 0 -0.75)
        (xy 0 0.75)
        (xy -0.55 0.75)
      ) (width 0) (fill yes))
    ) (tstamp 5d59d247-92d5-4da0-b220-5f60e8f7d215))
)
