(module ST_LPS25HB (layer F.Cu) (tedit 552980FD)
  (solder_mask_margin -0.02)
  (solder_paste_margin -0.07)
  (attr smd)
  (fp_text reference REF** (at 0 -1.95) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value ST_LPS25HB (at 0 2) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_circle (center -1.8 -1.25) (end -1.9 -1.25) (layer F.SilkS) (width 0.2))
  (fp_line (start -1 1.45) (end -1.45 1.45) (layer F.SilkS) (width 0.127))
  (fp_line (start -1.45 1.45) (end -1.45 1) (layer F.SilkS) (width 0.127))
  (fp_line (start 1.45 1) (end 1.45 1.45) (layer F.SilkS) (width 0.127))
  (fp_line (start 1.45 1.45) (end 1 1.45) (layer F.SilkS) (width 0.127))
  (fp_line (start 1 -1.45) (end 1.45 -1.45) (layer F.SilkS) (width 0.127))
  (fp_line (start 1.45 -1.45) (end 1.45 -1) (layer F.SilkS) (width 0.127))
  (fp_line (start -1 -1.45) (end -1.45 -1.45) (layer F.SilkS) (width 0.127))
  (fp_line (start -1.45 -1.45) (end -1.45 -1) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.42 -0.21) (end 0.71 -0.21) (layer F.Fab) (width 0.05))
  (fp_line (start 0.71 -0.21) (end 0.71 0.91) (layer F.Fab) (width 0.05))
  (fp_line (start -0.42 0.91) (end 0.71 0.91) (layer F.Fab) (width 0.05))
  (fp_line (start -0.42 0.91) (end -0.42 -0.21) (layer F.Fab) (width 0.05))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 1.5) (end -1.5 -1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer F.CrtYd) (width 0.05))
  (pad 1 smd oval (at -1.1 -0.3) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -1.1 0.3) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at 1.1 0.3) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at 1.1 -0.3) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -0.6 1.1 90) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at 0 1.1 90) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at 0.6 1.1 90) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at 0.6 -1.1 90) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at 0 -1.1 90) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at -0.6 -1.1 90) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask))
)
