(footprint "JST_SHD_SM40B-SRDS-G-TF_2x20_P1.0_Right_Angle" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Field2" "")
  (property "Sheetfile" "Flight Controller.kicad_sch")
  (property "Sheetname" "Flight Controller")
  (property "ki_description" "Generic connectable mounting pin connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr through_hole)
  (fp_text reference "J32" (at -12.4 0 90 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 99bd2e7b-353d-4624-9700-6c783f299e9b)
  )
  (fp_text value "PWM" (at 0 4.3 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 49e00e30-3ea7-4104-bc44-b5ad816949df)
  )
  (fp_text user "${REF}" (at 0 1.15 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5fb6e351-feeb-4c8a-ba85-a15dc9d2f302)
  )
  (fp_arc (start -11.775 -2.7) (mid -11.753033 -2.753033) (end -11.7 -2.775)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 04a6fa6d-d81f-48ea-88b6-a75b260deb42))
  (fp_arc (start 11.7 -2.775) (mid 11.753033 -2.753033) (end 11.775 -2.7)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 9ac5cd04-e21e-4e56-acf7-16d90f4de1d2))
  (fp_poly
    (pts
      (xy 9.5 -3.75)
      (xy 9.4 -3.9)
      (xy 9.6 -3.9)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp c567bb77-3183-438f-8563-6266ac2a01d5))
  (fp_poly
    (pts
      (xy -9.95 2.85)
      (xy -10.6 2.85)
      (xy -10.6 2.7)
      (xy -9.95 2.7)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 78569853-26aa-4dcc-b85e-b6fac8597917))
  (fp_poly
    (pts
      (xy 10.6 2.85)
      (xy 9.95 2.85)
      (xy 9.95 2.7)
      (xy 10.6 2.7)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp a3e7fbe7-4ba1-4189-9779-98b21ec61816))
  (fp_poly
    (pts
      (xy -11.85 2.85)
      (xy -11.7 2.85)
      (xy -11.7 -2.7)
      (xy -9.95 -2.7)
      (xy -9.95 -2.85)
      (xy -11.7 -2.85)
      (xy -11.85 -2.7)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e8bcd049-dfc4-40ef-bbdb-880bdbc76761))
  (fp_poly
    (pts
      (xy 11.85 2.85)
      (xy 11.7 2.85)
      (xy 11.7 -2.7)
      (xy 9.95 -2.7)
      (xy 9.95 -2.85)
      (xy 11.7 -2.85)
      (xy 11.85 -2.7)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp afbb780e-8ca7-477f-81f1-a5194d75287f))
  (fp_line (start -11.8 -2.55) (end -11.75 2.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp efd46e61-449f-4a61-a9a7-9dbb0900d99e))
  (fp_line (start -11.55 -2.8) (end -9.95 -2.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1ac11f0d-06d6-4ccf-a5ee-1f0bb95bdea9))
  (fp_line (start -11.5 2.9) (end -9.95 2.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b2150809-6500-400f-a472-aa19355a9e17))
  (fp_line (start -9.95 -2.8) (end -9.95 -3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 95c28c14-58ed-4a8b-9727-40afd0ee2081))
  (fp_line (start -9.95 2.9) (end -9.95 3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5ecfcbf3-157e-49c9-b4ab-3bec3f0e8484))
  (fp_line (start -9.6 -3.8) (end 9.6 -3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4e8ab5ab-340f-4644-877b-d1e31dc56b4e))
  (fp_line (start 9.6 3.8) (end -9.6 3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a7d91819-fb65-4f7f-b329-78124427bf83))
  (fp_line (start 9.95 -2.8) (end 9.95 -3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2ba2707f-dd52-4f50-8f13-b6ec57b30bf0))
  (fp_line (start 9.95 2.9) (end 9.95 3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 20a0e6f4-2107-4d49-87ad-993c19616cd6))
  (fp_line (start 11.5 2.9) (end 9.95 2.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c2f533b1-7784-4820-aa32-b8ad53ed4739))
  (fp_line (start 11.55 -2.8) (end 9.95 -2.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fde5cf6d-2dd7-4afd-b7ba-1b3124bef1a8))
  (fp_line (start 11.8 -2.55) (end 11.75 2.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 80107b46-6994-4c68-af7e-01227fa33407))
  (fp_arc (start -11.8 -2.55) (mid -11.726777 -2.726777) (end -11.55 -2.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp cdc5e326-4333-416c-a6f2-9563da5a50f2))
  (fp_arc (start -11.5 2.9) (mid -11.676777 2.826777) (end -11.75 2.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ad1908ed-637c-4275-bc7b-3aa22740666c))
  (fp_arc (start -9.95 -3.45) (mid -9.847487 -3.697487) (end -9.6 -3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 721d6014-4561-48e3-a3b9-ac17a245a1e3))
  (fp_arc (start -9.6 3.8) (mid -9.847487 3.697487) (end -9.95 3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d3ffab15-53ea-42c1-81bc-0ba81df4405f))
  (fp_arc (start 9.6 -3.8) (mid 9.847487 -3.697487) (end 9.95 -3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9d4a7d52-3c16-471a-8eb6-b151d2c106ee))
  (fp_arc (start 9.95 3.45) (mid 9.847487 3.697487) (end 9.6 3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d0d9e056-a708-4d2c-9900-f89bae5f7fc5))
  (fp_arc (start 11.55 -2.8) (mid 11.726777 -2.726777) (end 11.8 -2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a92340fa-5290-4f9c-8c40-fe4ea806fd72))
  (fp_arc (start 11.75 2.65) (mid 11.676777 2.826777) (end 11.5 2.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 33334a06-cd7a-4278-8475-06dbecf74034))
  (fp_line (start -11.55 2.8) (end -11.55 3.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ff2b7834-9f17-42c7-b9d4-edb9edef50f4))
  (fp_line (start -11.55 3.3) (end -11.55 3.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15f09610-c708-4708-856a-13e4b22e822a))
  (fp_line (start -11.55 3.8) (end -11.55 4.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5d3a817b-411c-4ea0-a186-da8f0135afd1))
  (fp_line (start -11.55 4.3) (end -11.55 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6403585c-2a67-49f0-b56d-7ce36f84c024))
  (fp_line (start -11.55 4.55) (end -11.3 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b6802af-c26a-4aa0-8ffb-0b8eeef03d11))
  (fp_line (start -11 4.55) (end -10.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ee26d24b-6223-4c3b-b84d-ad3a51bb96f1))
  (fp_line (start -10.5 4.55) (end -10.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4adff96d-0ac2-4f99-a7bf-9c40f2ab470e))
  (fp_line (start -10 4.55) (end -9.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 51e5adba-d615-457b-b1f7-789d33e92c7a))
  (fp_line (start -9.5 4.55) (end -9.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 399bba57-6320-4f80-bed0-793890f33ce6))
  (fp_line (start -4 4.55) (end -3.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f21606fd-2a90-44bf-94b4-1d237a737840))
  (fp_line (start -3.5 4.55) (end -3.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8207fccf-4fee-4ae4-8de8-046917a97ef6))
  (fp_line (start -3 4.55) (end -2.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b5b0f79e-1e64-4219-ad51-115245ab54cf))
  (fp_line (start -2.5 4.55) (end -2.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2867b583-91d8-4fbe-9cca-b9af30308b89))
  (fp_line (start -2 4.55) (end -1.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1dd4f62c-0eb3-447d-8ae1-6ab135f034f9))
  (fp_line (start -1.5 4.55) (end -1.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 34b085cf-68a9-4c9e-a73d-04e56fdef900))
  (fp_line (start -1 4.55) (end -0.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7f566b06-2a36-408e-9b15-df2b41d73e9c))
  (fp_line (start -0.5 4.55) (end -0.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1f6f7700-a05b-44fc-9ed8-0378d0ea2c1e))
  (fp_line (start 0.25 4.55) (end 0.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ce14926f-00a4-4e85-8d3e-5395d7eaf820))
  (fp_line (start 0.75 4.55) (end 1 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f9207daa-cf10-498b-992e-243ae3677f26))
  (fp_line (start 1.25 4.55) (end 1.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d6425363-ccfd-453e-9932-80e79287a2c5))
  (fp_line (start 1.75 4.55) (end 2 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cd99d841-e1c3-499b-ba99-081d4f475a0f))
  (fp_line (start 2.25 4.55) (end 2.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 66c97d5e-82c7-4970-802e-af6c2ba6bb60))
  (fp_line (start 2.75 4.55) (end 3 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0a93cbb8-97ed-4615-9170-2e41d38bab2f))
  (fp_line (start 3.25 4.55) (end 3.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 455e511b-6560-40f5-842e-a3a5240a0a5c))
  (fp_line (start 3.75 4.55) (end 4 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a498ebee-f150-4f9c-94f2-a6eebdd1a5c1))
  (fp_line (start 9.25 4.55) (end 9.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f307ad50-14fb-4285-bf57-4a710ae64614))
  (fp_line (start 9.75 4.55) (end 10 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 43d1f0b2-9431-420d-b8b9-14c29d29a485))
  (fp_line (start 10.25 4.55) (end 10.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 22882644-fb12-4d69-a116-50b759099e45))
  (fp_line (start 10.75 4.55) (end 11 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b8e2276e-4586-4aa9-8e6b-1b97fe59cbf6))
  (fp_line (start 11.55 2.8) (end 11.55 3.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 035ff582-9e62-46b3-8ba0-461a3bec7b88))
  (fp_line (start 11.55 3.3) (end 11.55 3.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d1802c2d-0f4c-47fd-a56e-a6244e913e14))
  (fp_line (start 11.55 3.8) (end 11.55 4.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 59d84a85-5c34-4ba1-a41c-e8241e3017c0))
  (fp_line (start 11.55 4.3) (end 11.55 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f4bba12d-ed01-47a4-9cbb-14ccb8b0a190))
  (fp_line (start 11.55 4.55) (end 11.3 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2574a2e7-0600-43d1-a0a9-510895476033))
  (fp_rect (start -11.55 2.55) (end 11.55 -2.55)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 6aa641e0-b2c9-4962-8693-d6dd6b6b87da))
  (pad "1" smd roundrect (at 9.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 20656fca-a928-4c61-a8e1-4e2989d93105))
  (pad "2" smd roundrect (at 9.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 862618d4-b9b4-4b47-81e4-e4e7ed11781a))
  (pad "3" smd roundrect (at 8.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp e79234ea-94dd-4b5f-a3f8-2de892412b1b))
  (pad "4" smd roundrect (at 8.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 1908e435-4776-48a4-b7f0-7fea88fbb5f9))
  (pad "5" smd roundrect (at 7.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 9e18ee70-c36a-4155-afe8-a841fbcab98c))
  (pad "6" smd roundrect (at 7.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 4d8b5e2d-f51f-440b-83f8-8d7e1e3250b1))
  (pad "7" smd roundrect (at 6.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 96228e0b-eb23-4b7c-a4bf-2c96e7d1e616))
  (pad "8" smd roundrect (at 6.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 92c72bd1-a7ca-4169-bff8-057b86baae61))
  (pad "9" smd roundrect (at 5.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 22e03341-7d3b-4525-8f20-49bbf81194fb))
  (pad "10" smd roundrect (at 5.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 643be91a-5b1b-4054-993f-929c68787326))
  (pad "11" smd roundrect (at 4.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp cfb03fa4-309f-4e66-9217-672b09d14589))
  (pad "12" smd roundrect (at 4.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 200944ec-a44c-4049-8750-353b6f52b0ca))
  (pad "13" smd roundrect (at 3.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp bdbf5d24-14ec-4712-a49c-dd033bc6e2e9))
  (pad "14" smd roundrect (at 3.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 222718e2-b07d-4d3d-a84f-5ac424144193))
  (pad "15" smd roundrect (at 2.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 45ec0407-d032-429e-bccb-6c994aad3c3d))
  (pad "16" smd roundrect (at 2.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp acb1030a-c923-4e3f-8c30-842a350625f2))
  (pad "17" smd roundrect (at 1.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 84c68469-db3e-477f-b840-a5a5fba309a9))
  (pad "18" smd roundrect (at 1.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp fb5e0545-4734-4db1-8d14-de2cad4e937a))
  (pad "19" smd roundrect (at 0.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 77898057-d99b-447c-a2db-062ab2dcee13))
  (pad "20" smd roundrect (at 0.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp d1b92394-1625-4411-9baf-250c7d7f2702))
  (pad "21" smd roundrect (at -0.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp cfc3c37d-2370-48ca-a208-2abf2804b97d))
  (pad "22" smd roundrect (at -0.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp b8ceb660-2afb-44b9-9132-104787472ddd))
  (pad "23" smd roundrect (at -1.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp f6c97816-2149-4751-8d37-f57ff61b6dca))
  (pad "24" smd roundrect (at -1.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 845ce37d-6bb4-4508-b6d2-5ef3a501e3f8))
  (pad "25" smd roundrect (at -2.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 1a9e4909-cace-4954-9b39-6761487d23e9))
  (pad "26" smd roundrect (at -2.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp a0fdbfee-a83e-4bb7-9def-d829ec5d7b6d))
  (pad "27" smd roundrect (at -3.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp f5eaa7e7-e208-4017-911a-8c1c5c37d1d4))
  (pad "28" smd roundrect (at -3.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp b8fb6c8b-a0f0-4b65-8792-1389f01f1ce2))
  (pad "29" smd roundrect (at -4.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 90af98ba-a4d7-4f78-aa9e-4bedeaaf20dd))
  (pad "30" smd roundrect (at -4.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 6ba402e7-0e60-4eb6-bc1d-2656ec4c781a))
  (pad "31" smd roundrect (at -5.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 151e2343-8d82-43fb-901b-8d6934ab118c))
  (pad "32" smd roundrect (at -5.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 53d85815-a83f-40d5-83dc-19bf8a73709c))
  (pad "33" smd roundrect (at -6.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp ed70ed54-76ff-49d1-8e21-a4d441eb845e))
  (pad "34" smd roundrect (at -6.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 7ffc8325-d5c3-4baa-840f-a9eb962450fa))
  (pad "35" smd roundrect (at -7.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp ff8a6f19-be36-463a-9e91-443610dd6dde))
  (pad "36" smd roundrect (at -7.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 84a1b20e-8c1d-4a22-9ec7-778be20236f5))
  (pad "37" smd roundrect (at -8.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 98122a6a-c915-4571-af03-83e35594bffa))
  (pad "38" smd roundrect (at -8.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp f7f09746-fe5f-4d7b-aa13-9c6252572a6b))
  (pad "39" smd roundrect (at -9.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 050e7b02-367d-4078-82b1-0d78ff10f55f))
  (pad "40" smd roundrect (at -9.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp d3027076-25f1-4b57-bed3-e39ffba8d540))
  (pad "MP" smd roundrect (at -11.175 1.85) (size 0.85 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.118) (tstamp 41686522-788b-4689-8534-d89feaa7123a))
  (pad "MP" smd roundrect (at 11.175 1.85) (size 0.85 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.118) (tstamp 8d47c37b-e3ad-4d9f-91b8-a6d803ecad4b))
  (model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/SM40B-SRDS-G-TF.STEP"
    (offset (xyz 0 -2.55 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -90))
  )
)
