(footprint "1P_7x4.5_SQ" (version 20210424) (generator pcbnew) (layer "F.Cu")
  (tedit 609BD37C)
  (property "Sheetfile" "ESC12S30.kicad_sch")
  (property "Sheetname" "")
  (fp_text reference "J1" (at -4.25 0 90 unlocked) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 36bc9efb-14ca-41f4-b038-ffbe9a6781fa)
  )
  (fp_text value "A" (at -0.1 -8.725 unlocked) (layer "F.Fab") hide
    (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp 07540996-8a72-4ba8-82c1-db34d4014a63)
  )
  (fp_text user "${REF}" (at -0.1 -7.225 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fdb2e782-1f39-4c37-a13a-b784681029d1)
  )
  (pad "1" connect rect (at 0 0) (size 7 4.5) (layers "F.Cu" "F.Mask") (tstamp 6b325a24-6993-4ca3-a82c-88b95a6eb020))
)
