(footprint "Arc_Ri0.9_0.15-0.15_x12_180deg" (version 20221019) (generator pcbnew)
  (layer "F.Cu")
  (zone_connect 0)
  (attr board_only exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -8.075 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2c79dc91-7d87-4312-a8b9-19715fd00ffa)
  )
  (fp_text value "Arc_Ri0.9_0.15-0.15_x12_180deg" (at 0 -6.575 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5beec144-4cc1-474b-a704-c5bb50798690)
  )
  (fp_text user "${REFERENCE}" (at 0 -5.075 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 329fd6c7-7418-4566-b934-69bde1aafa29)
  )
  (pad "1" smd custom (at -0.975 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.975 -0.975) (end 1.95 0) (width 0.15))
    ))
  (pad "1" smd custom (at 0.975 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -1.95 0) (mid -0.975 -0.975) (end 0 0) (width 0.15))
    ))
  (pad "2" smd custom (at -1.275 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 1.275 -1.275) (end 2.55 0) (width 0.15))
    ))
  (pad "2" smd custom (at 1.275 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -2.55 0) (mid -1.275 -1.275) (end 0 0) (width 0.15))
    ))
  (pad "3" smd custom (at -1.575 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 1.575 -1.575) (end 3.15 0) (width 0.15))
    ))
  (pad "3" smd custom (at 1.575 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.15 0) (mid -1.575 -1.575) (end 0 0) (width 0.15))
    ))
  (pad "4" smd custom (at -1.875 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 1.875 -1.875) (end 3.75 0) (width 0.15))
    ))
  (pad "4" smd custom (at 1.875 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.75 0) (mid -1.875 -1.875) (end 0 0) (width 0.15))
    ))
  (pad "5" smd custom (at -2.175 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 2.175 -2.175) (end 4.35 0) (width 0.15))
    ))
  (pad "5" smd custom (at 2.175 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -4.35 0) (mid -2.175 -2.175) (end 0 0) (width 0.15))
    ))
  (pad "6" smd custom (at -2.475 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 2.475 -2.475) (end 4.95 0) (width 0.15))
    ))
  (pad "6" smd custom (at 2.475 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -4.95 0) (mid -2.475 -2.475) (end 0 0) (width 0.15))
    ))
  (pad "7" smd custom (at -2.775 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 2.775 -2.775) (end 5.55 0) (width 0.15))
    ))
  (pad "7" smd custom (at 2.775 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -5.55 0) (mid -2.775 -2.775) (end 0 0) (width 0.15))
    ))
  (pad "8" smd custom (at -3.075 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 3.075 -3.075) (end 6.15 0) (width 0.15))
    ))
  (pad "8" smd custom (at 3.075 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -6.15 0) (mid -3.075 -3.075) (end 0 0) (width 0.15))
    ))
  (pad "9" smd custom (at -3.375 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 3.375 -3.375) (end 6.75 0) (width 0.15))
    ))
  (pad "9" smd custom (at 3.375 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -6.75 0) (mid -3.375 -3.375) (end 0 0) (width 0.15))
    ))
  (pad "10" smd custom (at -3.675 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 3.675 -3.675) (end 7.35 0) (width 0.15))
    ))
  (pad "10" smd custom (at 3.675 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -7.35 0) (mid -3.675 -3.675) (end 0 0) (width 0.15))
    ))
  (pad "11" smd custom (at -3.975 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 3.975 -3.975) (end 7.95 0) (width 0.15))
    ))
  (pad "11" smd custom (at 3.975 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -7.95 0) (mid -3.975 -3.975) (end 0 0) (width 0.15))
    ))
  (pad "12" smd custom (at -4.275 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 4.275 -4.275) (end 8.55 0) (width 0.15))
    ))
  (pad "12" smd custom (at 4.275 0) (size 0.15 0.15) (layers "F.Cu")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -8.55 0) (mid -4.275 -4.275) (end 0 0) (width 0.15))
    ))
)

