(module ST_IIS2DH (layer F.Cu) (tedit 5751603A)
  (solder_mask_margin -0.02)
  (solder_paste_margin -0.06)
  (attr smd)
  (fp_text reference U10 (at 0 -1.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value ST_IIS2DH (at 0 1.75) (layer F.Fab)
    (effects (font (size 0.4 0.4) (thickness 0.1)))
  )
  (fp_line (start -1 -1) (end 1 -1) (layer F.Fab) (width 0.05))
  (fp_line (start 1 -1) (end 1 1) (layer F.Fab) (width 0.05))
  (fp_line (start 1 1) (end -1 1) (layer F.Fab) (width 0.05))
  (fp_line (start -1 1) (end -1 -1) (layer F.Fab) (width 0.05))
  (fp_line (start -1.2 1) (end -1.2 1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.2 1.2) (end 1.2 1) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.2 -1.2) (end 1.2 -1) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.2 -1.2) (end -1.2 -1) (layer F.SilkS) (width 0.125))
  (fp_circle (center -1.45 -1.1) (end -1.55 -1.1) (layer F.SilkS) (width 0.125))
  (fp_line (start 0.8 1.2) (end 1.2 1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.2 1.2) (end -0.8 1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start 0.8 -1.2) (end 1.2 -1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.2 -1.2) (end -0.8 -1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.25 -1.25) (end 1.25 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.25 1.25) (end -1.25 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.25 1.25) (end -1.25 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.25 -1.25) (end 1.25 -1.25) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -0.925 -0.75) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad 2 smd roundrect (at -0.925 -0.25) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad 3 smd roundrect (at -0.925 0.25) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad 4 smd roundrect (at -0.925 0.75) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad 7 smd roundrect (at 0.9375 0.75) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad 8 smd roundrect (at 0.9375 0.25) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad 9 smd roundrect (at 0.9375 -0.25) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad 10 smd roundrect (at 0.925 -0.75) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad 11 smd roundrect (at 0.25 -0.925 90) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad 12 smd roundrect (at -0.25 -0.925 90) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad 5 smd roundrect (at -0.25 0.925 90) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad 6 smd roundrect (at 0.25 0.925 90) (size 0.65 0.29) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.33))
  (pad "" smd roundrect (at 0 0 90) (size 1.1 1.1) (layers F.Mask)(roundrect_rratio 0.05))
)
