(module Address_pads_3P_linear (layer F.Cu) (tedit 586D2F77)
  (solder_mask_margin 0.001)
  (solder_paste_margin -0.001)
  (attr virtual)
  (fp_text reference REF** (at 1 0 270) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value Address_pads_3P_waver (at 0 -2.1) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.03175)))
  )
  (fp_text user 0 (at -0.9 -1.2) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user 1 (at -0.9 0) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user 2 (at -0.9 1.2) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -0.7 -1.8) (end -1.1 -1.8) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.7 -0.6) (end -1.1 -0.6) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.1 -0.6) (end -1.1 -0.7) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.1 -0.7) (end -1.1 -0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.7 0.6) (end -1.1 0.6) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.1 0.6) (end -1.1 0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.1 0.5) (end -1.1 0.7) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.7 1.8) (end -1.1 1.8) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.7 -0.7) (end -0.7 -0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.7 0.5) (end -0.7 0.7) (layer F.SilkS) (width 0.125))
  (pad 1 connect rect (at 0 0) (size 1 0.4) (layers F.Cu F.Mask))
  (pad 2 connect rect (at 0 1.2) (size 1 0.4) (layers F.Cu F.Mask))
  (pad 0 connect rect (at 0 -1.2) (size 1 0.4) (layers F.Cu F.Mask))
  (pad H connect rect (at 0 -0.6) (size 1 0.4) (layers F.Cu F.Mask))
  (pad L connect rect (at 0 1.8) (size 1 0.4) (layers F.Cu F.Mask))
  (pad L connect rect (at 0 -1.8) (size 1 0.4) (layers F.Cu F.Mask))
  (pad H connect rect (at 0 0.6) (size 1 0.4) (layers F.Cu F.Mask))
  (pad 3 connect roundrect (at 0 0) (size 1.1 4.1) (layers F.Mask)(roundrect_rratio 0.045))
)
