(module LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 58610E52)
  (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
  (tags "QFP 0.5")
  (solder_mask_margin 0.025)
  (attr smd)
  (fp_text reference U2 (at -4.2 -4.2) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value STM32L152CCTx (at 0 5.7) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -3.6 -3.1) (end -4.7 -3.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.6 -3.6) (end 3.1 -3.6) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.6 3.6) (end 3.1 3.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.6 3.6) (end -3.1 3.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.6 -3.6) (end -3.1 -3.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.6 3.6) (end -3.6 3.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.6 3.6) (end 3.6 3.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.6 -3.6) (end 3.6 -3.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.6 -3.6) (end -3.6 -3.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.2 5.1) (end 3.2 5.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.2 -5.1) (end 3.2 -5.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.1 -3.2) (end 5.1 3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.1 -3.2) (end -5.1 3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.5 3.5) (end -3.5 -3.5) (layer F.Fab) (width 0.05))
  (fp_line (start 3.5 3.5) (end -3.5 3.5) (layer F.Fab) (width 0.05))
  (fp_line (start 3.5 -3.5) (end 3.5 3.5) (layer F.Fab) (width 0.05))
  (fp_line (start -3.5 -3.5) (end 3.5 -3.5) (layer F.Fab) (width 0.05))
  (fp_text user %R (at 0 2.9) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_circle (center -3.1 -3.1) (end -3.1 -3.3) (layer F.Fab) (width 0.05))
  (fp_line (start -5.1 -3.2) (end -3.8 -3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.8 -3.2) (end -3.8 -3.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.8 -3.8) (end -3.2 -3.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.2 -3.8) (end -3.2 -5.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.2 -5.1) (end 3.2 -3.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.2 -3.8) (end 3.8 -3.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.8 -3.8) (end 3.8 -3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.8 -3.2) (end 5.1 -3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.1 3.2) (end 3.8 3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.8 3.2) (end 3.8 3.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.8 3.8) (end 3.2 3.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.2 3.8) (end 3.2 5.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.2 5.1) (end -3.2 3.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.2 3.8) (end -3.8 3.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.8 3.8) (end -3.8 3.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.8 3.2) (end -5.1 3.2) (layer F.CrtYd) (width 0.05))
  (pad 13 smd roundrect (at -2.75 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 1 smd roundrect (at -4.25 -2.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 2 smd roundrect (at -4.25 -2.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 3 smd roundrect (at -4.25 -1.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 4 smd roundrect (at -4.25 -1.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 5 smd roundrect (at -4.25 -0.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 6 smd roundrect (at -4.25 -0.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 7 smd roundrect (at -4.25 0.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 8 smd roundrect (at -4.25 0.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 9 smd roundrect (at -4.25 1.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 10 smd roundrect (at -4.25 1.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 11 smd roundrect (at -4.25 2.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 12 smd roundrect (at -4.25 2.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 25 smd roundrect (at 4.25 2.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 14 smd roundrect (at -2.25 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 15 smd roundrect (at -1.75 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 16 smd roundrect (at -1.25 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 17 smd roundrect (at -0.75 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 18 smd roundrect (at -0.25 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 19 smd roundrect (at 0.25 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 20 smd roundrect (at 0.75 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 21 smd roundrect (at 1.25 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 22 smd roundrect (at 1.75 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 23 smd roundrect (at 2.25 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 24 smd roundrect (at 2.75 4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 37 smd roundrect (at 2.75 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 26 smd roundrect (at 4.25 2.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 27 smd roundrect (at 4.25 1.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 28 smd roundrect (at 4.25 1.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 29 smd roundrect (at 4.25 0.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 30 smd roundrect (at 4.25 0.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 31 smd roundrect (at 4.25 -0.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 32 smd roundrect (at 4.25 -0.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 33 smd roundrect (at 4.25 -1.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 34 smd roundrect (at 4.25 -1.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 35 smd roundrect (at 4.25 -2.25) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 36 smd roundrect (at 4.25 -2.75) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 38 smd roundrect (at 2.25 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 39 smd roundrect (at 1.75 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 40 smd roundrect (at 1.25 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 41 smd roundrect (at 0.75 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 42 smd roundrect (at 0.25 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 43 smd roundrect (at -0.25 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 44 smd roundrect (at -0.75 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 45 smd roundrect (at -1.25 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 46 smd roundrect (at -1.75 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 47 smd roundrect (at -2.25 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (pad 48 smd roundrect (at -2.75 -4.25 90) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.3))
  (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
