(footprint "SolderJumper-2_1.2x1.2mm_Bridged_Rounded"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
	(tags "net tie solder jumper bridged")
	(property "Reference" "JP7"
		(at 0 -1.8 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "58a1a450-ad38-4019-a3a3-d0f02e1bf186")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "IMU-AUX_SDA"
		(at 0 1.9 180)
		(layer "F.Fab")
		(uuid "826e3681-1650-44ad-b9bd-4a32e394a525")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Jumper:SolderJumper-2_1.2x1.2mm_Bridged_Rounded"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7a31e07c-b695-45e8-bc15-f92391d93d90")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cd5e22c9-c2dd-48c4-8698-4c7f6132a495")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Solder Jumper, 2-pole, closed/bridged"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3c70ff0c-a8db-486b-8d8a-8d03716a3c68")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Enable" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d4e892a2-8da2-4be5-bddb-40b266f2cfe0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(net_tie_pad_groups "1, 2")
	(fp_poly
		(pts
			(xy 0.15 -0.1) (xy -0.15 -0.1) (xy -0.15 0.1) (xy 0.15 0.1)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.Cu")
		(uuid "1029cd0e-f1fb-45da-afa3-9459dde75d46")
	)
	(fp_line
		(start -0.9 0.3)
		(end -0.9 -0.3)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3d1486f8-24db-49b4-bcbd-241badf7c2f2")
	)
	(fp_line
		(start -0.4 -0.8)
		(end 0.4 -0.8)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d5d14e2b-12a2-49ee-9a96-59e5ab3e5573")
	)
	(fp_line
		(start 0.4 0.8)
		(end -0.4 0.8)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "65fbaed7-509e-4da0-b61c-4879211a22c5")
	)
	(fp_line
		(start 0.9 -0.3)
		(end 0.9 0.3)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "04a403cc-af80-4bf1-81f5-e29eecdb4172")
	)
	(fp_arc
		(start -0.9 -0.3)
		(mid -0.753553 -0.653553)
		(end -0.4 -0.8)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f96f4847-ee41-43c9-8d6d-56d08be86034")
	)
	(fp_arc
		(start -0.4 0.8)
		(mid -0.753553 0.653553)
		(end -0.9 0.3)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "7c3ef44b-82c9-471b-a3fe-3c9ed43b07c4")
	)
	(fp_arc
		(start 0.4 -0.8)
		(mid 0.753553 -0.653553)
		(end 0.9 -0.3)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "17648670-c2c1-4dd2-b359-7b4eec0fa5b1")
	)
	(fp_arc
		(start 0.9 0.3)
		(mid 0.753553 0.653553)
		(end 0.4 0.8)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ae385f2f-1f5e-4819-9803-40ca313c7614")
	)
	(fp_poly
		(pts
			(xy 0.1 0.6) (xy 0.1 -0.6) (xy -0.1 -0.6) (xy -0.1 0.6)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.Mask")
		(uuid "4380515a-fddb-47d5-a808-35aa93cd50cb")
	)
	(fp_line
		(start -0.949999 -0.3)
		(end -0.949999 0.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9e75e97c-79f5-4fde-8823-5f418b5c45ec")
	)
	(fp_line
		(start -0.4 0.85)
		(end 0.4 0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8cfeeae8-529e-4662-b251-de29ecb83fa5")
	)
	(fp_line
		(start 0.4 -0.85)
		(end -0.4 -0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8f6aa3bb-979c-45de-9bb8-89ccd95bd8a1")
	)
	(fp_line
		(start 0.949999 0.3)
		(end 0.949999 -0.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "66dd99f7-4d86-49c1-a12d-6355ea0adbe0")
	)
	(fp_arc
		(start -0.949999 -0.3)
		(mid -0.788908 -0.688908)
		(end -0.4 -0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fecdc722-7397-4c7a-95d8-5dc05292e185")
	)
	(fp_arc
		(start -0.4 0.85)
		(mid -0.788909 0.688909)
		(end -0.949999 0.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "196a5a47-7aa8-4c15-b758-0d86aec76f3d")
	)
	(fp_arc
		(start 0.4 -0.85)
		(mid 0.788909 -0.688909)
		(end 0.949999 -0.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3f8ef6ec-8275-44da-b99c-e52a2f75df2d")
	)
	(fp_arc
		(start 0.949999 0.3)
		(mid 0.788908 0.688908)
		(end 0.4 0.85)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9803a7a6-04e8-4f64-a551-af8f115badda")
	)
	(pad "1" smd roundrect
		(at -0.499999 0 180)
		(size 0.6 1.2)
		(drill
			(offset -0.1 0)
		)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left bottom_left)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.2)
			(max_length 0.2)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2310968a-d664-42b4-9304-63e484b40707")
	)
	(pad "2" smd roundrect
		(at 0.499999 0)
		(size 0.6 1.2)
		(drill
			(offset -0.1 0)
		)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left bottom_left)
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.2)
			(max_length 0.2)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4fe58d9e-9883-4cdc-baa3-2f91808646e0")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "8c05b7e7-3c04-4c9e-bb93-853218233b85")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.075 -0.6) (xy -0.075 -0.125) (xy 0.075 -0.125) (xy 0.075 -0.6)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "f53c982b-4480-4c1d-ab17-33b19ce315e7")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.075 0.125) (xy -0.075 0.6) (xy 0.075 0.6) (xy 0.075 0.125)
			)
		)
	)
)
