(module Program_Pogo_5P_1.25mm (layer F.Cu) (tedit 547E2474)
  (solder_mask_margin 0.001)
  (fp_text reference P1 (at -1.8 0 90) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value CONN-5 (at 1.7 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user 1 (at 0 -3.7) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (pad 1 thru_hole rect (at 0 -2.5) (size 2 1.05) (drill 0.74) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 -1.25) (size 2 1.05) (drill 0.74) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 0) (size 2 1.05) (drill 0.74) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 1.25) (size 2 1.05) (drill 0.74) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 0 2.5) (size 2 1.05) (drill 0.74) (layers *.Cu *.Mask))
)
