(module Kingbright_APBD3224LSURKCGKC_Dual_SMD_LED (layer F.Cu) (tedit 5BEC75E8)
  (solder_mask_margin 0.02)
  (solder_paste_margin -0.02)
  (fp_text reference D1 (at 0 -1.9) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value PWR_READY (at 0 1.7) (layer F.Fab)
    (effects (font (size 0.2 0.2) (thickness 0.05)))
  )
  (fp_line (start 1.6 -1.2) (end 1.6 1.2) (layer F.Fab) (width 0.05))
  (fp_line (start 1.6 1.2) (end -1.6 1.2) (layer F.Fab) (width 0.05))
  (fp_line (start -1.6 1.2) (end -1.6 -1.2) (layer F.Fab) (width 0.05))
  (fp_line (start -1.6 -1.2) (end 1.6 -1.2) (layer F.Fab) (width 0.05))
  (fp_circle (center 0 0) (end 0 -1) (layer F.Fab) (width 0.05))
  (fp_circle (center 2.1 -1.4) (end 2.1 -1.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.7 -1.2) (end -1.7 -1.3) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.7 -1.3) (end 1.7 -1.3) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.7 -1.3) (end 1.7 -1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.7 1.2) (end -1.7 1.3) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.7 1.3) (end 1.7 1.3) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.7 1.3) (end 1.7 1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.7 -0.2) (end 1.7 0.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.7 0) (end -2 -0.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -2 -0.2) (end -2 0.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -2 0.2) (end -1.7 0) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.9 -0.1) (end -1.9 0.1) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.9 0.1) (end -1.8 0) (layer F.SilkS) (width 0.125))
  (fp_text user "Polarity Mark" (at -1.4 0 90) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.03175)))
  )
  (fp_circle (center 0 -0.3) (end 0 -0.4) (layer F.Fab) (width 0.05))
  (fp_circle (center 0 0.3) (end 0 0.2) (layer F.Fab) (width 0.05))
  (fp_text user RED (at 0.4 -0.3) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.03175)))
  )
  (fp_text user GREEN (at 0.5 0.3) (layer F.Fab)
    (effects (font (size 0.127 0.127) (thickness 0.03175)))
  )
  (fp_line (start -0.15 -0.7) (end 0.15 -0.7) (layer F.Fab) (width 0.05))
  (fp_line (start -0.05 -0.8) (end -0.05 -0.6) (layer F.Fab) (width 0.05))
  (fp_line (start -0.05 -0.6) (end -0.05 -0.6) (layer F.Fab) (width 0.05))
  (fp_line (start -0.05 -0.7) (end 0.05 -0.8) (layer F.Fab) (width 0.05))
  (fp_line (start 0.05 -0.8) (end 0.05 -0.6) (layer F.Fab) (width 0.05))
  (fp_line (start 0.05 -0.6) (end -0.05 -0.7) (layer F.Fab) (width 0.05))
  (fp_line (start -0.15 0.7) (end 0.15 0.7) (layer F.Fab) (width 0.05))
  (fp_line (start -0.05 0.7) (end 0.05 0.6) (layer F.Fab) (width 0.05))
  (fp_line (start 0.05 0.8) (end -0.05 0.7) (layer F.Fab) (width 0.05))
  (fp_line (start -0.05 0.6) (end -0.05 0.8) (layer F.Fab) (width 0.05))
  (fp_line (start 0.05 0.6) (end 0.05 0.8) (layer F.Fab) (width 0.05))
  (fp_line (start -0.05 0.8) (end -0.05 0.8) (layer F.Fab) (width 0.05))
  (pad RA smd roundrect (at 1.6 -0.7) (size 1.6 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad RK smd roundrect (at -1.6 -0.7) (size 1.6 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad GA smd roundrect (at 1.6 0.7) (size 1.6 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad GK smd roundrect (at -1.6 0.7) (size 1.6 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (model LED_SMD.3dshapes/Kingbright_APBD3224LSURKCGKC.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
