(footprint "USB_C_Receptacle_XKB_U263-24XN-4BQC14" (version 20210228) (generator pcbnew) (layer "F.Cu")
  (tedit 6065B8F5)
  (property "MPN" "U263-24XN-4BQC14")
  (property "Sheet file" "/home/stefan/Projects/Current/Thunderbolt3_PCB/Thunderbolt3_PCB.kicad_sch")
  (property "Sheet name" "")
  (attr smd)
  (fp_text reference "J2" (at 0 1.875 -90 unlocked) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify left))
    (tstamp 3ee1729b-c69b-4483-9202-4aa7703d28c7)
  )
  (fp_text value "U263-24XN-4BQC14" (at 0 -6.56 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b6d2b97f-4a32-4ef1-a5dd-a91e11ff2d71)
  )
  (fp_text user "${REF}" (at 0 -8.27 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp db3ddf19-6591-4190-ba42-c8879880d9f8)
  )
  (fp_line (start -4.75 0) (end 4.75 0) (layer "F.SilkS") (width 0.05) (tstamp 29838348-c849-4ae6-8224-b4abe8ceab64))
  (fp_line (start -4.55 -3.65) (end -5.05 -3.65) (layer "Dwgs.User") (width 0.01) (tstamp 1d5f6eff-afe5-4eb4-8338-8f6840c4d1f2))
  (fp_line (start 2.17 0) (end 4.55 0) (layer "Dwgs.User") (width 0.01) (tstamp 1e819e43-863a-4005-ac62-a27c623bd7ae))
  (fp_line (start 4.55 -3.65) (end 5.05 -3.65) (layer "Dwgs.User") (width 0.01) (tstamp 2f384ec8-1cb8-4d44-8d7a-7a5abf172c95))
  (fp_line (start -4.55 0) (end -4.55 -3.65) (layer "Dwgs.User") (width 0.01) (tstamp 37fcbbb8-d670-4f36-b4b1-ecfec8f2485c))
  (fp_line (start 2.17 -0.4) (end 2.17 0) (layer "Dwgs.User") (width 0.01) (tstamp 410fe47a-fdcc-40c2-b663-2e5183df563b))
  (fp_line (start -4.55 0) (end -2.17 0) (layer "Dwgs.User") (width 0.01) (tstamp 594b52ec-2d76-4e5b-a465-a55fbd40d19d))
  (fp_line (start -2.17 0) (end -2.17 -0.4) (layer "Dwgs.User") (width 0.01) (tstamp 973aac86-f270-433c-bc51-1cbf9f461916))
  (fp_line (start 4.55 0) (end 4.55 -3.65) (layer "Dwgs.User") (width 0.01) (tstamp a3f4fb2e-6c2c-48d6-b8ea-b67be9ff0a0c))
  (fp_line (start -2.17 -0.4) (end 2.17 -0.4) (layer "Dwgs.User") (width 0.01) (tstamp c9c180a2-e7a4-4c04-963b-67b056e9701f))
  (fp_poly (pts (xy 4.47 1.05)
    (xy 3.9 1.05)
    (xy 3.9 0)
    (xy -3.9 0)
    (xy -3.9 1.05)
    (xy -4.47 1.05)
    (xy -4.47 -5.75)
    (xy 4.47 -5.75)) (layer "F.Fab") (width 0) (fill solid) (tstamp f558b7d7-eab5-4642-b40c-75cb1e6cf0e1))
  (pad "A1" smd roundrect (at 2.75 0.9) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp c4908fd6-575f-4f4a-a2d4-7b744afc7bc9))
  (pad "A2" smd roundrect (at 2.25 0.9) (size 0.25 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 3e45c1ec-dc8d-4a8d-ab88-a353d5133a01))
  (pad "A3" smd roundrect (at 1.75 0.8) (size 0.25 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp f270015a-1cd7-41cd-89a4-85ba32d0ff61))
  (pad "A4" smd roundrect (at 1.25 0.8) (size 0.4 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp aecef12e-6fc1-4484-9c81-d5abcfaf9502))
  (pad "A5" smd roundrect (at 0.75 0.8) (size 0.25 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 0fd38af3-3b80-49b9-9c67-3e4145deb11f))
  (pad "A6" smd roundrect (at 0.25 0.8) (size 0.25 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp fe79dd2a-24e3-478c-b576-231dd3030314))
  (pad "A7" smd roundrect (at -0.25 0.8) (size 0.25 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp f9c40c1e-5a21-4c23-a86f-6d0c52038d25))
  (pad "A8" smd roundrect (at -0.75 0.8) (size 0.25 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp bdb3070f-70d6-4318-a412-7ca294f415ed))
  (pad "A9" smd roundrect (at -1.25 0.8) (size 0.4 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 60e757c4-629d-4cb0-a0f3-c3f5128cc1e5))
  (pad "A10" smd roundrect (at -1.75 0.8) (size 0.25 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp cee64b6d-bbbf-40d7-8d21-3e882c93aceb))
  (pad "A11" smd roundrect (at -2.25 0.9) (size 0.25 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp fc6f211c-8f46-4257-9cf1-a36053166db2))
  (pad "A12" smd roundrect (at -2.75 0.9) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 71e627b7-e25e-42cc-afd8-f26dd1c9ae7b))
  (pad "B1" smd roundrect (at -2.75 0.9 180) (size 0.4 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.125) (tstamp dc4ca915-49f5-4489-9f57-f397804632ab))
  (pad "B2" smd roundrect (at -2.25 0.9 180) (size 0.25 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2) (tstamp cd20c37d-f459-48f3-a3a1-3163157de549))
  (pad "B3" smd roundrect (at -1.75 0.8 180) (size 0.25 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2) (tstamp b218345b-0ea7-42b8-b4db-1ff5e8cb3e25))
  (pad "B4" smd roundrect (at -1.25 0.8 180) (size 0.4 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.125) (tstamp ddddcce1-ac36-4749-9505-efa0552b8215))
  (pad "B5" smd roundrect (at -0.75 0.8 180) (size 0.25 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2) (tstamp 516822a0-ce16-48e6-a581-722903c8d5d4))
  (pad "B6" smd roundrect (at -0.25 0.8 180) (size 0.25 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2) (tstamp 4a9f47b8-c73d-4876-825f-24a784adc5e1))
  (pad "B7" smd roundrect (at 0.25 0.8 180) (size 0.25 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2) (tstamp 6e5936cf-1d0a-42f4-9d3b-70d46afd2974))
  (pad "B8" smd roundrect (at 0.75 0.8 180) (size 0.25 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2) (tstamp 0bbac1be-7355-409e-8832-d120c5f9517d))
  (pad "B9" smd roundrect (at 1.25 0.8 180) (size 0.4 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.125) (tstamp 01ab741e-bd1c-404a-9bc2-699f1531d456))
  (pad "B10" smd roundrect (at 1.75 0.8 180) (size 0.25 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2) (tstamp 505993f7-23f5-4386-8903-9fa34f29fc32))
  (pad "B11" smd roundrect (at 2.25 0.9 180) (size 0.25 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2) (tstamp c071b97e-00d7-43ac-b153-c520e31711e2))
  (pad "B12" smd roundrect (at 2.75 0.9 180) (size 0.4 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.125) (tstamp b5fa0c3c-1cfb-4bad-8d34-3752271b6684))
  (pad "S1" smd roundrect (at 4.22 0.9 180) (size 0.8 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.062) (tstamp 1f6e7ced-89b0-4c42-acfe-e23391c95f31))
  (pad "S1" smd roundrect (at -3.92 0.9 180) (size 1.4 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.036) (tstamp 61f114a8-87b3-42a3-872e-8de7e7e42acf))
  (pad "S1" smd roundrect (at 3.92 0.9) (size 1.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.036) (tstamp 6cca887c-6b73-4bbb-9558-92f755425d34))
  (pad "S1" smd roundrect (at -4.22 0.9) (size 0.8 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp c1dffd14-1eeb-45f8-88ee-224adef73b27))
  (model "${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_XKB_U263-24XN-4BQC14.step"
    (offset (xyz 0 2.875 -0.4))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 0 0))
  )
)
