(module Pin_Header_Straight_1x03_2mm (layer F.Cu) (tedit 5819ABB4)
  (solder_mask_margin -0.02)
  (fp_text reference JP2 (at -3.5 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value BOOT_MODE (at 0 -1.7) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_circle (center -2.9 0.9) (end -2.9 1) (layer B.SilkS) (width 0.125))
  (fp_circle (center -2.9 1.3) (end -2.9 1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -1 -1) (end -1 1) (layer F.SilkS) (width 0.125))
  (fp_line (start -3 1) (end -3 -1) (layer F.SilkS) (width 0.125))
  (fp_line (start 3 1) (end -3 1) (layer F.SilkS) (width 0.125))
  (fp_line (start 3 -1) (end 3 1) (layer F.SilkS) (width 0.125))
  (fp_line (start -3 -1) (end 3 -1) (layer F.SilkS) (width 0.125))
  (pad 3 connect roundrect (at 2.000001 0) (size 1.4 1.7) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 2 connect roundrect (at 0 0) (size 1.4 1.7) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 1 connect roundrect (at -2.000001 0) (size 1.4 1.7) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 3 thru_hole circle (at 2.000001 0) (size 1.25 1.25) (drill 0.75) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 0) (size 1.25 1.25) (drill 0.75) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.000001 0) (size 1.25 1.25) (drill 0.75) (layers *.Cu *.Mask))
  (model Pin_Header_Straight_1x03_2mm.step
    (at (xyz -0.07874015748031496 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
