(module Coilcraft_XAL40xx (layer F.Cu) (tedit 5BDDB405)
  (solder_mask_margin 0.025)
  (solder_paste_margin -0.001)
  (attr smd)
  (fp_text reference L2 (at -2.75 -0.5 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value 2.2uH (at 0 1.75) (layer F.Fab)
    (effects (font (size 0.3 0.3) (thickness 0.075)))
  )
  (fp_circle (center -2.4 -2.15) (end -2.4 -2.2) (layer F.SilkS) (width 0.125))
  (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -2.25 2.25) (end 2.25 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.25 2.25) (end 2.25 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.25 -2.25) (end -2.25 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.25 -2.25) (end -2.25 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.6 2.2) (end -2.2 2.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -2.2 2.2) (end -2.2 1.6) (layer F.SilkS) (width 0.125))
  (fp_line (start 2.2 1.6) (end 2.2 2.2) (layer F.SilkS) (width 0.125))
  (fp_line (start 2.2 2.2) (end 1.6 2.2) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.6 -2.2) (end 2.2 -2.2) (layer F.SilkS) (width 0.125))
  (fp_line (start 2.2 -2.2) (end 2.2 -1.6) (layer F.SilkS) (width 0.125))
  (fp_line (start -2.2 -2.2) (end -1.6 -2.2) (layer F.SilkS) (width 0.125))
  (fp_line (start -2.2 -2.2) (end -2.2 -1.6) (layer F.SilkS) (width 0.125))
  (fp_line (start 2 -2) (end 2 2) (layer F.Fab) (width 0.05))
  (fp_line (start 2 2) (end -2 2) (layer F.Fab) (width 0.05))
  (fp_line (start -2 2) (end -2 -2) (layer F.Fab) (width 0.05))
  (fp_line (start -2 -2) (end 2 -2) (layer F.Fab) (width 0.05))
  (pad 2 smd roundrect (at 1.185 1.3) (size 1 1) (layers F.Paste) (roundrect_rratio 0.3))
  (pad 2 smd roundrect (at 1.185 0) (size 1 1) (layers F.Paste) (roundrect_rratio 0.3))
  (pad 2 smd roundrect (at 1.185 -1.3) (size 1 1) (layers F.Paste) (roundrect_rratio 0.3))
  (pad 1 smd roundrect (at -1.185 1.3) (size 1 1) (layers F.Paste) (roundrect_rratio 0.3))
  (pad 1 smd roundrect (at -1.185 0) (size 1 1) (layers F.Paste) (roundrect_rratio 0.3))
  (pad 1 smd roundrect (at -1.185 -1.3) (size 1 1) (layers F.Paste) (roundrect_rratio 0.3))
  (pad 1 smd roundrect (at -1.185 0) (size 1 3.7) (layers F.Cu F.Mask) (roundrect_rratio 0.05)
    (zone_connect 2))
  (pad 2 smd roundrect (at 1.185 0) (size 1 3.7) (layers F.Cu F.Mask) (roundrect_rratio 0.05)
    (zone_connect 2))
  (model ${KICAD7_3DMODEL_DIR}/Inductor_SMD.3dshapes/Coilcraft_XEL4020.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
