(footprint "USB_C_Receptacle_XKB_U262-061N-4BVC11" (version 20211232) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61F97F5D)
  (tags "USB C Type-C Receptacle SMD")
  (property "MFG" "XKB")
  (property "MPN" "U262-16XN-4BVC11")
  (property "Sheetfile" "Dumbbell_Base_Board.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (fp_text reference "J1" (at 0 -5.715) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2189cff3-d37e-4f27-a1b2-a93764dc3afa)
  )
  (fp_text value "USB_C_Receptacle_USB-PD" (at 0 4.935) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e4243ddd-cefe-4c5f-9160-c242ab745460)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 36107421-a1c7-4f89-92f6-79c699dd154a)
  )
  (fp_line (start -4.58 -1.85) (end -4.58 0.07)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2888517d-b5b4-414b-8c54-833fc144ea56))
  (fp_line (start -4.58 3.785) (end -4.58 2.08)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 276f4b63-644f-40d7-a3c9-ae5923c863e5))
  (fp_line (start 4.58 0.07) (end 4.58 -1.85)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e3b1339b-b5c5-4e0f-a235-a02456b4d67d))
  (fp_line (start 4.58 2.08) (end 4.58 3.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8884e70f-e5f7-4a8a-b350-6a911e985324))
  (fp_line (start 4.58 3.785) (end -4.58 3.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 29210db5-1fe4-44ab-a61f-703001336dce))
  (fp_line (start -5.32 -4.75) (end 5.32 -4.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 88dd35a7-30cf-41da-8383-8e06001dbe7a))
  (fp_line (start -5.32 4.18) (end -5.32 -4.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f8b1afbe-8635-4ac4-b9d4-c1a6f56d69b3))
  (fp_line (start 5.32 -4.75) (end 5.32 4.18)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4fa84034-c81b-498b-865f-f32da495001e))
  (fp_line (start 5.32 4.18) (end -5.32 4.18)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3067c460-8965-44b2-9272-1824c5bee577))
  (fp_line (start -4.47 -3.675) (end -4.47 3.675)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 18b03b6c-3eb5-4931-9e00-90a86c749f22))
  (fp_line (start -4.47 -3.675) (end 4.47 -3.675)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f3d7f2e-abff-4c83-a34e-3e3d809d8c05))
  (fp_line (start -4.47 3.675) (end 4.47 3.675)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 26dcfef9-c372-435f-b01d-b0e802c38888))
  (fp_line (start 4.47 3.675) (end 4.47 -3.675)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 64a4f6e0-4cbd-4fd5-ac9c-8047ed491dd7))
  (pad "A5" smd roundrect (at 0.48 -3.635) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
    (thermal_bridge_angle 45) (tstamp ed6f15be-23bd-4184-9a19-cf02a4499c42))
  (pad "A9" smd roundrect (at 1.48 -3.635) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
    (thermal_bridge_angle 45) (tstamp 378e6384-d8ff-4452-8510-ce38f037afe1))
  (pad "A12" smd roundrect (at 2.75 -3.635) (size 1 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
    (thermal_bridge_angle 45) (tstamp 6ee745e2-e4f6-4849-b0a5-0c7af2b51aca))
  (pad "B5" smd roundrect (at -0.52 -3.635) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
    (thermal_bridge_angle 45) (tstamp 0e4999d6-cd08-4c7d-a83a-c1249a260a9c))
  (pad "B9" smd roundrect (at -1.52 -3.635) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
    (thermal_bridge_angle 45) (tstamp 9104ff40-9a3c-4c5b-8edd-5d4af42e6e1b))
  (pad "B12" smd roundrect (at -2.75 -3.635) (size 1 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
    (thermal_bridge_angle 45) (tstamp f647814e-fc6f-45f3-a93d-2806406fdfd7))
  (pad "S1" thru_hole oval (at -4.32 -3.105) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask) (tstamp e634cc7d-54a3-42f4-953a-2b921807b7de))
  (pad "S1" thru_hole oval (at -4.32 1.075) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask) (tstamp 156e71bd-e626-4b6a-a91c-a31140e4e15a))
  (pad "S1" thru_hole oval (at 4.32 -3.105) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask) (tstamp 34444577-33cc-4992-9da1-a8585df323e6))
  (pad "S1" thru_hole oval (at 4.32 1.075) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask) (tstamp 3c5ef32c-4145-420d-b2b9-fae73bd49f01))
  (model "${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/XKB_U262-16XN-4BVC11.stp"
    (offset (xyz 0 -3.67 1.67))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
