(module CP_Elec_6.3x7.7 (layer F.Cu) (tedit 5930FBDF)
  (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
  (solder_mask_margin -0.05)
  (solder_paste_margin -0.05)
  (attr smd)
  (fp_text reference REF** (at -3.8 -2.3 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value CP_Elec_6.3x7.7 (at -0.05 -3.7) (layer F.Fab)
    (effects (font (size 0.3 0.3) (thickness 0.075)))
  )
  (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.125))
  (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.125))
  (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.125))
  (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.125))
  (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.125))
  (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.125))
  (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.125))
  (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.125))
  (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.05))
  (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.05))
  (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.05))
  (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.05))
  (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.05))
  (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.05))
  (fp_text user + (at -3.75 1.15) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user + (at -1.73 -0.08) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 0 3.15) (layer F.Fab) (width 0.05))
  (pad 2 smd roundrect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
)
