(module Socket_Straight_2x05_2mm_Mirrored (layer F.Cu) (tedit 584EFD35)
  (descr "Through hole pin header, 2x05, 2.00mm pitch, double row")
  (tags "pin header double row")
  (fp_text reference P1 (at 0 -5.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value uPSU_header (at -2.75 0 90) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -2 -5) (end 2 -5) (layer F.SilkS) (width 0.125))
  (fp_line (start 2 -5) (end 2 -3) (layer F.SilkS) (width 0.125))
  (fp_line (start 2 -3) (end 2 5) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 5) (end -2 5) (layer F.SilkS) (width 0.125))
  (fp_line (start -2 5) (end -2 -5) (layer F.SilkS) (width 0.125))
  (fp_line (start -2.6 -5.6) (end 2.6 -5.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.6 -5.6) (end 2.6 5.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.6 5.6) (end -2.6 5.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.6 5.6) (end -2.6 -5.6) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole rect (at 1 -4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 1 -2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 1 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 1 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 1 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -1 -4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -1 -2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -1 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at -1 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at -1 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
  (model Pin_header_socket_2x5_2mm.step
    (at (xyz 0.03937007874015748 -0.1574803149606299 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
