(module 2x10_1.5mm (layer F.Cu) (tedit 575366A3)
  (solder_mask_margin -0.02)
  (attr virtual)
  (fp_text reference REF** (at 0 -8) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value 2x10_1.5mm (at 2 0 90) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -1.75 -7.75) (end 1.75 -7.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 -7.75) (end 1.75 7.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 7.75) (end -1.75 7.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 7.75) (end -1.75 -7.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 -7.5) (end 1.5 -7.5) (layer F.Fab) (width 0.05))
  (fp_line (start 1.5 -7.5) (end 1.5 7.5) (layer F.Fab) (width 0.05))
  (fp_line (start 1.5 7.5) (end -1.5 7.5) (layer F.Fab) (width 0.05))
  (fp_line (start -1.5 7.5) (end -1.5 -7.5) (layer F.Fab) (width 0.05))
  (fp_text user 1 (at -1.75 -6.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (pad 1 connect roundrect (at -0.75 -6.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 2 connect roundrect (at 0.75 -6.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 3 connect roundrect (at -0.75 -5.25) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 4 connect roundrect (at 0.75 -5.25) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 5 connect roundrect (at -0.75 -3.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 6 connect roundrect (at 0.75 -3.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 7 connect roundrect (at -0.75 -2.25) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 8 connect roundrect (at 0.75 -2.25) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 9 connect roundrect (at -0.75 -0.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 10 connect roundrect (at 0.75 -0.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 11 connect roundrect (at -0.75 0.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 12 connect roundrect (at 0.75 0.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 13 connect roundrect (at -0.75 2.25) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 14 connect roundrect (at 0.75 2.25) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 15 connect roundrect (at -0.75 3.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 16 connect roundrect (at 0.75 3.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 17 connect roundrect (at -0.75 5.25) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 18 connect roundrect (at 0.75 5.25) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 19 connect roundrect (at -0.75 6.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
  (pad 20 connect roundrect (at 0.75 6.75) (size 1.05 1.05) (layers F.Cu F.Mask)(roundrect_rratio 0.33))
)
