(footprint "2520_C" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "LCSC" "C98034")
  (property "MFG" "Murata")
  (property "MPN" "LQM2HPN1R5MG0L")
  (property "Sheetfile" "NightLight.kicad_sch")
  (property "Sheetname" "")
  (solder_mask_margin 0.025)
  (solder_paste_margin -0.001)
  (attr smd)
  (fp_text reference "L2" (at 1.5 0 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify left))
    (tstamp fd2005fc-c181-41e6-829e-6274aa2ca71b)
  )
  (fp_text value "1.5uH" (at 0 -0.55 -180) (layer "Cmts.User")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp 4d0eb2b2-8d0c-42c6-942c-ecda1615e645)
  )
  (fp_rect (start -0.55 -1.025) (end 0.55 -1.175)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 66229c2c-b19b-4df4-b99c-fc90e6d720f7))
  (fp_rect (start -0.55 1.175) (end 0.55 1.025)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp ee701515-3ff7-4218-8d51-0a833f34eff9))
  (fp_line (start -1.55 1) (end -1.55 -1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3f930c14-880f-4880-97ca-44da8e9cfc22))
  (fp_line (start -1.3 -1.25) (end 1.3 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ee739e43-8438-4bf4-9ca5-2dc48b008b0d))
  (fp_line (start 1.3 1.25) (end -1.3 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9ba9ea91-01e8-4ac8-9110-16b15e7fa97b))
  (fp_line (start 1.55 -1) (end 1.55 1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 52968344-896d-4b69-8ea4-a356220d9094))
  (fp_arc (start -1.55 -1) (mid -1.476777 -1.176777) (end -1.3 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f0d8a6e8-2156-4659-84de-af751e57cc68))
  (fp_arc (start -1.3 1.25) (mid -1.476777 1.176777) (end -1.55 1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5e8e45dd-2b07-4d07-8f3f-2c2bba5c03b7))
  (fp_arc (start 1.3 -1.25) (mid 1.476777 -1.176777) (end 1.55 -1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3d901af7-4ac1-4738-8845-9672eda6def8))
  (fp_arc (start 1.55 1) (mid 1.476777 1.176777) (end 1.3 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1a584ba4-70d8-48dd-9993-4a9e64c193d8))
  (fp_line (start -1.25 -1) (end 1.25 -1)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 9dddd77e-3a63-4997-965b-a951e80d1ca8))
  (fp_line (start -1.25 1) (end -1.25 -1)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 58833a1e-4fa7-41b2-a9e4-a2a670e77f4a))
  (fp_line (start 1.25 -1) (end 1.25 1)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp f37b01d3-22de-42bf-b358-28f9d4370349))
  (fp_line (start 1.25 1) (end -1.25 1)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 19d4499b-ea5a-4a5a-a194-972f91cb936a))
  (pad "" smd oval (at -1.025 0) (size 0.75 1.8) (layers "F.Paste") (tstamp 05a7d327-b2e1-45b8-ae42-da7e1070b548))
  (pad "" smd oval (at 1.025 0) (size 0.75 1.8) (layers "F.Paste") (tstamp 0f798a42-8c4f-4a46-83bc-fe2312eb8c1e))
  (pad "1" smd roundrect (at -1.025 0) (size 0.75 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.05)
    (zone_connect 2) (tstamp c183be40-f005-406e-a71e-20697ac2eba9))
  (pad "2" smd roundrect (at 1.025 0) (size 0.75 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.05)
    (zone_connect 2) (tstamp 58ba3b50-7163-4068-bbb9-6da5333af7ed))
  (model "${KICAD7_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
