(footprint "SOT-23-5" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "SOT TO_SOT_SMD")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "250-mA Ultra-Low-Noise Low-IQ LDO, 3.3V, SOT-23")
  (property "ki_keywords" "Single Output LDO Low-Noise")
  (attr smd)
  (fp_text reference "U37" (at 0 -2.25) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 51ef0db3-853c-4c0a-bf19-faa445b27303)
  )
  (fp_text value "LP5907MFX-3.3" (at -0.3 0 -90) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold))
    (tstamp c57f708c-156b-4b21-8f1b-11e28040ce62)
  )
  (fp_text user "${REFERENCE}" (at 0.35 -0.025 90) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold))
    (tstamp 0e44d9c6-2c37-4fc7-9f1d-494a50118346)
  )
  (fp_rect (start -1.55 -1.65) (end 0.8 -1.5)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp cd5cdece-41d8-4b2e-ac7f-6a0682ceec52))
  (fp_rect (start -0.8 1.5) (end 0.8 1.65)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp ed178b96-e3a6-4e4a-b532-69ff5482d642))
  (fp_line (start -1.95 -1.05) (end -1.95 1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d5cf837e-32fb-4757-ae95-d8fadb078955))
  (fp_line (start -1.6 -1.4) (end -1.05 -1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 41d00bd4-172f-4400-90e2-42b27d0aafe6))
  (fp_line (start -1.6 1.4) (end -1.05 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 353582ff-d7e5-4398-8570-597f775c3a45))
  (fp_line (start -1.05 -1.4) (end -1.05 -1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 26566fa9-ee31-4dda-a1ba-703a4dc3e525))
  (fp_line (start -1.05 1.4) (end -1.05 1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4977c737-f372-4e78-82a0-0b43e7413e7c))
  (fp_line (start 0.8 -1.7) (end -0.8 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 689d14f7-8ef6-4b3f-8817-5a27c08711e8))
  (fp_line (start 0.8 1.7) (end -0.8 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fd301e63-0bf0-4e97-8648-c81ee496dbb2))
  (fp_line (start 1.05 -1.4) (end 1.05 -1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 93cf3717-9f11-48f9-a6d1-6863838b57d3))
  (fp_line (start 1.05 -0.5) (end 1.05 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4521c239-01b9-4406-9082-6aec63653a17))
  (fp_line (start 1.05 0.5) (end 1.6 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e9f36a34-d435-4bf3-b567-68deaee7b0ce))
  (fp_line (start 1.05 1.4) (end 1.05 1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 983ca5b9-ed85-41a0-8fbf-3a3489ad3916))
  (fp_line (start 1.6 -1.4) (end 1.05 -1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 38cd7924-dcff-4b27-975e-e45ec080c271))
  (fp_line (start 1.6 -0.5) (end 1.05 -0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ed90571f-3954-402a-b458-7dcb635af9d5))
  (fp_line (start 1.6 1.4) (end 1.05 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8621b178-1d2a-41fa-b916-259d83b04d1b))
  (fp_line (start 1.95 -1.05) (end 1.95 -0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 917661c1-0f23-43af-ab60-16d27edc2df4))
  (fp_line (start 1.95 0.85) (end 1.95 1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 61efe08f-59ce-4ca1-a938-2e5c001c1173))
  (fp_arc (start -1.95 -1.05) (mid -1.847487 -1.297487) (end -1.6 -1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1b4c9206-2328-4eff-ac2c-979e4bf452b1))
  (fp_arc (start -1.6 1.4) (mid -1.847487 1.297487) (end -1.95 1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 44e76443-dab8-4a61-8968-9a8c56bd7fb9))
  (fp_arc (start -1.05 -1.45) (mid -0.976777 -1.626777) (end -0.8 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ca83bf1c-08dd-444e-bfb2-cb080a1e054d))
  (fp_arc (start -0.8 1.7) (mid -0.976777 1.626777) (end -1.05 1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5edc6f0b-e23c-4c83-bfd7-13bdd38b0be7))
  (fp_arc (start 0.8 -1.7) (mid 0.976777 -1.626777) (end 1.05 -1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4765582c-8c82-4a4f-8054-85efd959c4b6))
  (fp_arc (start 1.05 1.45) (mid 0.976777 1.626777) (end 0.8 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 69dc093f-8828-4557-bb22-715693d87f8f))
  (fp_arc (start 1.6 -1.4) (mid 1.847487 -1.297487) (end 1.95 -1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 77e48d03-fa6a-4016-a218-169f2888a701))
  (fp_arc (start 1.6 0.5) (mid 1.847487 0.602513) (end 1.95 0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5e34c193-4315-4dd0-8047-c226383bb612))
  (fp_arc (start 1.95 -0.85) (mid 1.847487 -0.602513) (end 1.6 -0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2e809ed6-a230-4316-b956-5646ff677fe3))
  (fp_arc (start 1.95 1.05) (mid 1.847487 1.297487) (end 1.6 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 859c2692-851e-4c8b-a272-b6d43ce1ae56))
  (fp_line (start -0.8 -1.05) (end -0.4 -1.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b6b7833-3733-40ed-84fb-d0c5cef2beea))
  (fp_line (start -0.8 1.45) (end -0.8 -1.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4ae160b7-d1e4-41db-bd08-489cb9e015a6))
  (fp_line (start -0.4 -1.45) (end 0.8 -1.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c32c0b69-8e2f-43ae-bff1-1e9d92545e4a))
  (fp_line (start 0.8 -1.45) (end 0.8 1.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp afebf466-0130-444a-967c-c6947d4a2c50))
  (fp_line (start 0.8 1.45) (end -0.8 1.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 301654ff-afa5-4f63-8060-630c62c9f03f))
  (pad "" smd oval (at -1.135 -0.95) (size 1.1 0.5) (layers "F.Paste") (tstamp 2fe3e456-20f9-4013-adad-9878eb28627b))
  (pad "" smd oval (at -1.135 0) (size 1.1 0.5) (layers "F.Paste") (tstamp e241574a-2bb9-4400-ad02-2c9a6cf1e583))
  (pad "" smd oval (at -1.135 0.95) (size 1.1 0.5) (layers "F.Paste") (tstamp 81b8e44f-e11c-4ecf-bf15-853c8d7ca9ff))
  (pad "" smd oval (at 1.135 -0.95) (size 1.1 0.5) (layers "F.Paste") (tstamp cab95a2a-67f7-4646-80c0-3f0fd6b16ddb))
  (pad "" smd oval (at 1.135 0.95) (size 1.1 0.5) (layers "F.Paste") (tstamp 8e52526a-2d87-430a-b91e-677b5e0e83e1))
  (pad "1" smd roundrect (at -1.135 -0.95) (size 1.3 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 27514b3b-f600-417b-abf4-261ad505171b))
  (pad "2" smd roundrect (at -1.1375 0) (size 1.3 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp af929d6a-ac0a-4c1a-b741-937c3901bd38))
  (pad "3" smd roundrect (at -1.1375 0.95) (size 1.3 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 15bf574f-1607-43c1-bce8-5e81f0a4def7))
  (pad "4" smd roundrect (at 1.1375 0.95 180) (size 1.3 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp 4ddda866-8331-4306-83e6-3f6edadbdec5))
  (pad "5" smd roundrect (at 1.1375 -0.95 180) (size 1.3 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer top_right bottom_right) (tstamp d8f1b012-9087-4481-9223-f70460ee4131))
  (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
