(footprint "1P_6x3.4"
	(version 20231231)
	(generator "pcbnew")
	(generator_version "7.99")
	(layer "F.Cu")
	(property "Reference" "J4"
		(at 9 -1.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "389ae9e5-66a3-435f-936d-4104bc76da2a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "PHASE A"
		(at 9 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "2c026d93-1236-42c3-a957-8f500294988d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "SH_Solder_Pads:1P_6x3.4"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fb976a95-9399-480f-a2b1-66b163b4311a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "10440c76-d1e6-418d-bf56-2864f65c9721")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4e5c4a80-4532-477e-8210-c1b3109afa28")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Preferred" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "96df270d-d321-4dd4-a619-40db5c20b28c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 9 1.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "6204a5c9-521a-47bb-8e39-f8a82ca281ba")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at 0 0)
		(size 6 3.4)
		(layers "F.Cu" "F.Mask")
		(uuid "b1bec019-eb39-46a6-9d90-678a1ab5dadb")
	)
)