(footprint "JST_XH_B4B-XH-AM_1x04_P2.50mm_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "JST XH series connector, B4B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST XH vertical boss")
  (property "LCSC" "C144395")
  (property "MFG" "JST")
  (property "MPN" "B4B-XH-A(LF)(SN)")
  (property "Sheetfile" "tmc2209_driver.kicad_sch")
  (property "Sheetname" "TMC2209_Driver")
  (attr through_hole)
  (fp_text reference "M5" (at 0 -3.55 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bb6fbfae-a858-41c4-9ca7-dd473983f393)
  )
  (fp_text value "Bipolar_Stepper_Motor" (at 0 4.25 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2514d787-673a-4e67-8f86-d3a29b82f7b7)
  )
  (fp_text user "${REFERENCE}" (at 0 2.7 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a852a8f1-24c1-4810-ab97-3d4f1055b500)
  )
  (fp_line (start -6.31 -2.46) (end -6.31 3.51)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fe30ff3e-257f-42c4-a923-c1117e50faf1))
  (fp_line (start -6.31 3.51) (end 6.31 3.51)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ac5d8bdb-eb7e-4816-ad31-320f9d4bcfcb))
  (fp_line (start -6.3 -2.45) (end -6.3 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f9ccdfac-d01c-45f5-a90a-f4f035061d53))
  (fp_line (start -6.3 -1.7) (end -4.5 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 18e8880e-e978-41f9-b3fd-3a212ea07f07))
  (fp_line (start -6.3 -0.2) (end -5.55 -0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c2a93c5-247a-43f3-af39-0ea54714e1b3))
  (fp_line (start -5.55 -0.2) (end -5.55 1.14)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2febfd97-11db-41a7-bc7d-55edb59bf574))
  (fp_line (start -4.5 -2.45) (end -6.3 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b3380468-5763-47f8-93de-b950446563eb))
  (fp_line (start -4.5 -1.7) (end -4.5 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2630169a-4a9a-4a5e-a906-48f0a3307d5a))
  (fp_line (start -3 -2.45) (end -3 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 067caac6-1971-4771-a748-68fc483e2a8f))
  (fp_line (start -3 -1.7) (end 3 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1905aa64-017f-45e4-a482-17b4d0258155))
  (fp_line (start 0 2.75) (end -4.49 2.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f456aca3-1202-439d-814c-11764e538dbb))
  (fp_line (start 3 -2.45) (end -3 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b34b0f87-a135-47d6-8f44-5fd4d48d79d9))
  (fp_line (start 3 -1.7) (end 3 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0199e3a7-9bf4-45a2-a2d5-5d3bdcceeba7))
  (fp_line (start 4.5 -2.45) (end 4.5 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f1d1e20a-4417-4111-b06c-630d1fba7bff))
  (fp_line (start 4.5 -1.7) (end 6.3 -1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a883bbdb-bdbb-4365-8b83-387d34eceaf1))
  (fp_line (start 5.55 -0.2) (end 5.55 2.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c8e1dd1e-27ae-4e9a-8d9e-cdfd3e1e60e9))
  (fp_line (start 5.55 2.75) (end 0 2.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 011c73bf-82ff-454d-8db0-6a6be97a442f))
  (fp_line (start 6.3 -2.45) (end 4.5 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da5b459f-3149-4022-971e-c1fee438309f))
  (fp_line (start 6.3 -1.7) (end 6.3 -2.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3c24a563-1ea6-4035-a8c8-edf368c1a731))
  (fp_line (start 6.3 -0.2) (end 5.55 -0.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0ec464ed-9eda-4959-91fe-968e2a0b42db))
  (fp_line (start 6.31 -2.46) (end -6.31 -2.46)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 260b0663-d359-48e7-85ab-aa0aa7f5413b))
  (fp_line (start 6.31 3.51) (end 6.31 -2.46)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9747a84f-f38b-4d5b-a7ac-d8b5169a7240))
  (fp_line (start -6.7 -2.35) (end -6.7 3.4)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a36c75a3-6ce9-4f7f-9c45-926bacc4fede))
  (fp_line (start -6.2 3.9) (end 6.2 3.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 81899cff-2b46-4f84-b1b6-8e9b1929e3e6))
  (fp_line (start 6.2 -2.85) (end -6.2 -2.85)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e7d1534c-b5ef-4426-9543-a2afc1f84bda))
  (fp_line (start 6.7 3.4) (end 6.7 -2.35)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ab0d3e3a-313f-497b-b098-d5309318c0be))
  (fp_arc (start -6.7 -2.35) (mid -6.553553 -2.703553) (end -6.2 -2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2ea938a9-58e2-4efa-b6b1-2f1694eab905))
  (fp_arc (start -6.2 3.9) (mid -6.553553 3.753553) (end -6.7 3.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ca055bc2-fd21-445b-a2f8-f6ca551ad6ab))
  (fp_arc (start 6.2 -2.85) (mid 6.553553 -2.703553) (end 6.7 -2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1db8a057-fc3d-4137-b262-e9cc655e6ac3))
  (fp_arc (start 6.7 3.4) (mid 6.553553 3.753553) (end 6.2 3.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ee11b490-2852-49bc-bb94-e4f27abd90c2))
  (fp_line (start -6.2 -2.35) (end -6.2 3.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1d81547f-b82c-4270-b985-67c2b94847e0))
  (fp_line (start -6.2 3.4) (end 6.2 3.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 38446a95-1a3e-43fe-a06a-4aebe47d925b))
  (fp_line (start -4.375 -2.35) (end -3.75 -1.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f92376b0-c1c9-43be-bbbc-2b42b611b0ea))
  (fp_line (start -3.75 -1.35) (end -3.125 -2.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c570f9b5-f01d-4044-bdd6-b0e318e91f39))
  (fp_line (start 6.2 -2.35) (end -6.2 -2.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b907a126-103c-4a1f-a807-0c8f92ecbe5b))
  (fp_line (start 6.2 3.4) (end 6.2 -2.35)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a8205722-6782-4e52-9e7c-87348d247cb6))
  (pad "" np_thru_hole circle (at -5.35 2) (size 1.2 1.2) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp f099dd33-d852-4a2c-92bb-98c18a186b65))
  (pad "1" thru_hole roundrect (at -3.75 0) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.147059) (tstamp 318c0879-cbb8-4ef0-87b5-33276e7bd5c4))
  (pad "2" thru_hole oval (at -1.25 0) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (tstamp 4b4b2b72-2d34-4653-9528-a70687b768be))
  (pad "3" thru_hole oval (at 1.25 0) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (tstamp ad138f7c-b9c6-4c1b-9d91-f64d98862694))
  (pad "4" thru_hole oval (at 3.75 0) (size 1.7 1.95) (drill 0.95) (layers "*.Cu" "*.Mask") (tstamp 84e4290c-b815-4ded-b794-d93b91367d8b))
  (model ":KICAD7_3DMODEL_DIR:Connector_JST.3dshapes/B4B-XH-A.STEP"
    (offset (xyz 0 -0.5 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 180))
  )
)
