(module QFN-48-1EP_6x6mm_P0.4mm_EP4.3x4.3mm (layer F.Cu) (tedit 5BA942A7)
  (descr "QFN, 48 Pin (https://www.espressif.com/sites/default/files/documentation/esp32_datasheet_en.pdf (page 38)), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
  (tags "QFN DFN_QFN")
  (attr smd)
  (fp_text reference U7 (at 0.774999 -4.625001) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value X-Powers_AXP203 (at 0 4.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.56 -3.11) (end 3.11 -3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.11 -3.11) (end 3.11 -2.56) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.56 3.11) (end -3.11 3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.11 3.11) (end -3.11 2.56) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.56 3.11) (end 3.11 3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.11 3.11) (end 3.11 2.56) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.56 -3.11) (end -3.11 -3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 -3) (end 3 -3) (layer F.Fab) (width 0.1))
  (fp_line (start 3 -3) (end 3 3) (layer F.Fab) (width 0.1))
  (fp_line (start 3 3) (end -3 3) (layer F.Fab) (width 0.1))
  (fp_line (start -3 3) (end -3 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -3 -2) (end -2 -3) (layer F.Fab) (width 0.1))
  (fp_line (start -3.6 -3.6) (end -3.6 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.6 3.6) (end 3.6 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.6 3.6) (end 3.6 -3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.6 -3.6) (end -3.6 -3.6) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 49 smd roundrect (at 0 0) (size 4.3 4.3) (layers F.Cu F.Mask) (roundrect_rratio 0.05814))
  (pad "" smd roundrect (at -1.43 -1.43) (size 1.16 1.16) (layers F.Paste) (roundrect_rratio 0.215517))
  (pad "" smd roundrect (at -1.43 0) (size 1.16 1.16) (layers F.Paste) (roundrect_rratio 0.215517))
  (pad "" smd roundrect (at -1.43 1.43) (size 1.16 1.16) (layers F.Paste) (roundrect_rratio 0.215517))
  (pad "" smd roundrect (at 0 -1.43) (size 1.16 1.16) (layers F.Paste) (roundrect_rratio 0.215517))
  (pad "" smd roundrect (at 0 0) (size 1.16 1.16) (layers F.Paste) (roundrect_rratio 0.215517))
  (pad "" smd roundrect (at 0 1.43) (size 1.16 1.16) (layers F.Paste) (roundrect_rratio 0.215517))
  (pad "" smd roundrect (at 1.43 -1.43) (size 1.16 1.16) (layers F.Paste) (roundrect_rratio 0.215517))
  (pad "" smd roundrect (at 1.43 0) (size 1.16 1.16) (layers F.Paste) (roundrect_rratio 0.215517))
  (pad "" smd roundrect (at 1.43 1.43) (size 1.16 1.16) (layers F.Paste) (roundrect_rratio 0.215517))
  (pad 1 smd roundrect (at -2.95 -2.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -2.95 -1.8) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -2.95 -1.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -2.95 -1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at -2.95 -0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at -2.95 -0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at -2.95 0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at -2.95 0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at -2.95 1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at -2.95 1.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at -2.95 1.8) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at -2.95 2.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at -2.2 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at -1.8 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 15 smd roundrect (at -1.4 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 16 smd roundrect (at -1 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 17 smd roundrect (at -0.6 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 18 smd roundrect (at -0.2 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 19 smd roundrect (at 0.2 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 20 smd roundrect (at 0.6 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 21 smd roundrect (at 1 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 22 smd roundrect (at 1.4 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 23 smd roundrect (at 1.8 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 24 smd roundrect (at 2.2 2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 25 smd roundrect (at 2.95 2.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 26 smd roundrect (at 2.95 1.8) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 27 smd roundrect (at 2.95 1.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 28 smd roundrect (at 2.95 1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 29 smd roundrect (at 2.95 0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 30 smd roundrect (at 2.95 0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 31 smd roundrect (at 2.95 -0.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 32 smd roundrect (at 2.95 -0.6) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 33 smd roundrect (at 2.95 -1) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 34 smd roundrect (at 2.95 -1.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 35 smd roundrect (at 2.95 -1.8) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 36 smd roundrect (at 2.95 -2.2) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 37 smd roundrect (at 2.2 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 38 smd roundrect (at 1.8 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 39 smd roundrect (at 1.4 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 40 smd roundrect (at 1 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 41 smd roundrect (at 0.6 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 42 smd roundrect (at 0.2 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 43 smd roundrect (at -0.2 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 44 smd roundrect (at -0.6 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 45 smd roundrect (at -1 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 46 smd roundrect (at -1.4 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 47 smd roundrect (at -1.8 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 48 smd roundrect (at -2.2 -2.95) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (model ${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-48-1EP_6x6mm_0.4mm.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
