(module "LQFP-48_7x7mm_P0.5mm" (layer F.Cu) (tedit 5D6EAF1A)
  (descr "LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "LQFP QFP")
  (solder_paste_ratio -0.125)
  (attr smd)
  (fp_text reference "U5" (at -0.35 -5.6 180) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_text value "STM32L433CCTx" (at 0 5.85 -180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.16 3.61) (end 3.61 3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.61 3.61) (end 3.61 3.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.16 3.61) (end -3.61 3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.61 3.61) (end -3.61 3.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.16 -3.61) (end 3.61 -3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.61 -3.61) (end 3.61 -3.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.16 -3.61) (end -3.61 -3.61) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.61 -3.61) (end -3.61 -3.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.61 -3.16) (end -4.9 -3.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.5 -3.5) (end 3.5 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 3.5 -3.5) (end 3.5 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 3.5 3.5) (end -3.5 3.5) (layer F.Fab) (width 0.1))
  (fp_line (start -3.5 3.5) (end -3.5 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -3.5 -2.5) (end -2.5 -3.5) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -5.15) (end -3.15 -5.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.15 -5.15) (end -3.15 -3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.15 -3.75) (end -3.75 -3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.75 -3.75) (end -3.75 -3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.75 -3.15) (end -5.15 -3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.15 -3.15) (end -5.15 0) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 -5.15) (end 3.15 -5.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.15 -5.15) (end 3.15 -3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.15 -3.75) (end 3.75 -3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.75 -3.75) (end 3.75 -3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.75 -3.15) (end 5.15 -3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.15 -3.15) (end 5.15 0) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 5.15) (end -3.15 5.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.15 5.15) (end -3.15 3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.15 3.75) (end -3.75 3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.75 3.75) (end -3.75 3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.75 3.15) (end -5.15 3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.15 3.15) (end -5.15 0) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 5.15) (end 3.15 5.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.15 5.15) (end 3.15 3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.15 3.75) (end 3.75 3.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.75 3.75) (end 3.75 3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.75 3.15) (end 5.15 3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.15 3.15) (end 5.15 0) (layer F.CrtYd) (width 0.05))
  (fp_text user "%R" (at 0 0 -180) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (pad "1" smd roundrect (at -4.1625 -2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -4.1625 -2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "3" smd roundrect (at -4.1625 -1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "4" smd roundrect (at -4.1625 -1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "5" smd roundrect (at -4.1625 -0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "6" smd roundrect (at -4.1625 -0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "7" smd roundrect (at -4.1625 0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "8" smd roundrect (at -4.1625 0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "9" smd roundrect (at -4.1625 1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "10" smd roundrect (at -4.1625 1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "11" smd roundrect (at -4.1625 2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "12" smd roundrect (at -4.1625 2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "13" smd roundrect (at -2.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "14" smd roundrect (at -2.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "15" smd roundrect (at -1.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "16" smd roundrect (at -1.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "17" smd roundrect (at -0.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "18" smd roundrect (at -0.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "19" smd roundrect (at 0.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "20" smd roundrect (at 0.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "21" smd roundrect (at 1.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "22" smd roundrect (at 1.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "23" smd roundrect (at 2.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "24" smd roundrect (at 2.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "25" smd roundrect (at 4.1625 2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "26" smd roundrect (at 4.1625 2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "27" smd roundrect (at 4.1625 1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "28" smd roundrect (at 4.1625 1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "29" smd roundrect (at 4.1625 0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "30" smd roundrect (at 4.1625 0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "31" smd roundrect (at 4.1625 -0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "32" smd roundrect (at 4.1625 -0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "33" smd roundrect (at 4.1625 -1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "34" smd roundrect (at 4.1625 -1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "35" smd roundrect (at 4.1625 -2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "36" smd roundrect (at 4.1625 -2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "37" smd roundrect (at 2.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "38" smd roundrect (at 2.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "39" smd roundrect (at 1.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "40" smd roundrect (at 1.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "41" smd roundrect (at 0.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "42" smd roundrect (at 0.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "43" smd roundrect (at -0.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "44" smd roundrect (at -0.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "45" smd roundrect (at -1.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "46" smd roundrect (at -1.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "47" smd roundrect (at -2.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "48" smd roundrect (at -2.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (model "${KICAD7_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
