(footprint "Yageo_ANT3216LL00R2400A"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(locked yes)
	(layer "F.Cu")
	(property "Reference" "AE1"
		(at 6.9 4.65 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "9dc4639b-93bf-4002-a9d6-1d0c3cb82325")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Antenna_Chip"
		(at 0 -9.849999 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "47031ca8-812e-4a37-9e8f-f6ad9d825597")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "RF_Antenna:Yageo_ANT3216LL00R2400A"
		(at 0 -10.85 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f5486731-9631-41b2-a8d4-96de412b6994")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 -10.85 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c2af0882-4fa7-41d6-82fb-21e53b99de6b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "5.05dBi Chip Antenna Linear 160MHz 2.45GHz 1W 1206"
		(at 0 -10.85 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c7017b96-a456-48cd-8065-a6b39b90ee54")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB_PreferredPart" "N"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "68e102f2-f909-45e6-896f-05107b70d2ca")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB_StandardOnly" "N"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "10faa83a-cb3c-4bba-8038-76ba254ea792")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C293767"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a7ad85bf-2d73-4378-a0c7-2537bb1cd083")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "YAGEO"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5fe54273-a5a2-4d73-a34c-b22d078287e5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "ANT3216LL00R2400A"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "31ac3961-a8a3-4474-9ff2-848ea35be1e4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_text user "Adjust width of feed pads 1 & 2 to 50-ohm"
		(at -1.1 -0.950001 90)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "aa93f7d8-bd47-4ab5-bba7-4c38587de5e8")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(fp_text user "board edge"
		(at 0 -6.25 0)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "c479e8e3-4084-4cc4-9d06-5e61c925103c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 -8.35 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7c456512-bb9a-4f58-85e7-ba71ffc2f278")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd oval
		(at 0 -1.55)
		(size 1.7 0.35)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "967088f2-5991-464a-b37a-50d1ba252fed")
	)
	(pad "" smd oval
		(at 0 1.55)
		(size 1.7 0.35)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5de34fb7-aca2-4f92-aa93-7eb999be8d1c")
	)
	(pad "1" smd rect
		(at 0 1.55)
		(size 1.8 0.4)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "536ed7ee-c2e2-49b9-a7a8-c443df2a0a2f")
	)
	(pad "1" smd rect
		(at 0 2.75)
		(size 0.342 2)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1e2ddb4c-058f-4698-b8a4-4e772898b29e")
	)
	(pad "2" smd rect
		(at 0 -3)
		(size 0.342 2.5)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7a424d87-0625-49bc-befa-529afe2b6c9d")
	)
	(pad "2" smd rect
		(at 0 -1.55)
		(size 1.8 0.4)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 0.3)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "90c63dfc-6cca-422c-8c47-6043df95f569")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu")
		(uuid "32be60a9-49c6-4d68-bdab-ff46bc1444c8")
		(hatch edge 0.2)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.9 1.75) (xy 0.9 1.75) (xy 0.9 3.75) (xy -0.9 3.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu")
		(uuid "f3f40fba-46bb-4bef-a691-d8a3acfc2c9e")
		(hatch edge 0.2)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -9 -6.25) (xy 9 -6.25) (xy 9 3.75) (xy 0.9 3.75) (xy 0.9 1.75) (xy -0.9 1.75) (xy -0.9 3.75)
				(xy -9 3.75)
			)
		)
	)
	(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -90)
		)
	)
)
