(footprint "M.2 3052S3_0.5H" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (attr exclude_from_pos_files)
  (fp_text reference "A2" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 415bd6a9-e404-4df3-a01d-96c327cd4d32)
  )
  (fp_text value "5G Module" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2d46411a-b760-4b18-8cbc-3c7730d05815)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c5e49348-08e3-49b5-afbc-910e717dafa9)
  )
  (fp_rect (start -15 -52) (end 15 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "Cmts.User") (tstamp 1c00fc89-397a-41bb-a4d5-0f19af5416f6))
  (model ":KICAD7_3DMODEL_DIR:Module.3dshapes/M.2 3052S3 Card.step"
    (offset (xyz 0 0 0.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
