(module D_SOD-323HE_AK (layer F.Cu) (tedit 5BCB12E6)
  (descr "SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf")
  (tags SOD-323HE)
  (attr smd)
  (fp_text reference REF** (at 0 -1.85) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value D_SOD-323HE_AK (at 0.1 1.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 -1.85) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.75 -0.85) (end -1.75 0.85) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.2 0) (end 0.45 0) (layer F.Fab) (width 0.1))
  (fp_line (start 0.2 0.35) (end -0.3 0) (layer F.Fab) (width 0.1))
  (fp_line (start 0.2 -0.35) (end 0.2 0.35) (layer F.Fab) (width 0.1))
  (fp_line (start -0.3 0) (end 0.2 -0.35) (layer F.Fab) (width 0.1))
  (fp_line (start -0.3 0) (end -0.5 0) (layer F.Fab) (width 0.1))
  (fp_line (start -0.3 -0.35) (end -0.3 0.35) (layer F.Fab) (width 0.1))
  (fp_line (start -0.9 0.7) (end -0.9 -0.7) (layer F.Fab) (width 0.1))
  (fp_line (start 0.9 0.7) (end -0.9 0.7) (layer F.Fab) (width 0.1))
  (fp_line (start 0.9 -0.7) (end 0.9 0.7) (layer F.Fab) (width 0.1))
  (fp_line (start -0.9 -0.7) (end 0.9 -0.7) (layer F.Fab) (width 0.1))
  (fp_line (start -1.85 -0.95) (end 1.7 -0.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.7 -0.95) (end 1.7 0.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.85 0.95) (end 1.7 0.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.85 -0.95) (end -1.85 0.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 0.85) (end 1.05 0.85) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.75 -0.85) (end 1.05 -0.85) (layer F.SilkS) (width 0.12))
  (pad A smd rect (at -0.65 0) (size 2 1.1) (layers F.Cu F.Paste F.Mask))
  (pad K smd rect (at 1.25 0) (size 0.8 1.1) (layers F.Cu F.Paste F.Mask))
  (model ${KICAD7_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323F.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
