(module 9P_Oval_3x1_1.25mm (layer F.Cu) (tedit 56EDE38B)
  (solder_mask_margin 0.01)
  (attr virtual)
  (fp_text reference J1 (at -6 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value PROG (at 0 2.1) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_circle (center -5.75 1.75) (end -5.65 1.75) (layer F.SilkS) (width 0.2))
  (pad 1 connect rect (at -5 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 2 connect oval (at -3.75 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 3 connect oval (at -2.5 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 4 connect oval (at -1.25 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 5 connect oval (at 0 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 6 connect oval (at 1.25 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 7 connect oval (at 2.5 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 8 connect oval (at 3.75 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 9 connect oval (at 5 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 2 thru_hole circle (at -3.75 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu))
  (pad 9 thru_hole circle (at 5 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu))
)
