(footprint "Murata_NFG0NCN162HL3" (version 20221018) (generator pcbnew)
  locked (layer "F.Cu")
  (property "LCSC" "C3212004")
  (property "MFG" "Murata")
  (property "MPN" "NFG0NCN162HL3D")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "EMI 3-inductor common mode filter")
  (property "ki_keywords" "EMI common mode filter c-phy")
  (attr smd)
  (fp_text reference "FL4" (at 0 -0.75 unlocked) (layer "F.SilkS") hide
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp b2a5d7c2-15bd-4ff3-a710-dc7d34efa4c3)
  )
  (fp_text value "Filter_EMI_Trio_CommonMode" (at 0.05 0.8 unlocked) (layer "F.Fab") hide
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp 2b3c3fcb-2939-4eb2-b6b4-4c997a9161b1)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.75 unlocked) (layer "F.Fab") hide
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp 6feea808-59fa-42d9-aa57-7e14e164cba6)
  )
  (fp_poly
    (pts
      (xy -0.55 -0.35)
      (xy -0.55 0.35)
      (xy -0.7 0.35)
      (xy -0.7 -0.35)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 700af3e4-98d6-4d56-9fc6-da2465239a30))
  (fp_poly
    (pts
      (xy 0.7 -0.35)
      (xy 0.7 0.35)
      (xy 0.55 0.35)
      (xy 0.55 -0.35)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp efb3052d-feed-442f-a27e-b6aad20314ec))
  (fp_line (start -0.7 0.35) (end -0.7 -0.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2610ca63-3625-4b44-a31e-603216182ea4))
  (fp_line (start 0.45 -0.6) (end -0.45 -0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 045af9a1-f200-4aed-bbb3-0164216ecfd1))
  (fp_line (start 0.45 0.6) (end -0.45 0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4cbe9c60-08d2-415f-a971-54ed66ee2eb7))
  (fp_line (start 0.7 -0.35) (end 0.7 0.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 39d5c9f3-07ca-4757-9c90-217cb9b26ba3))
  (fp_arc (start -0.7 -0.35) (mid -0.626777 -0.526777) (end -0.45 -0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c866fe9f-c8f0-4ba3-8a86-e447b1e3867b))
  (fp_arc (start -0.45 0.6) (mid -0.626777 0.526777) (end -0.7 0.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 73e87b84-6a3c-483f-89b6-39548ffb28a5))
  (fp_arc (start 0.45 -0.6) (mid 0.626777 -0.526777) (end 0.7 -0.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9b66abad-bad0-400f-8d41-b5a4a1ccaa23))
  (fp_arc (start 0.7 0.35) (mid 0.626777 0.526777) (end 0.45 0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7e816a13-52fd-42d6-865b-8cf41e6990df))
  (fp_rect (start -0.45 -0.34) (end 0.45 0.34)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.Fab") (tstamp 7a0a854f-1aa2-4b48-82a2-52ab26977a6b))
  (pad "" smd oval locked (at -0.35 -0.3) (size 0.2 0.25) (layers "F.Paste") (tstamp 6edb9eb5-ad2a-4a27-b933-355174592716))
  (pad "" smd oval locked (at -0.35 0.3) (size 0.2 0.25) (layers "F.Paste") (tstamp 008df04f-ef80-46a8-922c-45ed366451d5))
  (pad "" smd oval locked (at 0 -0.3) (size 0.2 0.25) (layers "F.Paste") (tstamp 851a579f-99c1-4f09-a1c9-e6d9be4a23d2))
  (pad "" smd oval locked (at 0 0.3) (size 0.2 0.25) (layers "F.Paste") (tstamp 4b98ab78-1e20-4907-92e9-32da71f869ef))
  (pad "" smd oval locked (at 0.35 -0.3) (size 0.2 0.25) (layers "F.Paste") (tstamp ccf76e72-b886-4513-9785-e22cbabdd59f))
  (pad "" smd oval locked (at 0.35 0.3) (size 0.2 0.25) (layers "F.Paste") (tstamp 269298d1-5f43-4fd5-a556-6a9f5bd243fe))
  (pad "1" smd roundrect locked (at -0.35 -0.3) (size 0.2 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer bottom_left bottom_right) (tstamp 4f95d9a5-49af-4792-94ed-783cd9632f0f))
  (pad "2" smd roundrect locked (at -0.35 0.3 180) (size 0.2 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer bottom_left bottom_right) (tstamp 9f4ac075-963b-464b-831f-8431dc39bed4))
  (pad "3" smd roundrect locked (at 0 -0.3) (size 0.2 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer bottom_left bottom_right) (tstamp 0065e36f-6ea9-4e7e-be3c-34b3be241794))
  (pad "4" smd roundrect locked (at 0 0.3 180) (size 0.2 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer bottom_left bottom_right) (tstamp 1677d220-ec9e-48fd-86ec-4ef1ee2e12bc))
  (pad "5" smd roundrect locked (at 0.35 -0.3) (size 0.2 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer bottom_left bottom_right) (tstamp 0579978e-426d-42d9-a60b-fa588ad93bdb))
  (pad "6" smd roundrect locked (at 0.35 0.3 180) (size 0.2 0.35) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.1) (chamfer bottom_left bottom_right) (tstamp bd899182-73bd-418f-a1b3-f13e2f353e53))
  (model ":KICAD7_3DMODEL_DIR:Filter.3dshapes/Murata NFG0NCN162HL3.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
