(module PLCC8 (layer F.Cu) (tedit 59D1F81C)
  (attr smd)
  (fp_text reference D3 (at 0 -3.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Cree_CLQ6A-TKW (at 0 3.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 2.5) (end 2.5 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 1.5) (end -1.5 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -3.1 -3) (end -3.1 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.1 -3) (end -2.1 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.1 -3) (end 3.1 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.1 -3) (end 3.1 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.1 3) (end 3.1 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.1 3) (end 3.1 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.1 3) (end -3.1 3) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.1 3) (end -3.1 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.1 3) (end -3 2.9) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.1 2.5) (end -2.6 3) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.8 2.9) (end -3 2.9) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 2.9) (end -3 2.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 2.7) (end -2.9 2.8) (layer F.SilkS) (width 0.15))
  (fp_circle (center -3.4 -2.9) (end -3.4 -3) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -0.99 -1.81) (size 3.32 0.78) (layers F.Cu F.Mask))
  (pad 4 smd rect (at -0.99 1.81) (size 3.32 0.78) (layers F.Cu F.Mask))
  (pad 2 smd rect (at -1.775 -0.45) (size 1.75 0.64) (layers F.Cu F.Mask))
  (pad 3 smd rect (at -1.775 0.45) (size 1.75 0.64) (layers F.Cu F.Mask))
  (pad 5 smd rect (at 1.81 1.75) (size 1.68 0.9) (layers F.Cu F.Mask))
  (pad 8 smd rect (at 1.81 -1.75) (size 1.68 0.9) (layers F.Cu F.Mask))
  (pad 6 smd rect (at 1.025 0.49) (size 3.25 0.72) (layers F.Cu F.Mask))
  (pad 7 smd rect (at 1.025 -0.49) (size 3.25 0.72) (layers F.Cu F.Mask))
  (pad 1 smd rect (at -0.485 -1.645) (size 2.31 1.11) (layers F.Cu F.Mask))
  (pad 4 smd rect (at -0.485 1.645) (size 2.31 1.11) (layers F.Cu F.Mask))
  (pad 6 smd rect (at 1.81 0.565) (size 1.68 0.87) (layers F.Cu F.Mask))
  (pad 7 smd rect (at 1.81 -0.565) (size 1.68 0.87) (layers F.Cu F.Mask))
  (pad 4 smd trapezoid (at -2.145 1.505) (size 1.01 0.5) (rect_delta -0.33 0 ) (layers F.Cu F.Mask))
  (pad 1 smd trapezoid (at -2.145 -1.505) (size 1.01 0.5) (rect_delta -0.33 0 ) (layers F.Cu F.Mask))
  (pad 2 smd trapezoid (at -2.225 -0.725) (size 0.85 0.3) (rect_delta 0.21 0 ) (layers F.Cu F.Mask))
  (pad 3 smd trapezoid (at -2.225 0.725) (size 0.85 0.3) (rect_delta 0.21 0 ) (layers F.Cu F.Mask))
  (pad 1 smd roundrect (at -0.9 -1.8) (size 3 0.9) (layers F.Paste)(roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -0.9 1.8) (size 3 0.9) (layers F.Paste)(roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 1.81 -1.75) (size 1.6 0.8) (layers F.Paste)(roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 1.81 1.75) (size 1.6 0.8) (layers F.Paste)(roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -1.775 -0.45) (size 1.6 0.6) (layers F.Paste)(roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -1.775 0.45) (size 1.6 0.6) (layers F.Paste)(roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 1.025 -0.49) (size 3 0.65) (layers F.Paste)(roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 1 0.5) (size 3 0.65) (layers F.Paste)(roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -2.5 -1.805) (size 1 0.78) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -2.5 1.805) (size 1 0.78) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -2.8 -0.555) (size 0.4 0.85) (layers F.Cu F.Mask)(roundrect_rratio 0.5))
  (pad 2 smd rect (at -2.725 -0.555) (size 0.15 0.85) (layers F.Cu F.Mask))
  (pad 3 smd roundrect (at -2.8 0.555) (size 0.4 0.85) (layers F.Cu F.Mask)(roundrect_rratio 0.5))
  (pad 3 smd rect (at -2.72 0.555) (size 0.15 0.85) (layers F.Cu F.Mask))
  (pad 8 smd roundrect (at 2.16 -1.75) (size 1.68 0.9) (layers F.Cu F.Mask)(roundrect_rratio 0.22))
  (pad 5 smd roundrect (at 2.16 1.75) (size 1.68 0.9) (layers F.Cu F.Mask)(roundrect_rratio 0.22))
  (pad 7 smd roundrect (at 2.16 -0.565) (size 1.68 0.87) (layers F.Cu F.Mask)(roundrect_rratio 0.23))
  (pad 6 smd roundrect (at 2.16 0.565) (size 1.68 0.87) (layers F.Cu F.Mask)(roundrect_rratio 0.23))
)
