(footprint "51338-1074 100P P0.4_Odd-Even" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "SoM Headers.kicad_sch")
  (property "Sheetname" "SoM Headers")
  (attr smd)
  (fp_text reference "J21" (at 0 -2.45 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 9c39b287-e135-413a-bfa1-7223c6da7c5b)
  )
  (fp_text value "Forlinx_FET3588-C_Bottom-Left" (at -11.4 -0.2 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)) (justify left))
    (tstamp 9bf012b2-9cf9-4cf5-b5e1-2ea49cc349a2)
  )
  (fp_text user "Own signals only" (at 0 0.55 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp 081e4496-1c32-4dd4-9cef-5b1fb4997172)
  )
  (fp_text user "${REFERENCE}" (at -11.4 0.3 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)) (justify left))
    (tstamp fe8d2dec-217d-41c1-8a48-6cfda592b8bd)
  )
  (fp_arc (start -11.775 -1.85) (mid -11.753033 -1.903033) (end -11.7 -1.925)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 7cf5c722-acbe-4c12-8d06-8cfc3f6f3d98))
  (fp_arc (start -11.7 1.925) (mid -11.753033 1.903033) (end -11.775 1.85)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp e3ca98be-f66c-402e-8ff4-e4093579c327))
  (fp_arc (start 11.7 -1.925) (mid 11.753033 -1.903033) (end 11.775 -1.85)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 1ec088d6-cda7-4e35-b502-d2da8d890511))
  (fp_arc (start 11.775 1.85) (mid 11.753033 1.903033) (end 11.7 1.925)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp b0db8b09-a008-4df4-a68a-3a90579056c3))
  (fp_poly
    (pts
      (xy -9.8 2.05)
      (xy -9.95 2.35)
      (xy -9.65 2.35)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 92004833-c93d-4e89-915e-4fd7e5f00155))
  (fp_poly
    (pts
      (xy -10.25 -1.85)
      (xy -11.7 -1.85)
      (xy -11.7 1.85)
      (xy -10.25 1.85)
      (xy -10.25 2)
      (xy -11.7 2)
      (xy -11.85 1.85)
      (xy -11.85 -1.85)
      (xy -11.7 -2)
      (xy -10.25 -2)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 4512920c-77a4-462e-b2fb-02da4b2a3f0b))
  (fp_poly
    (pts
      (xy 10.25 1.85)
      (xy 11.7 1.85)
      (xy 11.7 -1.85)
      (xy 10.25 -1.85)
      (xy 10.25 -2)
      (xy 11.7 -2)
      (xy 11.85 -1.85)
      (xy 11.85 1.85)
      (xy 11.7 2)
      (xy 10.25 2)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp a7ca71c3-6c49-4d40-a7af-d6f0cb1e29a6))
  (fp_rect (start -9.95 -1.25) (end 9.95 -0.8)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp ad20cee1-562f-49fb-9529-c1e27be399f7))
  (fp_rect (start -9.95 0.75) (end 9.95 1.2)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp e761e9be-00dc-4317-bfff-b93d60fa52ad))
  (fp_line (start -11.7 -1.7) (end -11.7 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f8a48021-148c-4d7c-9d69-69f7a182d672))
  (fp_line (start -11.35 2.05) (end 11.35 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b156b01c-c9e2-467a-8ff5-d618c1a11fd6))
  (fp_line (start 11.35 -2.05) (end -11.35 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d6f409a9-bcb8-457d-b66b-34cd99b2737c))
  (fp_line (start 11.7 1.7) (end 11.7 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9331ddb2-1f2e-4e28-a8c3-4d0e53130ae6))
  (fp_arc (start -11.7 -1.7) (mid -11.597487 -1.947487) (end -11.35 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 80fc000b-2e36-43bd-bdf5-c4b9b92f879f))
  (fp_arc (start -11.35 2.05) (mid -11.597487 1.947487) (end -11.7 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4e2d2064-cc53-4e71-adc5-b5aaef57e549))
  (fp_arc (start 11.35 -2.05) (mid 11.597487 -1.947487) (end 11.7 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 85839ac7-d050-43ea-921d-f212c06b815c))
  (fp_arc (start 11.7 1.7) (mid 11.597487 1.947487) (end 11.35 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c481779c-87cf-4045-baf3-e322a9045fb3))
  (fp_rect (start -11.55 -1.7) (end 11.55 1.7)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 4648d6ef-a71e-4a01-86b7-a8392213c77d))
  (pad "" smd oval (at -9.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 62afb48a-068e-42d8-94da-4a3213c342b7))
  (pad "" smd oval (at -9.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fb10199a-301b-4a30-8c0a-7b09f3dc38c4))
  (pad "" smd oval (at -9.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fc33ccb5-041d-4c3c-a423-45bbb6c2ede5))
  (pad "" smd oval (at -9.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 8765b59b-94da-42d1-9626-e92e9902bf6e))
  (pad "" smd oval (at -9 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp bce255df-6070-4b7d-a588-f6523493e8bd))
  (pad "" smd oval (at -9 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7fd3782b-1a9f-41e7-b625-f427ab7f7986))
  (pad "" smd oval (at -8.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d434dffe-ffeb-479b-baac-21394d102322))
  (pad "" smd oval (at -8.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d97a1c91-5ca5-4038-8771-fa729b98b0d4))
  (pad "" smd oval (at -8.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 2bd819fe-51b9-4e84-8888-66146b833d71))
  (pad "" smd oval (at -8.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 374d614f-f780-4c20-993b-ad10b905dd98))
  (pad "" smd oval (at -7.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 98f34a1b-1924-4c3f-b8b6-fd16e475f666))
  (pad "" smd oval (at -7.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7ef7bc37-e074-4917-a2b6-1da5b50128e7))
  (pad "" smd oval (at -7.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp dfa30d27-0044-470a-984c-7d3cef402b11))
  (pad "" smd oval (at -7.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a739137b-e9e0-4bfb-93ce-bd0a882b52dd))
  (pad "" smd oval (at -7 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 396fc51b-22a9-4d76-b91e-f8d3a4a1bae9))
  (pad "" smd oval (at -7 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 6a549824-fa5e-4482-94f1-8adbc7074179))
  (pad "" smd oval (at -6.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0a80e8ca-b6bd-42a3-bece-27423703a16d))
  (pad "" smd oval (at -6.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7a8e1bdb-37c2-43cf-998a-81e3f46780a4))
  (pad "" smd oval (at -6.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1577210c-f8a8-46f9-a3ee-161d192ad3f6))
  (pad "" smd oval (at -6.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0a9e2917-fd4d-44a7-84d2-f0074ab3d53b))
  (pad "" smd oval (at -5.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d2fb8bf4-d532-41f5-b621-19f319b598a1))
  (pad "" smd oval (at -5.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp eb1c14a9-0543-46b8-adc3-8eaeb847df38))
  (pad "" smd oval (at -5.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f9cd718b-3f6b-4738-ac8d-3c021bdccd4c))
  (pad "" smd oval (at -5.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp dd09290f-c60a-4732-ad67-cb9db243b56f))
  (pad "" smd oval (at -5 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 30ed3815-53f4-48aa-af25-f829a0bde697))
  (pad "" smd oval (at -5 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d90e4bd3-5a03-4513-9ef9-637118c11b94))
  (pad "" smd oval (at -4.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0e477e1b-aa6e-41d9-a13e-e718d36eff88))
  (pad "" smd oval (at -4.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp c663fe38-b305-4fee-b106-fc2ec8d55673))
  (pad "" smd oval (at -4.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp da369772-ef12-4800-a51d-7d7bd55eb016))
  (pad "" smd oval (at -4.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 982f0ea8-3157-4f51-ae52-2d645ff0f3fa))
  (pad "" smd oval (at -3.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp df125bfa-0c95-40d6-ab66-6a3939b99c09))
  (pad "" smd oval (at -3.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 2c5778d2-9745-4f2e-9085-dc07fb657f30))
  (pad "" smd oval (at -3.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7ab059c2-ecd9-4229-84f1-7274442746f2))
  (pad "" smd oval (at -3.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 76549bf3-23b3-4668-9c20-ed6eb5174507))
  (pad "" smd oval (at -3 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1fec2de3-3955-463c-b562-325100301968))
  (pad "" smd oval (at -3 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp aa0368cf-d26c-46ac-8e73-5863fb933a3b))
  (pad "" smd oval (at -2.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a2e0f1ed-2b43-4846-9ba9-6652511bf698))
  (pad "" smd oval (at -2.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a905eee5-bfeb-45b7-bd95-c978ab1a0aa5))
  (pad "" smd oval (at -2.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5aa29cce-7e6a-44d7-b5a3-34c8352cb161))
  (pad "" smd oval (at -2.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 006e8c94-a407-47fe-886a-4633ac6d912f))
  (pad "" smd oval (at -1.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 378a659d-8c39-4787-9bf5-baa90637d2e7))
  (pad "" smd oval (at -1.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 85a67500-eb8c-4d57-82c1-a7b0c01725c7))
  (pad "" smd oval (at -1.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fb2fda11-3879-4245-87a4-3de8849a354c))
  (pad "" smd oval (at -1.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp de26f01c-783c-448a-bc2e-11354c20e6f4))
  (pad "" smd oval (at -1 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f63e0c8b-d90c-4262-9b66-7ac28d51598a))
  (pad "" smd oval (at -1 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0c441335-d776-4822-8e60-cd616a1458c9))
  (pad "" smd oval (at -0.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3f50ab8f-6843-40b8-beee-4bdebc27bbe5))
  (pad "" smd oval (at -0.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp cd6599fc-ba09-48d7-a881-5d92f29d04f0))
  (pad "" smd oval (at -0.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d2fc9632-47f4-4a6d-8e37-bbf42bebd503))
  (pad "" smd oval (at -0.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 46dbe0f4-8ec8-4032-a22c-bbb607c5b46c))
  (pad "" smd oval (at 0.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5cee3ffd-97dc-46cf-8ac2-bde629714e69))
  (pad "" smd oval (at 0.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp dfdf0a4e-2776-4607-ba02-cfe9bdf25d99))
  (pad "" smd oval (at 0.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5e171ec9-aec2-4f7d-94ab-3fd15e51750e))
  (pad "" smd oval (at 0.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 560a7f8e-4be7-4bd4-8c29-00c8d18b25f1))
  (pad "" smd oval (at 1 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 6a272755-2972-48eb-9829-a3320e04148a))
  (pad "" smd oval (at 1 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f8843421-e33b-458b-b644-c325d6a795cb))
  (pad "" smd oval (at 1.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 115daa0d-4f3c-4e73-99c3-9a783333fa24))
  (pad "" smd oval (at 1.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp abf68735-5c43-4a4e-82da-c1ab344c39be))
  (pad "" smd oval (at 1.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp bdf8118c-a43b-462d-8d70-352501545aeb))
  (pad "" smd oval (at 1.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 537cc5aa-a3a2-48a2-9ff8-056a271245e4))
  (pad "" smd oval (at 2.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7533f41c-a01c-4f09-ba18-59cc9fe51efb))
  (pad "" smd oval (at 2.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b71d4ae4-18b3-4bc4-8705-72a7bc46d3c0))
  (pad "" smd oval (at 2.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 164ab360-2e37-47ad-b19b-0f4281389fc4))
  (pad "" smd oval (at 2.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 211b863a-7e09-4053-9299-2da926266662))
  (pad "" smd oval (at 3 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5b6096ec-6099-490d-9f76-9cea98c3ff58))
  (pad "" smd oval (at 3 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 9ce90b55-ce11-4510-85ca-1631f786c937))
  (pad "" smd oval (at 3.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 84e2bf65-85b1-4462-b7fc-c755c530ed1d))
  (pad "" smd oval (at 3.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4ef4f5ce-4f26-48f7-95b8-5da5e020b830))
  (pad "" smd oval (at 3.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 8261f07f-8511-4fbd-8e33-78f75364b60f))
  (pad "" smd oval (at 3.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 47477c8b-b7e8-4441-bbab-9bf0cf2e76a7))
  (pad "" smd oval (at 4.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 9a0ff1f2-7ac1-4a9d-9de8-d60a791d0030))
  (pad "" smd oval (at 4.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 9ba7c44a-acc6-4aa5-aea5-94c9f2f33dc8))
  (pad "" smd oval (at 4.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp c8b1a32c-f7b1-4006-8b38-94ea2aff01e3))
  (pad "" smd oval (at 4.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e537c528-61c0-47b3-886c-c289d00d3fad))
  (pad "" smd oval (at 5 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp c8751634-f800-4f79-939e-a60df0c33305))
  (pad "" smd oval (at 5 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 499056b7-111d-438f-81ea-18e5e439f764))
  (pad "" smd oval (at 5.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 066339a1-08c9-4786-ae0a-e92eddad9ac2))
  (pad "" smd oval (at 5.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7ac31498-4868-4b06-b2b5-48defa489635))
  (pad "" smd oval (at 5.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a724c659-5fcb-4b5a-862a-6298491a0d29))
  (pad "" smd oval (at 5.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 104769de-4ae3-4039-9c49-63a3597ddbcd))
  (pad "" smd oval (at 6.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f1c5a75e-eaae-4e40-99c6-83da2b610628))
  (pad "" smd oval (at 6.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp beed7c8c-c7d6-4126-a213-5a6d99d0bba2))
  (pad "" smd oval (at 6.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d7a0db15-4439-4065-a801-c481668292e6))
  (pad "" smd oval (at 6.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp bcf75712-5198-4c3b-abc8-0bfa2a4164fb))
  (pad "" smd oval (at 7 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 614c0870-49c9-414a-898b-6733cfaebd39))
  (pad "" smd oval (at 7 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 138fed1c-e044-442f-a6d6-464376bcb9ae))
  (pad "" smd oval (at 7.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp c0d86d0a-7aa6-4372-b445-be1475bfbfa2))
  (pad "" smd oval (at 7.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 2aeb0c12-57f4-47fd-bac9-55be4fe4c173))
  (pad "" smd oval (at 7.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a255aafd-9fe9-4e8a-8d04-babcb9891ab9))
  (pad "" smd oval (at 7.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp cb1bb2d9-c3b9-446e-9889-27fcfe31fb23))
  (pad "" smd oval (at 8.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 38c49388-88cd-40b1-92e4-5b6dbfaf3419))
  (pad "" smd oval (at 8.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 8c4e56e9-fb4d-4b4b-8354-684ce02763ad))
  (pad "" smd oval (at 8.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 07dbdbab-56b5-424e-a1b2-03df93ac73ae))
  (pad "" smd oval (at 8.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a9559597-8591-4977-acdd-d7aadcb70604))
  (pad "" smd oval (at 9 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fd500fa1-3898-4f13-aec3-f423bfd1653e))
  (pad "" smd oval (at 9 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 6273bf02-18d9-40be-9bfb-d8ede965b7e7))
  (pad "" smd oval (at 9.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4ee005e5-096c-4298-9f83-4e756ac6f669))
  (pad "" smd oval (at 9.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp ead3a9ff-89c1-4f8f-9c1d-f74d73aaab35))
  (pad "" smd oval (at 9.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 50aa3fda-beeb-4de5-86ee-89f35e0e5c17))
  (pad "" smd oval (at 9.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 331b0868-b899-4bc0-b3bb-da922d8a6003))
  (pad "1" smd roundrect (at -9.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 62fabb54-4039-4055-a6c6-c5ae21f45957))
  (pad "2" smd roundrect (at -9.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 720ac49a-ff9d-44cb-9250-1c9c97ce8c00))
  (pad "3" smd roundrect (at -9.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp dd96c3e2-5a86-4237-9a6b-09f197618661))
  (pad "4" smd roundrect (at -9.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b9c18109-95de-4c11-8164-dd5bd339540d))
  (pad "5" smd roundrect (at -9 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp bd4a8676-24d2-4d61-b724-2449b165bfbf))
  (pad "6" smd roundrect (at -9 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2bd42e46-67ae-4e6c-ba78-87eef330dd24))
  (pad "7" smd roundrect (at -8.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6f352cae-def6-44b2-8ded-75080baa78e6))
  (pad "8" smd roundrect (at -8.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5c970e67-310d-4e7d-b38b-d5aff75fd608))
  (pad "9" smd roundrect (at -8.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 394e7a57-f47b-408a-bb03-8c2ba0cb640e))
  (pad "10" smd roundrect (at -8.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b530afae-da2c-438b-bf0f-4b86c02e23a2))
  (pad "11" smd roundrect (at -7.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp c460e82d-2458-47fe-a1e3-c6d27753f6cd))
  (pad "12" smd roundrect (at -7.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 8cdcb7c0-3b5e-496a-a97c-d3f99d65fe8f))
  (pad "13" smd roundrect (at -7.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 3def16d7-943b-4f85-a4c1-83def88572d6))
  (pad "14" smd roundrect (at -7.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4e1f3a29-cc57-459f-b624-016b55206796))
  (pad "15" smd roundrect (at -7 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 1f07a489-be23-4310-8ad9-673d06279cb6))
  (pad "16" smd roundrect (at -7 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2df1252e-9a68-4ae9-ad6f-631a0a74f904))
  (pad "17" smd roundrect (at -6.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp dc340138-21a0-48c9-9729-0b9d4d6aa48f))
  (pad "18" smd roundrect (at -6.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp efeda116-4464-4d25-bbf3-8221228fa721))
  (pad "19" smd roundrect (at -6.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp a0a850a6-bb6d-466d-8af5-da705bfef0b2))
  (pad "20" smd roundrect (at -6.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b3dc846d-0eff-43e5-ad26-1c31ce8f8376))
  (pad "21" smd roundrect (at -5.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 8b1ca0b2-7a32-4afe-bb5c-145c0df109cb))
  (pad "22" smd roundrect (at -5.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4db3c06b-2d28-4974-a533-2e46b5c499d9))
  (pad "23" smd roundrect (at -5.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5157f674-6210-4bbf-8839-b128801933e6))
  (pad "24" smd roundrect (at -5.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5d072933-0e9b-4da7-8f0f-dd605780f677))
  (pad "25" smd roundrect (at -5 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 8a86e78f-0a8f-4d05-a526-402c4382425b))
  (pad "26" smd roundrect (at -5 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b29f09b9-b664-44b8-99f2-d766a1082bf6))
  (pad "27" smd roundrect (at -4.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2294cb09-9eae-48a8-9d47-7e59faf93b79))
  (pad "28" smd roundrect (at -4.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp f7b74e7b-dfb2-4b7c-9058-8a02963747ae))
  (pad "29" smd roundrect (at -4.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 51818cc0-7be3-4323-ac6c-570fbc56bdda))
  (pad "30" smd roundrect (at -4.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ea27c595-e231-4e71-8b5b-111585e11695))
  (pad "31" smd roundrect (at -3.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5cfef5b0-f2fc-42c6-b43f-37a7cc889965))
  (pad "32" smd roundrect (at -3.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6c63755c-6817-4a09-b7be-8a9ad3c085a7))
  (pad "33" smd roundrect (at -3.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 09d4ac6e-68b5-4123-ba33-410573afc1d2))
  (pad "34" smd roundrect (at -3.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp c5c7aa32-46ba-4a54-98f2-8fd785da0083))
  (pad "35" smd roundrect (at -3 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp f55b6366-3bd9-401c-b622-fdb13dfe8254))
  (pad "36" smd roundrect (at -3 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2da5f052-dd41-4d46-8c83-5e94e7dce0f1))
  (pad "37" smd roundrect (at -2.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 477b2b9e-c113-4b31-b4d7-7bd9175ac3a4))
  (pad "38" smd roundrect (at -2.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp d21c1f42-488c-4150-99b3-f546ba21f77a))
  (pad "39" smd roundrect (at -2.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4bbdcef3-7768-4e4c-8fd5-23e9d5f51d19))
  (pad "40" smd roundrect (at -2.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4c660636-a3c2-46fc-b1a0-a0584ca13093))
  (pad "41" smd roundrect (at -1.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 16a8d289-15c6-4b7b-9893-353ec7b5944c))
  (pad "42" smd roundrect (at -1.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 904f3d85-bbf0-4589-9a12-f602df7c8013))
  (pad "43" smd roundrect (at -1.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 61dc9e0c-ad2c-43ca-9575-cb77e18374ce))
  (pad "44" smd roundrect (at -1.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 10079ff3-200b-4412-a0ab-122c735fe7f7))
  (pad "45" smd roundrect (at -1 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5c842c48-93d1-4da8-867d-679d4dc09224))
  (pad "46" smd roundrect (at -1 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 21659d04-e29e-4f5f-8acc-55c48415355b))
  (pad "47" smd roundrect (at -0.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp a2a512fa-df0a-4c38-9e97-741f769c1033))
  (pad "48" smd roundrect (at -0.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 829a6e08-59a6-4ccd-8ecd-103942e9f881))
  (pad "49" smd roundrect (at -0.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ce6a318c-5f3e-4275-90d9-6340806b1875))
  (pad "50" smd roundrect (at -0.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp cad12fb6-599d-4551-a729-374554c9bf0e))
  (pad "51" smd roundrect (at 0.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp e7053cbe-fdbb-4730-b167-e7f735489051))
  (pad "52" smd roundrect (at 0.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5fb7e58e-0eca-4e1f-81de-9d5432a03aed))
  (pad "53" smd roundrect (at 0.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6d143c5e-682c-46fe-9662-716fd91a140c))
  (pad "54" smd roundrect (at 0.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ac887f12-0c8f-4ccc-9a74-3611c1c6a017))
  (pad "55" smd roundrect (at 1 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp acc0c64a-b394-496b-ab92-a798e19306a5))
  (pad "56" smd roundrect (at 1 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5cce1429-0ff2-49a4-9da5-439a0047fa79))
  (pad "57" smd roundrect (at 1.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 368b5d3d-e6c0-4bbd-a905-c4169657ab74))
  (pad "58" smd roundrect (at 1.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp fa2d08a5-db46-4909-8322-d234694a8ac5))
  (pad "59" smd roundrect (at 1.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 46a2a2c8-4dc7-4389-92fd-de480d4b0f66))
  (pad "60" smd roundrect (at 1.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 57641311-488f-451b-9a8c-77b8f7dea276))
  (pad "61" smd roundrect (at 2.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 15c1bc0d-a866-4bf0-81eb-104cc3077ebe))
  (pad "62" smd roundrect (at 2.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6ffbcbff-ca18-4a8b-83f7-ed4ed3fe3f4d))
  (pad "63" smd roundrect (at 2.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 879b2c07-6d1b-47a3-ab61-6b7f68ffaafa))
  (pad "64" smd roundrect (at 2.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 802abd78-f35b-4d06-98e5-891f1e5952eb))
  (pad "65" smd roundrect (at 3 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 34ca1c7e-fc36-4d74-b68e-0e79fe88627c))
  (pad "66" smd roundrect (at 3 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4d6a5fda-d217-4bd8-a01c-323a4bb71775))
  (pad "67" smd roundrect (at 3.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp f1046d0d-a363-4235-935a-427c74f919d1))
  (pad "68" smd roundrect (at 3.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b5e81e2b-2bd6-4560-87c2-f794d022bb07))
  (pad "69" smd roundrect (at 3.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 642107fc-eef1-43ed-beaf-582849562d69))
  (pad "70" smd roundrect (at 3.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b767665d-a66e-4c96-b2a0-356c83c88d6f))
  (pad "71" smd roundrect (at 4.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6ae31bb4-02e7-4bd3-bd69-c0e391f7f17e))
  (pad "72" smd roundrect (at 4.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5a933dd2-4362-47d2-803d-91d5c6de2238))
  (pad "73" smd roundrect (at 4.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp f98a5e43-8eeb-4e5f-9a97-77545321a08a))
  (pad "74" smd roundrect (at 4.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6bf496ec-bf08-420b-b1fa-af01d8e9334d))
  (pad "75" smd roundrect (at 5 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 876d4188-5623-42da-b211-92705fba75bc))
  (pad "76" smd roundrect (at 5 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 90b79239-513d-4938-9880-0ab106217c80))
  (pad "77" smd roundrect (at 5.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 505b10f2-2cac-447b-9999-37557746f964))
  (pad "78" smd roundrect (at 5.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 226ebab2-18eb-4ec1-92d4-841fba5d8d51))
  (pad "79" smd roundrect (at 5.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 1d83194b-d009-4d02-894a-97c4e69e3e59))
  (pad "80" smd roundrect (at 5.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 66404164-a973-46aa-b9ec-94b52b62c3c3))
  (pad "81" smd roundrect (at 6.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6ba1467a-e4ac-4213-b1ac-986ab8b62047))
  (pad "82" smd roundrect (at 6.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 3f8bda30-59f8-4086-8eb3-9c2aeba60f62))
  (pad "83" smd roundrect (at 6.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2f06f77c-e756-43d1-bf57-3e7b8f482914))
  (pad "84" smd roundrect (at 6.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5bdd572b-7dea-4e4b-97f1-8c454dcf718a))
  (pad "85" smd roundrect (at 7 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp e14280e8-84b4-4f25-9dcc-a8f712f30b6f))
  (pad "86" smd roundrect (at 7 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp a5478306-acc4-4390-a0f4-c451fabfdcb7))
  (pad "87" smd roundrect (at 7.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 0150428b-aa80-45a6-a257-745e76823473))
  (pad "88" smd roundrect (at 7.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 537b7d58-6cde-457b-aacb-12e278a5fbda))
  (pad "89" smd roundrect (at 7.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 35f40d03-5851-414d-bc17-3a6f25b616f0))
  (pad "90" smd roundrect (at 7.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp c6eda114-4a93-41a1-9fa8-f91cae6af4a5))
  (pad "91" smd roundrect (at 8.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp fb7d17e0-ead8-48e5-bd5c-0d092db6d049))
  (pad "92" smd roundrect (at 8.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 32c07ccd-f9f2-4940-9d08-77eeba66eb5f))
  (pad "93" smd roundrect (at 8.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b1e4c422-c565-4976-a164-8414652fca2c))
  (pad "94" smd roundrect (at 8.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 1c24b37f-e27f-490c-9ff6-d0a09c0e1063))
  (pad "95" smd roundrect (at 9 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp bf754647-8f2b-4a78-904a-a92c5dc27bb1))
  (pad "96" smd roundrect (at 9 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 1ddea5f5-8233-4c28-a8d4-17c3257b0768))
  (pad "97" smd roundrect (at 9.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 51e1316c-5c5a-4518-aef4-51e6e15c522c))
  (pad "98" smd roundrect (at 9.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 18796ada-ac4e-4e64-bbe8-8e0da36b9ad8))
  (pad "99" smd roundrect (at 9.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 58ea08ca-2ff5-44e9-abe1-51ff026c8f13))
  (pad "100" smd roundrect (at 9.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp db69076f-29fc-4b3b-b7ad-8ac8409e58dd))
  (pad "MP" smd roundrect (at -10.75 -1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 9ee4b8a7-1ff5-491e-97e5-4f4eb80ecdee))
  (pad "MP" smd roundrect (at -10.75 1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 665efc2e-2ab6-45e8-bae3-7a6a410919af))
  (pad "MP" smd roundrect (at 10.75 -1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 81f3d091-a2a1-4e3c-baad-16708cd4fafb))
  (pad "MP" smd roundrect (at 10.75 1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp ea5a57cc-cad7-42a2-b62c-c75cbc95a2e8))
  (model "${KICAD7_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex 51338-1074.stp"
    (offset (xyz 0 0 0.64))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
