(footprint "TH_4P_2x0.8_P1.05"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.95 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "21fd99b3-9688-4285-8448-8f6831869dba")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TH_4P_2x0.8_P1.05"
		(at 0 -2.55 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "cc1b64a1-1b8d-433c-8fd2-078d63828b2d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 14.35 -13.55 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f7726c32-4f3e-46b0-b996-2cb050aac1cc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 14.35 -13.55 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e037dfc8-3b49-4862-8a8d-dd60c956d078")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 14.35 -13.55 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "097ae411-7624-4076-85aa-4602b2ee2740")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_poly
		(pts
			(xy -1.6 1.75) (xy -1.75 1.95) (xy -1.45 1.95)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "2ee8dc0e-ecb9-4425-a67a-c83fd34e8a0b")
	)
	(fp_line
		(start -2.125 1.525)
		(end -2.125 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a268a05a-8a5a-46a0-93f3-440ec83df84a")
	)
	(fp_line
		(start -1.575 -0.55)
		(end 1.575 -0.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7e8d2c49-3a6e-4ea3-b621-9b1cd9a0d7f8")
	)
	(fp_line
		(start 1.9 1.75)
		(end -1.9 1.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "dfd014e1-d532-40cb-8b11-e53ec9cf982c")
	)
	(fp_line
		(start 2.125 0)
		(end 2.125 1.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "adb37fe5-292c-4269-a46b-7ad9f35a02c7")
	)
	(fp_arc
		(start -2.125 0)
		(mid -1.963909 -0.388909)
		(end -1.575 -0.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fafdda0f-f752-490a-8711-db47227db291")
	)
	(fp_arc
		(start -1.9 1.75)
		(mid -2.059099 1.684099)
		(end -2.125 1.525)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ab6e59f0-63c2-4070-a685-ee01cfa0c94e")
	)
	(fp_arc
		(start 1.575 -0.55)
		(mid 1.963909 -0.388909)
		(end 2.125 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a37b8fb5-07a8-44ae-93f5-0616a3e23637")
	)
	(fp_arc
		(start 2.125 1.525)
		(mid 2.059099 1.684099)
		(end 1.9 1.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b56e8fe0-999e-4677-93bc-93c795c4721b")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.05 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "cb87d749-7a37-4faa-a9ec-71108b095690")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -1.575 0)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "74113cc5-fd10-43ce-9ed0-175cf0e36245")
	)
	(pad "1" connect roundrect
		(at -1.575 0)
		(size 0.8 2)
		(drill
			(offset 0 0.6)
		)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer bottom_left bottom_right)
		(uuid "8014d863-e42a-47af-80fc-28fab1afb619")
	)
	(pad "2" thru_hole circle
		(at -0.525 0)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d1d2af6d-c454-49fd-87bd-efcab8147ce6")
	)
	(pad "2" connect roundrect
		(at -0.525 0)
		(size 0.8 2)
		(drill
			(offset 0 0.6)
		)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer bottom_left bottom_right)
		(uuid "ada8b8e6-607a-45da-b256-5693a70e08f3")
	)
	(pad "3" thru_hole circle
		(at 0.525 0)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1c59bf35-67da-4440-9bd1-5c397b86af6a")
	)
	(pad "3" connect roundrect
		(at 0.525 0)
		(size 0.8 2)
		(drill
			(offset 0 0.6)
		)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer bottom_left bottom_right)
		(uuid "eab09fc3-65f6-4654-b1ff-a965cc798384")
	)
	(pad "4" thru_hole circle
		(at 1.575 0)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "74d7e5e7-89fb-4360-9911-0643cbf7eae7")
	)
	(pad "4" connect roundrect
		(at 1.575 0)
		(size 0.8 2)
		(drill
			(offset 0 0.6)
		)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer bottom_left bottom_right)
		(uuid "41347297-740c-4573-a131-9c9a7c736a6a")
	)
)