(footprint "1608_C" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (tags "0603 1608 Capacitor")
  (property "Dielectric" "X5R")
  (property "Footprint_Density" "C")
  (property "Footprint_Library" "Capacitor_SMD")
  (property "MPN" "GRM188R61A226ME15D")
  (property "Package" "1608")
  (property "Sheet file" "/home/stefan/Projects/Current/StickHub/StickHub.kicad_sch")
  (property "Sheet name" "")
  (property "Spice_Model" "100n")
  (property "Spice_Netlist_Enabled" "Y")
  (property "Spice_Primitive" "C")
  (property "Tolerance" "20%")
  (property "Voltage" "10V")
  (solder_mask_margin 0.02)
  (solder_paste_margin -0.03)
  (attr smd)
  (fp_text reference "D12" (at 1.05 0 unlocked) (layer "F.SilkS")
      (effects (font (size 0.6 0.6) (thickness 0.125)) (justify left))
    (tstamp 9db52b07-7a9b-439b-bb1e-0453d7417e27)
  )
  (fp_text value "12V" (at 1.05 0.5 unlocked) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)) (justify left))
    (tstamp 61a07bf6-ac79-4860-a01d-92fdf946ffea)
  )
  (fp_arc (start -1.05 -0.275) (mid -0.984099 -0.434099) (end -0.825 -0.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp bf488275-601c-4f9d-9758-dfd1ce0d71cc))
  (fp_arc (start -0.825 0.5) (mid -0.984099 0.434099) (end -1.05 0.275)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp bbaa483f-83bb-445f-aed5-5a622435ddb8))
  (fp_poly
    (pts
      (xy -0.975 -0.275)
      (xy -0.975 0.275)
      (xy -1.125 0.275)
      (xy -1.125 -0.275)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 1074f85d-1337-4d08-9472-510aa415c5b4))
  (fp_poly
    (pts
      (xy 0.325 -0.425)
      (xy -0.825 -0.425)
      (xy -0.825 -0.575)
      (xy 0.325 -0.575)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 063483ce-7b79-4ef0-9332-dc9d23a00c60))
  (fp_poly
    (pts
      (xy 0.325 0.575)
      (xy -0.825 0.575)
      (xy -0.825 0.425)
      (xy 0.325 0.425)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp a539665b-3178-424c-b139-dd1a0f2b1c0c))
  (fp_line (start -1.05 0.275) (end -1.05 -0.275)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 277c9b8a-8e01-4254-8bee-7343f5eadf75))
  (fp_line (start -0.825 -0.5) (end 0.825 -0.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ec898fa3-e490-43da-a36f-deba3abab4fa))
  (fp_line (start 0.825 0.5) (end -0.825 0.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f5c0e207-4349-4f3c-a7c0-c85f56c5c80b))
  (fp_line (start 1.05 -0.275) (end 1.05 0.275)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dbf0de6e-abac-4d8c-a4b8-85644565e12b))
  (fp_arc (start -1.05 -0.275) (mid -0.984099 -0.434099) (end -0.825 -0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4e13f9e9-9377-4d1f-a6d4-40f6abdb636e))
  (fp_arc (start -0.825 0.5) (mid -0.984099 0.434099) (end -1.05 0.275)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 60a1e4e8-a2c8-49fd-817c-873cb30e1365))
  (fp_arc (start 0.825 -0.5) (mid 0.984099 -0.434099) (end 1.05 -0.275)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f8782fb0-7119-4c43-9019-e166caec9352))
  (fp_arc (start 1.05 0.275) (mid 0.984099 0.434099) (end 0.825 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 29e70418-c058-420f-9304-23cc4572a587))
  (fp_line (start -0.8 -0.4) (end 0.8 -0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp d33eb999-1ec5-4244-9539-70123d3e89cf))
  (fp_line (start -0.8 0.4) (end -0.8 -0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp ceac5a95-96bf-41c1-a842-a5b6ef5c89d3))
  (fp_line (start 0.8 -0.4) (end 0.8 0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 993a5579-c479-4982-8c41-3b8be0a94e8a))
  (fp_line (start 0.8 0.4) (end -0.8 0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp a29e2d64-b278-47cf-9dc2-96b8466c84f5))
  (pad "" smd oval (at -0.675 0) (size 0.4 0.6) (layers "F.Paste") (tstamp f333a996-54eb-46ce-9797-6cc8bb9cdd7d))
  (pad "" smd oval (at 0.675 0) (size 0.4 0.6) (layers "F.Paste") (tstamp f2653da4-bb52-4c7b-bdb1-61c1ed4df903))
  (pad "1" smd roundrect (at -0.675 0) (size 0.55 0.8) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp cac719bf-5915-437e-9ae1-dccd538cf813))
  (pad "2" smd roundrect (at 0.675 0) (size 0.55 0.8) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2)
    (chamfer_ratio 0.05) (chamfer top_left bottom_left) (tstamp e18aa015-1673-4156-9771-448f28004169))
  (model "${KICAD7_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
