(module "SOT-883B" (layer F.Cu) (tedit 5E35B97F)
  (solder_mask_margin 0.02)
  (solder_paste_margin -0.03)
  (attr smd)
  (fp_text reference "Q1" (at -1.25 0) (layer F.SilkS) hide
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value "PMZB600UNELYL" (at 0 0.75) (layer F.Fab)
    (effects (font (size 0.3 0.3) (thickness 0.075)))
  )
  (fp_circle (center -0.55 -0.6) (end -0.5 -0.6) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.9 -0.7) (end 0.9 -0.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.9 -0.7) (end 0.9 0.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.9 0.7) (end -0.9 0.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.9 0.7) (end -0.9 -0.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.65 -0.45) (end 0.65 -0.45) (layer F.Fab) (width 0.05))
  (fp_line (start 0.65 -0.45) (end 0.65 0.45) (layer F.Fab) (width 0.05))
  (fp_line (start 0.65 0.45) (end -0.65 0.45) (layer F.Fab) (width 0.05))
  (fp_line (start -0.65 0.45) (end -0.65 -0.45) (layer F.Fab) (width 0.05))
  (pad "3" smd rect (at 0.35 0) (size 0.4 0.7) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -0.35 0.225) (size 0.4 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at -0.35 -0.225) (size 0.4 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KICAD7_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-883B.step"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
