(footprint "JST_SHD_SM20B-SRDS-G-TF_2x10_P1.0_Right_Angle" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "G4ESC.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connectable mounting pin connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr through_hole)
  (fp_text reference "J2" (at -7.4 0 90 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp dc3dc8cb-c7da-40c3-8ca6-4fa118c01dc7)
  )
  (fp_text value "Conn_02x10_Odd_Even_MountingPin" (at 0 4.3 unlocked) (layer "F.SilkS") hide
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp ec252a8b-6c15-4c63-a88d-ff4b48c3a2ca)
  )
  (fp_text user "${REF}" (at 0 1.15 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 30a3d8ea-3c7a-467d-89fe-ed7596ad2ef6)
  )
  (fp_poly
    (pts
      (xy 4.5 -3.75)
      (xy 4.4 -3.9)
      (xy 4.6 -3.9)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp b5d3de5a-da64-4e3c-a055-85598fdcb835))
  (fp_poly
    (pts
      (xy -4.95 2.85)
      (xy -5.6 2.85)
      (xy -5.6 2.7)
      (xy -4.95 2.7)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 2122d32c-e5a9-4143-944c-b3f2669eb4ee))
  (fp_poly
    (pts
      (xy 5.6 2.85)
      (xy 4.95 2.85)
      (xy 4.95 2.7)
      (xy 5.6 2.7)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 58bd83e9-6044-44a8-a39d-c1a1c121c341))
  (fp_poly
    (pts
      (xy -6.85 2.85)
      (xy -6.7 2.85)
      (xy -6.7 -2.7)
      (xy -4.95 -2.7)
      (xy -4.95 -2.85)
      (xy -6.85 -2.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 286adb52-3c61-4443-b535-83a4d3df6398))
  (fp_poly
    (pts
      (xy 6.85 2.85)
      (xy 6.7 2.85)
      (xy 6.7 -2.7)
      (xy 4.95 -2.7)
      (xy 4.95 -2.85)
      (xy 6.85 -2.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 33438efd-7578-4889-a9c9-bf18b5407ae8))
  (fp_line (start -6.8 -2.55) (end -6.8 2.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 88bd2e40-da4e-483d-ac11-cb634141d867))
  (fp_line (start -6.55 -2.8) (end -4.95 -2.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4eea8075-a83d-4550-bc93-3fa5b96d3788))
  (fp_line (start -4.95 -2.8) (end -4.95 -3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 099a4301-3b4f-4743-b11d-5ca617a53dc4))
  (fp_line (start -4.95 2.9) (end -6.55 2.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ce7ce8a6-c12c-4787-96ec-1a47ba62636e))
  (fp_line (start -4.95 3.45) (end -4.95 2.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7584ac02-5af1-4222-8a3f-5fca8644ccb0))
  (fp_line (start -4.6 3.8) (end 4.6 3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 55b72c69-5032-4f71-8cb8-eb0081521816))
  (fp_line (start 4.6 -3.8) (end -4.6 -3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1ce01148-d1d9-4375-a280-6e820565dcde))
  (fp_line (start 4.95 -2.8) (end 4.95 -3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 23463bca-0f50-4fdd-a6d5-65463b3ff403))
  (fp_line (start 4.95 2.9) (end 6.55 2.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 638f65f7-2ecb-4f9b-8014-e64962c28622))
  (fp_line (start 4.95 3.45) (end 4.95 2.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 65cfe1b8-69fd-4f20-bfdc-af1ff6a3a523))
  (fp_line (start 6.55 -2.8) (end 4.95 -2.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5b75baa9-7779-4ec6-bf75-bc5359f565ca))
  (fp_line (start 6.8 -2.55) (end 6.8 2.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bc4118f1-ea8a-4d44-88b3-2ba097c3efc1))
  (fp_arc (start -6.8 -2.55) (mid -6.726777 -2.726777) (end -6.55 -2.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1962674e-0b88-4275-8a7a-6efba2e70776))
  (fp_arc (start -6.55 2.9) (mid -6.726777 2.826777) (end -6.8 2.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0c661959-5dd3-4798-9356-c9277672e5ad))
  (fp_arc (start -4.95 -3.45) (mid -4.847487 -3.697487) (end -4.6 -3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2d4ed947-5fff-4ae3-b414-e735a03fe223))
  (fp_arc (start -4.6 3.8) (mid -4.847487 3.697487) (end -4.95 3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c0df4ee2-9b60-4763-889a-3badc8af8cee))
  (fp_arc (start 4.6 -3.8) (mid 4.847487 -3.697487) (end 4.95 -3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 65744007-0143-4032-ade8-ae7af8da67a8))
  (fp_arc (start 4.95 3.45) (mid 4.847487 3.697487) (end 4.6 3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e5948ed5-caf6-4317-ac2b-c7bebf4895fc))
  (fp_arc (start 6.55 -2.8) (mid 6.726777 -2.726777) (end 6.8 -2.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4413d8e4-1d39-40f3-8c2c-8187856683e2))
  (fp_arc (start 6.8 2.65) (mid 6.726777 2.826777) (end 6.55 2.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 126c140b-3de0-4298-9923-49f4f9d7f8b2))
  (fp_line (start -6.55 2.8) (end -6.55 3.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e61875ad-9c2a-41fb-b74f-95a88e275782))
  (fp_line (start -6.55 3.3) (end -6.55 3.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c94db70d-c671-4686-ac2e-cd1b241653ac))
  (fp_line (start -6.55 3.8) (end -6.55 4.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d898832d-d2bc-4409-bf73-31a85450898b))
  (fp_line (start -6.55 4.3) (end -6.55 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cd8ee9c6-f554-40f7-9ebd-1c1623c417ea))
  (fp_line (start -6.55 4.55) (end -6.3 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 93faa7e5-95f9-488b-be50-0658ed216011))
  (fp_line (start -6 4.55) (end -5.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6e2adcdb-0631-4343-a8c8-feb9cbea0ae8))
  (fp_line (start -5.5 4.55) (end -5.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ab81beac-674c-4a94-a6c8-34c34aa1d121))
  (fp_line (start -5 4.55) (end -4.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6187b355-55e3-48bd-8810-0c1e8a971857))
  (fp_line (start -4.5 4.55) (end -4.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9921a2d6-5655-43e2-beb6-115d63e9a192))
  (fp_line (start -4 4.55) (end -3.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 23d595d7-7cdf-43a8-821f-ffdb50f154ed))
  (fp_line (start -3.5 4.55) (end -3.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 094f1027-977f-4aa0-b7b7-faae46642657))
  (fp_line (start -3 4.55) (end -2.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f69145fa-66a6-4e79-9fdd-0277d4e0c08f))
  (fp_line (start -2.5 4.55) (end -2.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a3deb797-feb6-4cc7-9f76-99695fd94b05))
  (fp_line (start -2 4.55) (end -1.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f502d50d-d09c-40cf-a4f5-f926dce67d0b))
  (fp_line (start -1.5 4.55) (end -1.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ec617529-822b-4b74-83ba-94d0b278c320))
  (fp_line (start -1 4.55) (end -0.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8dc2b7c0-acf5-4312-90cd-588cf3cc1079))
  (fp_line (start -0.5 4.55) (end -0.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d61f101c-3721-4410-beab-0fd1c744285b))
  (fp_line (start 0.25 4.55) (end 0.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a69c4c7d-ed27-4837-b459-7e0e8d12dc86))
  (fp_line (start 0.75 4.55) (end 1 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 22001252-6299-4f80-8e05-629718ced462))
  (fp_line (start 1.25 4.55) (end 1.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a604da84-d2ce-493d-8220-0275b8f2c3b1))
  (fp_line (start 1.75 4.55) (end 2 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 621e884c-d70c-4885-b773-87520ca6cf34))
  (fp_line (start 2.25 4.55) (end 2.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ba3860d6-fa8a-4174-b101-71c80e33ac2f))
  (fp_line (start 2.75 4.55) (end 3 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9cbd9625-3e2b-4c2c-968c-251f94699953))
  (fp_line (start 3.25 4.55) (end 3.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d0772d38-d27c-4057-8403-086bdb473afb))
  (fp_line (start 3.75 4.55) (end 4 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 987297e5-435f-469e-9ceb-e1fb035dbe93))
  (fp_line (start 4.25 4.55) (end 4.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c6ae0d50-77e3-4ff3-90db-4cb55e6e4340))
  (fp_line (start 4.75 4.55) (end 5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 729a1409-f3ee-4cfb-863c-05ca18b4e866))
  (fp_line (start 5.25 4.55) (end 5.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b3b6f469-0905-48d5-ab7a-f5b2e1bf3eef))
  (fp_line (start 5.75 4.55) (end 6 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 868a0100-f276-496f-b0ee-76bc973f15ee))
  (fp_line (start 6.55 2.8) (end 6.55 3.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5226c5ba-6fcb-47da-994c-04b301585801))
  (fp_line (start 6.55 3.3) (end 6.55 3.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8493d564-a23c-4230-b9e7-65de044eead2))
  (fp_line (start 6.55 3.8) (end 6.55 4.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 487a3830-014c-464c-ac29-3084f8403f0b))
  (fp_line (start 6.55 4.3) (end 6.55 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d5183742-bfb2-4b33-a3bf-8bf184393922))
  (fp_line (start 6.55 4.55) (end 6.3 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a499b03a-4a00-43ec-8842-4a65ee385e4d))
  (fp_rect (start -6.55 2.55) (end 6.55 -2.55)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 024dddb9-ad98-406a-9529-6d1863c2c106))
  (pad "1" smd roundrect (at 4.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 07da0cce-209e-4c53-977a-4a28f40a1e00))
  (pad "2" smd roundrect (at 4.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 60b452d6-e844-49dc-bd8c-3222a91df505))
  (pad "3" smd roundrect (at 3.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp f22ddbf7-ce49-4646-96b0-8e3828bb3223))
  (pad "4" smd roundrect (at 3.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp cadb89ab-e948-4c29-b292-7925dfbdd1d9))
  (pad "5" smd roundrect (at 2.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp d90c0c83-7c9c-4f37-a6eb-aa3a503c6c07))
  (pad "6" smd roundrect (at 2.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp da9f9c24-aa00-400a-a33f-13ab25d8465a))
  (pad "7" smd roundrect (at 1.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp d5878f41-d3b7-4c4c-a3d1-5e983cd1707a))
  (pad "8" smd roundrect (at 1.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 289099f7-8532-41ca-b42a-fddfd2afb08d))
  (pad "9" smd roundrect (at 0.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 7ba0a03e-627e-4cc8-9301-8c9a7707142e))
  (pad "10" smd roundrect (at 0.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 739f61c5-34f9-4d33-b0ef-457cc2c031e2))
  (pad "11" smd roundrect (at -0.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 028999af-f821-4e37-81e6-b9230d1f4b0e))
  (pad "12" smd roundrect (at -0.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp fb612523-184f-41a4-b87a-5a69831424c8))
  (pad "13" smd roundrect (at -1.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 85fbd0fe-9c35-41c0-820c-fc6abd2fff7d))
  (pad "14" smd roundrect (at -1.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp b55a8aef-2ff0-45ce-9acd-95f63e48cec9))
  (pad "15" smd roundrect (at -2.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp bd05d863-c768-4286-a72d-2f2980519fb0))
  (pad "16" smd roundrect (at -2.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp fcf13553-36fe-4197-b555-fe4b57f419d5))
  (pad "17" smd roundrect (at -3.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp c4f71281-9f3b-40a2-b5e3-4f997dbc43ec))
  (pad "18" smd roundrect (at -3.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 84498bf2-ee7f-4007-80db-be7cefdb6426))
  (pad "19" smd roundrect (at -4.5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 987a39a4-3077-4220-9b7f-87bb33f5a9d2))
  (pad "20" smd roundrect (at -4.5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp fb237fe1-bb81-4374-b301-ff2be413ba30))
  (pad "MP" smd roundrect (at -6.175 1.85) (size 0.85 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.118) (tstamp 7010ac2e-4c39-44d4-a375-18d1104a2378))
  (pad "MP" smd roundrect (at 6.175 1.85) (size 0.85 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.118) (tstamp 3c278dae-4c09-4ab8-a21b-c4794fb890b5))
  (model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/SM20B-SRDS-G-TF.STEP"
    (offset (xyz 0 -2.55 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -90))
  )
)
