(footprint "FPC_Pads_22P_P0.5" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "CameraCable.kicad_sch")
  (property "Sheetname" "")
  (attr exclude_from_pos_files)
  (fp_text reference "J2" (at -5.5 2.65 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)) (justify left))
    (tstamp a921629b-40c1-4508-a150-c5202991e5df)
  )
  (fp_text value "Camera_FPC_Connector_(22-pin_RPi,_module_side)" (at 0 -0.25 unlocked) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp be7f7ed0-27ae-4fa2-a345-9cb4693092ab)
  )
  (fp_text user "STIFFENER BOARD" (at 0.4 2.7 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.6 0.6) (thickness 0.15)))
    (tstamp f0c4d67e-3beb-4601-9106-d5e562517cc0)
  )
  (fp_text user "${REF}" (at 0 -1.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 24b7e3e2-3345-4984-84b1-0d314a6de674)
  )
  (fp_poly
    (pts
      (xy 5.5 2.75)
      (xy 5 2.75)
      (xy 5.25 2.25)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp a084808b-1ecc-46bb-ad86-bb80ae737832))
  (fp_rect (start -5.75 0) (end 5.75 3.25)
    (stroke (width 0.05) (type solid)) (fill none) (layer "Dwgs.User") (tstamp e637214a-f737-493c-b9ff-480f662e2d70))
  (pad "1" connect roundrect (at 5.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp a126b227-ff04-4fa7-8f8a-77f33ad5cabf))
  (pad "2" connect roundrect (at 4.75 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp be6b7c74-e5aa-432e-81ac-2aed28dc6639))
  (pad "3" connect roundrect (at 4.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 7d9232f4-0a1a-4753-b441-df0df90002e4))
  (pad "4" connect roundrect (at 3.75 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 297cc740-fa77-4314-8643-061349d35d9e))
  (pad "5" connect roundrect (at 3.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 5fd72855-8caf-405b-8b48-e739b6b038eb))
  (pad "6" connect roundrect (at 2.75 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp e5a042b7-7215-4ebd-977c-4490155f909d))
  (pad "7" connect roundrect (at 2.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 95f2301c-8f98-4d38-bc3a-3a6af90b97d8))
  (pad "8" connect roundrect (at 1.75 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp a361fb19-f6f0-4674-a965-3cf6c0217572))
  (pad "9" connect roundrect (at 1.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 4bd911de-9b81-4a38-9aa2-0adb7812593a))
  (pad "10" connect roundrect (at 0.75 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 8a6a3bf3-1644-4b37-beb6-f15df7b411cf))
  (pad "11" connect roundrect (at 0.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp e7ed39d8-f8c1-4358-86d3-5c7d84caa767))
  (pad "12" connect roundrect (at -0.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 903f1180-857f-43e7-b40f-e95dc14c5ccf))
  (pad "13" connect roundrect (at -0.75 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp d840f7e3-bc29-461a-90ad-3eac4afa2023))
  (pad "14" connect roundrect (at -1.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 7b4da4ff-8348-48a7-a3fb-2e731d380b7f))
  (pad "15" connect roundrect (at -1.75 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 6480ed17-1a27-4e73-91d4-2d4ae2c26983))
  (pad "16" connect roundrect (at -2.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 436a653d-8cda-4a0a-bb29-1fe196e63470))
  (pad "17" connect roundrect (at -2.75 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp fbdfbbcd-fbc2-4d50-838e-386d62f5df97))
  (pad "18" connect roundrect (at -3.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 86023516-1844-478a-bcf2-cdf765f886f6))
  (pad "19" connect roundrect (at -3.75 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp ca8cfb3c-6cb7-4182-9dfb-11c21e5fc54c))
  (pad "20" connect roundrect (at -4.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 01c6bc9f-d1fd-47db-8049-6eee75a9f0db))
  (pad "21" connect roundrect (at -4.75 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp d0800105-fd89-438f-ada3-593255dc2ca8))
  (pad "22" connect roundrect (at -5.25 1) (size 0.3 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
    (chamfer_ratio 0.1) (chamfer top_left top_right) (tstamp 3537353a-7a70-46e7-b17c-d0762ce49a6b))
)
