(footprint "Texas_R-PUQFN-N12" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Texas_R-PUQFN-N12 http://www.ti.com/lit/ds/symlink/txb0104.pdf")
  (tags "Texas_R-PUQFN-N12")
  (property "Sheetfile" "NeedleGripperDriver.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, Texas_PUQFN-12")
  (property "ki_keywords" "Level-Shifter CMOS-TTL-Translation")
  (attr smd)
  (fp_text reference "U2" (at 0 -1.95 180) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp d29531ce-ff9e-49b8-93bd-e02f821a0279)
  )
  (fp_text value "TXB0104RUT" (at 1.15 0 -90) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 7a47b5a7-a171-47c8-9553-f7dbf8b9f2c6)
  )
  (fp_text user "${REFERENCE}" (at -1.1 0 -90) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.03)))
    (tstamp 1eb2461e-685e-4762-96e1-c7a02c7a7b85)
  )
  (fp_line (start 0.5 1.3) (end -0.5 1.3)
    (stroke (width 0.1) (type solid)) (layer "F.SilkS") (tstamp 7cfa50a1-627b-4b01-b43a-791ce5f604e3))
  (fp_line (start 0.6 -1.3) (end -1.09 -1.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ae6628f-adf4-4fa8-bda2-c4289763b6cb))
  (fp_line (start -1.1 1) (end -1.1 -1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b440b171-f57c-4b6c-be42-098b02c7f2ce))
  (fp_line (start -0.85 -1.25) (end 0.85 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 34b4e939-c3e2-42d4-81a1-8baa45f10853))
  (fp_line (start 0.85 1.25) (end -0.85 1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp de78be70-64ce-4156-b281-3f26cfa7d7cf))
  (fp_line (start 1.1 -1) (end 1.1 1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 642e6685-e9f5-4cb2-8a37-78fdbe734ba6))
  (fp_arc (start -1.1 -1) (mid -1.026777 -1.176777) (end -0.85 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d91f9229-0e57-430f-b0ef-56e441ca370d))
  (fp_arc (start -0.85 1.25) (mid -1.026777 1.176777) (end -1.1 1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 65b6691f-026d-4a37-9f9d-ffc089ccc4c0))
  (fp_arc (start 0.85 -1.25) (mid 1.026777 -1.176777) (end 1.1 -1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 30a4e1b6-0425-480e-9578-d17b12c15bb9))
  (fp_arc (start 1.1 1) (mid 1.026777 1.176777) (end 0.85 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 292941a2-0539-4ae9-84e8-8d8e45deaa3d))
  (fp_line (start -0.85 1) (end -0.85 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7259577d-e8e0-4829-90c4-34270d499c47))
  (fp_line (start -0.5 -1) (end -0.85 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c7c12897-dc72-4ee8-af1e-9fef7aef8999))
  (fp_line (start -0.5 -1) (end 0.85 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 843f02ff-120f-40de-869f-50113e609683))
  (fp_line (start 0.85 -1) (end 0.85 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 17383f0e-0899-47ae-b218-afbff91d3ea5))
  (fp_line (start 0.85 1) (end -0.85 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5dcfbc14-7d6e-4cad-bb3c-67be44aa9b5f))
  (pad "" smd oval (at -0.65 -0.8 270) (size 0.2 0.45) (layers "F.Paste") (tstamp 9f16341a-1e85-40c5-9cd0-77d5a2e327b6))
  (pad "" smd oval (at -0.65 -0.4 270) (size 0.2 0.45) (layers "F.Paste") (tstamp 9be15da9-febc-4715-9427-c0f5b8affacf))
  (pad "" smd oval (at -0.65 0 270) (size 0.2 0.45) (layers "F.Paste") (tstamp 7bed1ec9-d2ac-49fe-9934-3e5d652e413a))
  (pad "" smd oval (at -0.65 0.4 270) (size 0.2 0.45) (layers "F.Paste") (tstamp ad027673-dc60-4998-b835-45c5e4b6133f))
  (pad "" smd oval (at -0.65 0.8 270) (size 0.2 0.45) (layers "F.Paste") (tstamp d03fe27c-6b8b-4a08-aeaf-af8ad91fad0a))
  (pad "" smd oval (at 0 -0.8) (size 0.2 0.45) (layers "F.Paste") (tstamp 046de7bb-b57c-4aed-be8f-e67683f752dd))
  (pad "" smd oval (at 0 0.8) (size 0.2 0.45) (layers "F.Paste") (tstamp d58e0b8a-03f1-4286-8f52-5e4d690bcdf7))
  (pad "" smd oval (at 0.65 -0.8 270) (size 0.2 0.45) (layers "F.Paste") (tstamp 1f8e57af-7e5e-4c54-b220-b6a49ebafe0e))
  (pad "" smd oval (at 0.65 -0.4 270) (size 0.2 0.45) (layers "F.Paste") (tstamp bb17467d-ac7b-4cf6-af0a-ddd5b4ef5b61))
  (pad "" smd oval (at 0.65 0 270) (size 0.2 0.45) (layers "F.Paste") (tstamp ecf338bb-9f38-47bc-a5c4-d2bd48f5d107))
  (pad "" smd oval (at 0.65 0.4 270) (size 0.2 0.45) (layers "F.Paste") (tstamp 8bbafc91-9c04-41c0-a02f-1157a291a66e))
  (pad "" smd oval (at 0.65 0.8 270) (size 0.2 0.45) (layers "F.Paste") (tstamp 2400f361-bce4-4c44-ad1f-61f5ef709a69))
  (pad "1" smd roundrect (at -0.65 -0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 9876b1cd-2fec-44bf-9a4a-9a85075a83c1))
  (pad "1" smd roundrect (at -0.425 -0.9) (size 0.15 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.3333333333) (tstamp d119464b-a0dc-4519-b0de-41e86cc3ab16))
  (pad "2" smd roundrect (at -0.65 -0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 60560224-e170-4333-bed4-e5632e34a43f))
  (pad "3" smd roundrect (at -0.65 0 270) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 9db89a98-0f93-49f2-9be3-ca2a50d90a36))
  (pad "4" smd roundrect (at -0.65 0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 02191370-2aec-40e8-bac8-31ce022b308a))
  (pad "5" smd roundrect (at -0.65 0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp ab3f555a-3293-45ce-8943-75448d3814f1))
  (pad "6" smd roundrect (at 0 0.8) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 1896656a-6015-4136-bb78-9ff9e30bd159))
  (pad "7" smd roundrect (at 0.65 0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp dbe603cd-12e2-4e9e-8e07-4b9c3d588752))
  (pad "8" smd roundrect (at 0.65 0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 7235a909-7f57-4f8a-81cd-329cf7ba9016))
  (pad "9" smd roundrect (at 0.65 0 270) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp a6f66453-90b3-4c20-9117-70a1c1b468ac))
  (pad "10" smd roundrect (at 0.65 -0.4 270) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 9004ba15-d6cd-497d-83f8-df820d5c436a))
  (pad "11" smd roundrect (at 0.65 -0.8 270) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 5d79140f-b58e-41a2-b631-39fe5ac1637d))
  (pad "12" smd roundrect (at 0 -0.8 180) (size 0.2 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25) (tstamp 770533a1-f66a-49b6-bc41-70bb7793085b))
  (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_R-PUQFN-N12.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
