(module 5P_2x0.8_1mm_pitch (layer F.Cu) (tedit 5BED30C8)
  (fp_text reference REF** (at 0 2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 5P_2x0.8_1mm_pitch (at 0 3) (layer F.Fab) hide
    (effects (font (size 0.25 0.25) (thickness 0.05)))
  )
  (pad 1 connect roundrect (at -2 0) (size 0.8 2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 2 connect roundrect (at -1 0) (size 0.8 2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 3 connect roundrect (at 0 0) (size 0.8 2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 4 connect roundrect (at 1 0) (size 0.8 2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 5 connect roundrect (at 2 0) (size 0.8 2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
)
