(footprint "0603_C" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (tags "0201 0603 LED")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (solder_mask_margin 0.03)
  (solder_paste_margin -0.02)
  (attr smd)
  (fp_text reference "D8" (at 0.6 0 unlocked) (layer "F.SilkS") hide
      (effects (font (size 0.4 0.4) (thickness 0.1)) (justify left))
    (tstamp ed226f17-2a0d-4724-b891-50853728984a)
  )
  (fp_text value "1k" (at 0.625 0.375 unlocked) (layer "F.Fab")
      (effects (font (size 0.15 0.15) (thickness 0.0375)) (justify left))
    (tstamp 6614335b-9c5d-45c4-b565-87d883505531)
  )
  (fp_poly
    (pts
      (xy -0.5 -0.15)
      (xy -0.5 0.15)
      (xy -0.65 0.15)
      (xy -0.65 -0.15)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 9ed926a6-d8cb-43e9-9ddb-31b43f7849bf))
  (fp_poly
    (pts
      (xy -0.15 0.25)
      (xy -0.075 0.175)
      (xy 0.075 0.175)
      (xy 0.15 0.25)
      (xy 0.15 0.3)
      (xy -0.15 0.3)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0d4a7941-1c9f-44b7-b961-0fdda8af2c51))
  (fp_poly
    (pts
      (xy 0.15 -0.25)
      (xy 0.075 -0.175)
      (xy -0.075 -0.175)
      (xy -0.15 -0.25)
      (xy -0.15 -0.3)
      (xy 0.15 -0.3)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 997c55b6-902f-41c5-9586-7d87c353e077))
  (fp_line (start -0.575 -0.075) (end -0.575 0.075)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d3cdf5e5-950c-48b1-a2ba-dfe691ecfdbd))
  (fp_line (start 0.35 -0.3) (end -0.35 -0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2a408ca5-275f-4112-b029-63a477878a50))
  (fp_line (start 0.35 0.3) (end -0.35 0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4142b081-33d1-4957-a45e-27422392113c))
  (fp_line (start 0.575 -0.075) (end 0.575 0.075)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fa1cc12c-8ed8-4a3c-ac7e-88562c456d86))
  (fp_arc (start -0.575 -0.075) (mid -0.509099 -0.234099) (end -0.35 -0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a53f8fcc-5318-431a-adb4-a463145ed7eb))
  (fp_arc (start -0.35 0.3) (mid -0.509099 0.234099) (end -0.575 0.075)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bcc0c571-1ad9-47fe-a8a1-790a5afe8c90))
  (fp_arc (start 0.35 -0.3) (mid 0.509099 -0.234099) (end 0.575 -0.075)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a4ec31e9-af16-4aa3-a42a-f85a89d544d1))
  (fp_arc (start 0.575 0.075) (mid 0.509099 0.234099) (end 0.35 0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b4d6cd58-223f-4fe5-a62a-ce0654c027de))
  (fp_rect (start -0.3 -0.15) (end 0.3 0.15)
    (stroke (width 0.025) (type solid)) (fill none) (layer "F.Fab") (tstamp 94dbaa42-51b1-4350-a14b-5be165d654d5))
  (pad "" smd oval (at -0.285 0) (size 0.225 0.25) (layers "F.Paste") (tstamp 2ba6e924-7dd4-4eb4-b0f6-15e2c82d8bec))
  (pad "" smd oval (at 0.285 0) (size 0.225 0.25) (layers "F.Paste") (tstamp b1a51949-c073-44b9-b46c-c3f0fbe64a95))
  (pad "A" smd roundrect (at 0.285 0) (size 0.27 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer top_left bottom_left) (tstamp ac4730b1-0088-4b6a-9499-8ef7b0c13c6f))
  (pad "K" smd roundrect (at -0.285 0) (size 0.27 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 824d775d-6145-4db6-8f76-d97d56dadb99))
  (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
