(footprint "2P_10x5_6_pitch" (version 20211232) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61F95C1D)
  (property "Sheetfile" "Dumbbell_Base_Board.kicad_sch")
  (property "Sheetname" "")
  (attr exclude_from_pos_files)
  (fp_text reference "J2" (at 0 -6.75 -180) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp aaf40b86-4d2b-4e75-9dca-541046b0ae21)
  )
  (fp_text value "outA" (at 2.8 0 -90) (layer "F.Fab")
    (effects (font (size 0.25 0.25) (thickness 0.05)))
    (tstamp 99e9c1a1-db06-4033-a83c-4d9d1a8d0c69)
  )
  (pad "1" connect roundrect (at 0 -3) (size 10 5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1) (tstamp 9b5f8ef7-fe95-4d33-810b-3aff18561610))
  (pad "2" connect roundrect (at 0 3) (size 10 5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1) (tstamp cf844a42-6ba6-4f10-a53a-67c0f3e7e45a))
)
