(footprint "1006_C_KA" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (tags "0402 1005 Capacitor")
  (property "Sheetfile" "120W 48 to 12V Power Supply.kicad_sch")
  (property "Sheetname" "120W 48 to 12V Power Supply")
  (property "Sim.Device" "SPICE")
  (property "Sim.Params" "type=\"C\" model=\"100n\" lib=\"\"")
  (property "Sim.Pins" "1=1 2=2")
  (solder_mask_margin 0.03)
  (solder_paste_margin -0.02)
  (attr smd)
  (fp_text reference "D12" (at 0.75 0 unlocked) (layer "F.SilkS")
      (effects (font (size 0.4 0.4) (thickness 0.1)) (justify left))
    (tstamp 3530127a-e8e7-49c4-b293-c7acfb6f4e43)
  )
  (fp_text value "12V" (at 0.75 0.375 unlocked) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)) (justify left))
    (tstamp d0b368ae-0e6e-47d5-bb76-765b4b9ffa2f)
  )
  (fp_arc (start -0.8 -0.225) (mid -0.734099 -0.384099) (end -0.575 -0.45)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp a6d2c378-ba89-46cc-8f50-fca7b952d384))
  (fp_arc (start -0.575 0.45) (mid -0.734099 0.384099) (end -0.8 0.225)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 2b7950f4-565e-43bf-ba2f-9fc931bfaa0d))
  (fp_poly
    (pts
      (xy -0.725 -0.225)
      (xy -0.725 0.225)
      (xy -0.875 0.225)
      (xy -0.875 -0.225)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e0f02d19-dd35-49c6-a776-f9faaa53845c))
  (fp_poly
    (pts
      (xy 0.225 -0.375)
      (xy -0.575 -0.375)
      (xy -0.575 -0.525)
      (xy 0.225 -0.525)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 8ddf032a-5d07-4607-b776-b84e257c3eab))
  (fp_poly
    (pts
      (xy 0.225 0.525)
      (xy -0.575 0.525)
      (xy -0.575 0.375)
      (xy 0.225 0.375)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp dbd2de7b-cd5e-4eb6-8b69-9c204d5f4554))
  (fp_line (start -0.8 -0.25) (end -0.8 0.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b2b2f92f-9be9-4f93-8bf7-3f873ed98c62))
  (fp_line (start -0.6 -0.45) (end 0.6 -0.45)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b771f4e8-82ba-4166-a790-ec7f3ad956be))
  (fp_line (start -0.6 0.45) (end 0.6 0.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7266a051-085c-41e1-9c9b-2d92980bdfa7))
  (fp_line (start 0.8 -0.25) (end 0.8 0.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 20a19dcd-c9c7-48ed-8cf8-196b8356e612))
  (fp_arc (start -0.8 -0.25) (mid -0.741421 -0.391421) (end -0.6 -0.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3182ea8f-18aa-4485-89b0-769dd9067d2b))
  (fp_arc (start -0.6 0.45) (mid -0.741421 0.391421) (end -0.8 0.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9e452897-feb1-4a8e-b424-46e150b54f08))
  (fp_arc (start 0.6 -0.45) (mid 0.741421 -0.391421) (end 0.8 -0.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7793f067-e754-42b4-a049-1ce76ac01612))
  (fp_arc (start 0.8 0.25) (mid 0.741421 0.391421) (end 0.6 0.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bd31dc39-1698-49b7-89d6-eeea69afba51))
  (fp_rect (start -0.5 -0.3) (end 0.5 0.3)
    (stroke (width 0.01) (type solid)) (fill none) (layer "F.Fab") (tstamp 3f9d82fb-8e80-4792-a66c-54e3b887aa0f))
  (pad "" smd oval (at -0.45 0) (size 0.3 0.5) (layers "F.Paste") (tstamp 1e600341-d7e5-4051-b561-63812ad96d26))
  (pad "" smd oval (at 0.45 0) (size 0.3 0.5) (layers "F.Paste") (tstamp 1191bb6f-2da7-4851-9009-22f636230e2c))
  (pad "A" smd roundrect (at 0.45 0) (size 0.4 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2)
    (chamfer_ratio 0.05) (chamfer top_left bottom_left) (tstamp c4bb74ca-5a3f-46cf-bc5b-2513edb338ac))
  (pad "K" smd roundrect (at -0.45 0) (size 0.4 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 4843c003-1423-4268-b906-56178c6dd21f))
  (model "${KICAD7_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
