(module KF7.62_3P (layer F.Cu) (tedit 58078D74)
  (descr "As measured")
  (solder_mask_margin -0.05)
  (fp_text reference J2 (at 0 -5.08 180) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value MAINS (at -3.96 6.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start 3.81 5.08) (end 3.81 -5.08) (layer F.SilkS) (width 0.125))
  (fp_line (start -11.43 -6) (end -11.43 6) (layer F.SilkS) (width 0.125))
  (fp_line (start 11.43 -6) (end -11.43 -6) (layer F.SilkS) (width 0.125))
  (fp_line (start -3.81 5) (end -3.81 -5) (layer F.SilkS) (width 0.125))
  (fp_line (start -11.43 6) (end 11.43 6) (layer F.SilkS) (width 0.125))
  (fp_line (start 11.43 -6) (end 11.43 6) (layer F.SilkS) (width 0.125))
  (fp_line (start -12.43 -7) (end -12.43 7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 12.43 7) (end -12.43 7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 12.43 -7) (end 12.43 7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -12.43 -7) (end 12.43 -7) (layer F.CrtYd) (width 0.05))
  (pad 3 connect roundrect (at 7.62 3.5) (size 3 3) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 2 connect roundrect (at 0 3.5) (size 3 3) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 1 connect roundrect (at -7.62 3.5) (size 3 3) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 2 thru_hole circle (at 0 3.5) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -7.62 3.5) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 7.62 3.5) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (model ${KICAD7_3DMODEL_DIR}/TerminalBlock.3dshapes/Terminal_7.62.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
  (model ${KICAD7_3DMODEL_DIR}/TerminalBlock.3dshapes/Terminal_7.62.step
    (at (xyz 0.3 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
  (model ${KICAD7_3DMODEL_DIR}/TerminalBlock.3dshapes/Terminal_7.62.step
    (at (xyz -0.3 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
