(module TCT40-18_Ultrasonic_Transceiver (layer F.Cu) (tedit 57EFE7B6)
  (tags "PIEZO TRANSCEIVER ULTRASONIC")
  (fp_text reference SP1 (at -9.75 0 270) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value 40kHz (at -3 0 90) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_circle (center 0 0) (end 0 -9) (layer F.SilkS) (width 0.125))
  (fp_text user + (at 6 -1.5) (layer B.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)) (justify mirror))
  )
  (pad 2 thru_hole circle (at 5.1 0) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -5.1 0) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask))
  (model "${KICAD7_3DMODEL_DIR}/Speaker_Transducer.3dshapes/Ultrasonic Tranceiver [Closed] [Waterproof] [Dual Use].step"
    (at (xyz 0 0 0.4763779527559055))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 0 0))
  )
)
