(footprint "3216_C"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(tags "1206 3216")
	(property "Reference" "C89"
		(at 1.75 0 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "2d6cfa43-3276-4e53-9c39-febf527a8564")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
				(bold yes)
			)
			(justify left)
		)
	)
	(property "Value" "47uF"
		(at 1.9 0.65 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "ed88bbb4-4194-435a-a89f-cc1676f58a59")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
			(justify left)
		)
	)
	(property "Footprint" "3216_C"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d82988b1-ad64-4f5b-b862-f63f796cdb8b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "cee0d528-0afc-4c28-a672-87efce8a636c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "9c8b9ca0-575e-4427-bb4d-c3aa3efefc5f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C96123"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "287560f9-6814-4009-8f34-1decf40daa13")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "Samsung"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "0abff109-2bcf-48c4-86a2-c09d242a901d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "CL31A476MPHNNNE"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "99985604-6783-40df-8f14-73b7ae55fa18")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Device" "SPICE"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "17fedde6-efdc-4f0f-9747-6533f4dec566")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Params" "type=\"C\" model=\"100n\" lib=\"\""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "928a8c4f-375b-4c97-89f2-8b6c4e2e1a49")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Pins" "1=1 2=2"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8a69f364-77a8-4f82-9bcb-8e4b84163ddd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.05)
	(solder_paste_margin -0.03)
	(attr smd)
	(fp_rect
		(start -0.95 -1)
		(end 0.95 -0.85)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "e90e33ca-cdba-49fc-ad42-149d3523f53c")
	)
	(fp_rect
		(start -0.95 0.85)
		(end 0.95 1)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "c18a0d26-7acb-46c7-b187-e83cc115750d")
	)
	(fp_line
		(start -1.9 0.675)
		(end -1.9 -0.675)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "10070a74-5f32-4496-a2d6-664362927a8a")
	)
	(fp_line
		(start -1.6 -0.975)
		(end 1.6 -0.975)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4d2ff07e-559a-492b-8ed4-37e622c468f5")
	)
	(fp_line
		(start 1.6 0.975)
		(end -1.6 0.975)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0dc73cee-40df-406f-9a6e-2e6d7e92a5e0")
	)
	(fp_line
		(start 1.9 -0.675)
		(end 1.9 0.675)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f762563d-08ac-46b0-a0e0-35119b73d3e2")
	)
	(fp_arc
		(start -1.9 -0.675)
		(mid -1.812132 -0.887132)
		(end -1.6 -0.975)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "326d9c48-a403-4a7a-a131-5df2b93f305b")
	)
	(fp_arc
		(start -1.6 0.975)
		(mid -1.812132 0.887132)
		(end -1.9 0.675)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4c99dde6-8ed3-4c24-8517-29f1d2df689d")
	)
	(fp_arc
		(start 1.6 -0.975)
		(mid 1.812132 -0.887132)
		(end 1.9 -0.675)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0d3eb534-3800-4485-9be0-ed8d6950e543")
	)
	(fp_arc
		(start 1.9 0.675)
		(mid 1.812132 0.887132)
		(end 1.6 0.975)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1f618215-48a8-44fe-a445-01d9477d576e")
	)
	(fp_line
		(start -1.6 -0.8)
		(end 1.6 -0.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d1610de6-87a3-4260-bf6f-5a641a905932")
	)
	(fp_line
		(start -1.6 0.8)
		(end -1.6 -0.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4d667da8-99be-4e0d-80c6-c1bfc5619da2")
	)
	(fp_line
		(start 1.6 -0.8)
		(end 1.6 0.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c987d6ba-6c65-4c42-b717-1a22514800a6")
	)
	(fp_line
		(start 1.6 0.8)
		(end -1.6 0.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5ad133e9-80ea-4030-b8c9-9c330ec1a270")
	)
	(pad "" smd oval
		(at -1.425 0)
		(size 0.55 1.4)
		(layers "F.Paste")
		(uuid "68f75f2d-26c8-4106-aede-d0f9028a717b")
	)
	(pad "" smd oval
		(at 1.425 0)
		(size 0.55 1.4)
		(layers "F.Paste")
		(uuid "b74dd18d-04d5-4416-b5df-9512455ed8c3")
	)
	(pad "1" smd roundrect
		(at -1.425 0)
		(size 0.65 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "a6586056-afd8-4b41-96bf-50322061f808")
	)
	(pad "2" smd roundrect
		(at 1.425 0)
		(size 0.65 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.05)
		(chamfer top_left bottom_left)
		(uuid "6ad3b6e7-c54c-4c34-a5d6-9d2c7d377f03")
	)
	(model "${KICAD7_3DMODEL_DIR}/Capacitor_SMD.3dshapes/Capacitor_SMD_3216.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
