(module CUI_UP2-AH-1-TH_USB_A (layer F.Cu) (tedit 5818AD1C)
  (solder_mask_margin -0.02)
  (fp_text reference P1 (at -3.5 6.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value USB_A (at 0 -1) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -6 0) (end 6 0) (layer F.Fab) (width 0.125))
  (fp_line (start -6 0) (end -6 5) (layer F.Fab) (width 0.125))
  (fp_line (start -6 5) (end 6 5) (layer F.Fab) (width 0.125))
  (fp_line (start 6 5) (end 6 0) (layer F.Fab) (width 0.125))
  (fp_line (start 9 0) (end 9 -5) (layer F.Fab) (width 0.05))
  (fp_line (start -9 0) (end -9 -5) (layer F.Fab) (width 0.05))
  (pad "" np_thru_hole circle (at 2.3 2.9) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1))
  (pad "" np_thru_hole circle (at -2.3 2.9) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask)
    (solder_mask_margin 0.1))
  (pad 1 thru_hole circle (at -3.5 5) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -1 5) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 1 5) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 3.5 5) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -5.85 2.9) (size 2.9 2.9) (drill 2.3) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 5.85 2.9) (size 2.9 2.9) (drill 2.3) (layers *.Cu *.Mask))
  (model ${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/CUI_INC_UP2-AH-1-TH.step
    (at (xyz 0 0.5866141732283465 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 90))
  )
)
